R1:
Current configuration : 3547 bytes
!
! Last configuration change at 13:58:58 UTC Mon Aug 19 2019
!
version 16.9
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
platform qfp utilization monitor load 80
no platform punt-keepalive disable-kernel-core
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$laRB$qBi1f5nFFfFPQv0.q8FBS1
!
no aaa new-model
!
no ip domain lookup
ip admission watch-list expiry-time 0
!
!
!
!
!
!
!
!
!
!
subscriber templating
multilink bundle-name authenticated
!
!
!
crypto pki trustpoint TP-self-signed-1562137005
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-1562137005
 revocation-check none
 rsakeypair TP-self-signed-1562137005
!
!
crypto pki certificate chain TP-self-signed-1562137005
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 31353632 31333730 3035301E 170D3139 30383139 31333136
  32315A17 0D333030 31303130 30303030 305A3031 312F302D 06035504 03132649
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D31 35363231
  33373030 35308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
  0A028201 0100D4EE 7A20B8CF 8A6BB1E3 5507630D 9B48927B D1647B1B F2A157C1
  9E574DD2 E24C65CC 71078E44 EA31884F ECAA73D2 6FB726D7 FF3EC443 D3D3E44D
  E9DEBF7F C23147C2 E94380B9 27E91666 A20070DE 060B863C 1FD812F1 CA0173C5
  FAD86696 785385A0 4C3A8595 05A12B26 C985EF13 3E98F2BD F6067AFC 1EBA6DFF
  AC1754E5 0259E7D8 CB81908B 3FC5AB00 7338E287 2DF42A1D 0A060AC9 5AB8D290
  D1C9C573 72343807 FA9CA51C 41F752FA 04C60A43 CB00C783 D1981580 D11A4C3A
  744293A9 45601848 06D72FD5 EF1ECBF7 63282B78 667297C9 14109715 6015B473
  212DCA09 614CD216 F80B5125 79339ED5 2BA7DF02 5C5013BD BACCB1FF A612E762
  8172F9B8 BF090203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
  301F0603 551D2304 18301680 14E8FCF7 B3D1CC33 6316D4C8 8F6CE5AD D1654AEC
  50301D06 03551D0E 04160414 E8FCF7B3 D1CC3363 16D4C88F 6CE5ADD1 654AEC50
  300D0609 2A864886 F70D0101 05050003 82010100 98FE94B7 82696E21 ED9EA0BC
  5E640444 6E294973 253A2B38 FC7EF0B2 04501EFC 1259C634 8885C93E D723241B
  629BBC69 97FA5726 96986632 93081497 517A910E F3305C5F 67F8F5B6 7109FF67
  6A59A56B 8439628D CC85FD18 AE04C51D 1F32F1A7 DA4CDA5F FD2FE45C 72B4DF7C
  5D454503 BC7440DD C007D002 6EDFE30C 041B0EEF 41F0734A 7D4D0745 1EC106C1
  A432E2EF 890DD2A0 AA747E92 55CE7153 316F42B2 875CCDF3 655CB4EF 5A95DF06
  73447BB9 FA0DCE33 F32DAE2C 4F3A17DF 51A2CD6A 61A75B33 441ED446 9BB9ED25

license udi pid ISR4221/K9 sn FGL224190DN
no license smart enable
diagnostic bootup level minimal
!
spanning-tree extend system-id
!
!
!
!
redundancy
 mode none
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0/0
 ip address 172.16.10.1 255.255.255.0
 negotiation auto
!
interface GigabitEthernet0/0/1
 ip address 172.16.11.1 255.255.255.0
 negotiation auto
!
interface Serial0/1/0
 no ip address
 shutdown
!
interface Serial0/1/1
 no ip address
 shutdown
!
ip forward-protocol nd
ip http server
ip http authentication local
ip http secure-server
!
!
!
!
!
!
control-plane
!
banner motd ^C Unauthorizrd access is prohibited ^C
!
line con 0
 password 7 110A1016141D
 login
 transport input none
 stopbits 1
line vty 0 4
 password 7 110A1016141D
 login
line vty 5 15
 password 7 110A1016141D
 login
!
!
!
!
!
!
End


IP int brief

R1#show ip int brief
Interface              IP-Address      OK? Method Status                Protocol
GigabitEthernet0/0/0   172.16.10.1     YES manual up                    up
GigabitEthernet0/0/1   172.16.11.1     YES manual up                    up
Serial0/1/0            unassigned      YES unset  administratively down down
Serial0/1/1            unassigned      YES unset  administratively down down

S1:
S1#show running-config
Building configuration...

Current configuration : 1460 bytes
!
! Last configuration change at 03:02:30 UTC Mon Mar 1 1993
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
system mtu routing 1500
!
!
!
!
!
!
!
no ip domain-lookup
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface FastEthernet0/1
!
interface FastEthernet0/2
!
interface FastEthernet0/3
!
interface FastEthernet0/4
!
interface FastEthernet0/5
!
interface FastEthernet0/6
!
interface FastEthernet0/7
!
interface FastEthernet0/8
!
interface FastEthernet0/9
!
interface FastEthernet0/10
!
interface FastEthernet0/11
!
interface FastEthernet0/12
!
interface FastEthernet0/13
!
interface FastEthernet0/14
!
interface FastEthernet0/15
!
interface FastEthernet0/16
!
interface FastEthernet0/17
!
interface FastEthernet0/18
!
interface FastEthernet0/19
!
interface FastEthernet0/20
!
interface FastEthernet0/21
!
interface FastEthernet0/22
!
interface FastEthernet0/23
!
interface FastEthernet0/24
!
interface GigabitEthernet0/1
!
interface GigabitEthernet0/2
!
interface Vlan1
 ip address 172.16.11.10 255.255.255.0
!
ip default-gateway 172.16.11.1
ip http server
ip http secure-server
!
no vstack
banner motd ^CNo unauthorized access^C
!
line con 0
line vty 0 4
 password cisco
 login
line vty 5 15
 password cisco
 login
!
end



Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  172.16.11.10    YES manual up                    up
FastEthernet0/1        unassigned      YES unset  down                  down
FastEthernet0/2        unassigned      YES unset  down                  down
FastEthernet0/3        unassigned      YES unset  down                  down
FastEthernet0/4        unassigned      YES unset  down                  down
FastEthernet0/5        unassigned      YES unset  up                    up
FastEthernet0/6        unassigned      YES unset  up                    up
FastEthernet0/7        unassigned      YES unset  down                  down
FastEthernet0/8        unassigned      YES unset  down                  down
FastEthernet0/9        unassigned      YES unset  down                  down
FastEthernet0/10       unassigned      YES unset  down                  down
FastEthernet0/11       unassigned      YES unset  down                  down
FastEthernet0/12       unassigned      YES unset  down                  down
FastEthernet0/13       unassigned      YES unset  down                  down
FastEthernet0/14       unassigned      YES unset  down                  down
FastEthernet0/15       unassigned      YES unset  down                  down
FastEthernet0/16       unassigned      YES unset  down                  down
FastEthernet0/17       unassigned      YES unset  down                  down
FastEthernet0/18       unassigned      YES unset  down                  down
FastEthernet0/19       unassigned      YES unset  down                  down
FastEthernet0/20       unassigned      YES unset  down                  down
FastEthernet0/21       unassigned      YES unset  down                  down
FastEthernet0/22       unassigned      YES unset  down                  down
FastEthernet0/23       unassigned      YES unset  down                  down
FastEthernet0/24       unassigned      YES unset  down                  down
GigabitEthernet0/1     unassigned      YES unset  down                  down
GigabitEthernet0/2     unassigned      YES unset  down                  down
S1#













[bookmark: _GoBack]PC-A:

[image: ]

[image: ]

PC-B:
[image: ]

image1.JPG
:\Users\Adnin>ping 172.16.16.254

Pinging 172.16.16.254 with 32 bytes of data:
Reply from 172.16.16.254: 2 timecins
Reply from 172.16.16.254; 2 timecins TTL-127
Reply from 172.16.16.254: 2 timecins TTL-127
Reply from 172.16.16.254: 2 timecins TTL-127

Ping statistics for 172.16.10.254:
Packets: Sent - 4, Received = 4, Lost = @ (6% loss),
Approximate round trip times in milli-seconds:
Mininun = ems, Maximum - ems, Average = 6ms

:\Users\Admin>
B
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Ethernet adapter Ethernet:

Connection-specific DNS Suffix
Description .

Physical Address.

DHCP Enabled. e
Autoconfiguration Enabled .
Link-local IPv6 Address .
1Pv4 Address.

Subnet Mask .

Default Gateway .

DHCPYV6 TATD .

DHCPV6 Client DUID.

DNS Servers .

NetBIOS over Tcpip.

C:\Users\Admin>

: Intel(R) Ethernet Connection (2) 1219-LM
8C-9D-92-BF-B9-FE

d108:b1c2:7668:9673%7 (Preferred)
172.16.11.254(Preferred)

: 255.255.255.8

172.16.11.1

51158418

: 60-61-00-01-23-4E-58-1C-0C-0D-02-BF-B9-FE
1%

fecB:0:0:FFFF::3%1
Enabled





image3.JPG
Ethernet adapter Ethernet:

Connection-specific DNS Suffix
Description .

Physical Address.

DHCP Enabled.
Autoconfiguration Enabled .
Link-local IPv6 Address .
1Pva Address.

Subnet Mask .

Default Gateway .

DHCPYV6 TATD .

DHCPY6 Client DUID.

DNS Servers .

Intel(R) Ethernet Connection (2) 1219-LM
C-9D-92-BF-BA-80

a53e:a4bc:5a70:9020%16 (Preferred)
: 172.16.10.254 (Preferred)

255.255.255.6

172.16.16.1

: 101490066
0-61-60-61-23-56-CC-C4-0C-9D-92-BF -BA-80

NetBIOS over Tcpip.




