Student Name: Dan Rowley
[bookmark: _GoBack]Switch 2:
S2(config)#do show run
Building configuration...

Current configuration : 1335 bytes
!
version 12.2
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname S2
!
!
!
no ip domain-lookup
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
interface FastEthernet0/1
switchport mode trunk
!
interface FastEthernet0/2
!
interface FastEthernet0/3
!
interface FastEthernet0/4
!
interface FastEthernet0/5
!
interface FastEthernet0/6
switchport access vlan 5
switchport mode access
!
interface FastEthernet0/7
!
interface FastEthernet0/8
!
interface FastEthernet0/9
!
interface FastEthernet0/10
!
interface FastEthernet0/11
!
interface FastEthernet0/12
!
interface FastEthernet0/13
!
interface FastEthernet0/14
!
interface FastEthernet0/15
!
interface FastEthernet0/16
!
interface FastEthernet0/17
!
interface FastEthernet0/18
switchport access vlan 23
switchport mode access
!
interface FastEthernet0/19
!
interface FastEthernet0/20
!
interface FastEthernet0/21
!
interface FastEthernet0/22
!
interface FastEthernet0/23
!
interface FastEthernet0/24
!
interface GigabitEthernet0/1
!
interface GigabitEthernet0/2
!
interface Vlan1
no ip address
shutdown
!
interface Vlan9
mac-address 00e0.8fae.7901
ip address 192.168.9.1 255.255.255.0
!
ip default-gateway 192.168.9.1
!
!
!
!
line con 0
!
line vty 0 4
login
line vty 5 15
login
!
!
!
!
end

Switch 1:
S1(config)#do sh run
Building configuration...

Current configuration : 1446 bytes
!
version 12.2
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname S1
!
!
!
no ip domain-lookup
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
interface FastEthernet0/1
switchport mode trunk
!
interface FastEthernet0/2
!
interface FastEthernet0/3
!
interface FastEthernet0/4
!
interface FastEthernet0/5
switchport access vlan 6
!
interface FastEthernet0/6
switchport access vlan 21
switchport mode access
!
interface FastEthernet0/7
!
interface FastEthernet0/8
!
interface FastEthernet0/9
!
interface FastEthernet0/10
!
interface FastEthernet0/11
!
interface FastEthernet0/12
!
interface FastEthernet0/13
!
interface FastEthernet0/14
switchport access vlan 6
switchport mode access
!
interface FastEthernet0/15
!
interface FastEthernet0/16
!
interface FastEthernet0/17
!
interface FastEthernet0/18
!
interface FastEthernet0/19
!
interface FastEthernet0/20
!
interface FastEthernet0/21
!
interface FastEthernet0/22
!
interface FastEthernet0/23
!
interface FastEthernet0/24
!
interface GigabitEthernet0/1
switchport mode trunk
!
interface GigabitEthernet0/2
!
interface Vlan1
no ip address
shutdown
!
interface Vlan9
mac-address 000c.85cb.d602
ip address 192.168.9.1 255.255.255.0
!
interface Vlan99
mac-address 000c.85cb.d601
no ip address
!
ip default-gateway 192.168.9.1
!
!
!
!
line con 0
!
line vty 0 4
login
line vty 5 15
login
!
!
!
!
end


Branch 1:
Branch1(config)#do sh run
Building configuration...

Current configuration : 2120 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname Branch1
!
!
!
!
ip dhcp excluded-address 192.168.5.1 192.168.5.11
ip dhcp excluded-address 192.168.6.1 192.168.6.11
ip dhcp excluded-address 192.168.7.1 192.168.7.11
ip dhcp excluded-address 192.168.8.1 192.168.8.11
!
ip dhcp pool vlan5
network 192.168.5.0 255.255.255.0
default-router 192.168.5.1
dns-server 209.165.200.25
ip dhcp pool vlan6
network 192.168.6.0 255.255.255.0
default-router 192.168.6.1
dns-server 209.165.200.25
ip dhcp pool vlan7
network 192.168.7.0 255.255.255.0
default-router 192.168.7.1
dns-server 209.165.200.25
ip dhcp pool vlan8
network 192.168.8.0 255.255.255.0
default-router 192.168.8.1
dns-server 209.165.200.25
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2901/K9 sn FTX1524M39E-
!
!
!
!
!
!
!
!
!
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface Loopback2
ip address 192.168.2.1 255.255.255.0
!
interface Loopback3
no ip address
!
interface GigabitEthernet0/0
no ip address
duplex auto
speed auto
!
interface GigabitEthernet0/0.5
encapsulation dot1Q 5
ip address 192.168.5.11 255.255.255.0
!
interface GigabitEthernet0/0.6
encapsulation dot1Q 6
ip address 192.168.6.11 255.255.255.0
!
interface GigabitEthernet0/0.7
encapsulation dot1Q 7
ip address 192.168.7.11 255.255.255.0
!
interface GigabitEthernet0/0.8
encapsulation dot1Q 8
ip address 192.168.8.11 255.255.255.0
!
interface GigabitEthernet0/0.9
encapsulation dot1Q 9
ip address 192.168.9.11 255.255.255.0
!
interface GigabitEthernet0/1
no ip address
duplex auto
speed auto
shutdown
!
interface Serial0/0/0
no ip address
clock rate 2000000
shutdown
!
interface Serial0/0/1
ip address 10.10.4.1 255.255.255.0
clock rate 2000000
!
interface Vlan1
no ip address
shutdown
!
router rip
network 10.0.0.0
network 192.168.5.0
network 192.168.6.0
network 192.168.7.0
network 192.168.8.0
network 192.168.9.0
network 209.165.200.0
!
ip classless
!
ip flow-export version 9
!
!
!
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
login
!
!
!
end


Branch 2:
Brunch2(config)#do sh run
Building configuration...

Current configuration : 950 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname Brunch2
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2901/K9 sn FTX1524PFRG-
!
!
!
!
!
!
!
!
!
no ip domain-lookup
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
ip address 209.165.200.31 255.255.255.0
duplex auto
speed auto
!
interface GigabitEthernet0/1
no ip address
duplex auto
speed auto
shutdown
!
interface Serial0/0/0
ip address 10.10.10.2 255.255.255.0
clock rate 2000000
!
interface Serial0/0/1
ip address 10.10.4.2 255.255.255.0
!
interface Vlan1
no ip address
shutdown
!
router rip
network 10.0.0.0
network 192.165.7.0
network 192.168.5.0
network 192.168.6.0
network 192.168.8.0
network 192.168.9.0
network 209.165.200.0
!
ip classless
!
ip flow-export version 9
!
!
!
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
login
!
!
!
end



Branch 3:
Branch3(config)#do sh run
Building configuration...

Current configuration : 923 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname Branch3
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2901/K9 sn FTX15244965-
!
!
!
!
!
!
!
!
!
no ip domain-lookup
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
no ip address
duplex auto
speed auto
shutdown
!
interface GigabitEthernet0/1
no ip address
duplex auto
speed auto
shutdown
!
interface Serial0/0/0
ip address 10.10.10.1 255.255.255.0
!
interface Serial0/0/1
no ip address
clock rate 2000000
shutdown
!
interface Vlan1
no ip address
shutdown
!
router rip
network 10.0.0.0
network 192.165.9.0
network 192.168.5.0
network 192.168.6.0
network 192.168.7.0
network 192.168.8.0
network 209.165.200.0
!
ip classless
!
ip flow-export version 9
!
!
!
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
login
!
!
!
end

