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IATG SAFERGUARD TRAINING MODULES
MODULE MA05 – QUANTITY DISTANCE EXERCISE 
MINI-EXERCISE
ANNEX B
EXPLOSIVE FACILITY – DETAILS:
ESH 1:    

A small, earth covered (igloo) type ESH. Earth on the roof and against 3 walls. 

Headwall and door may be resistant to low velocity projections.  Door faces south.
Category C lighting system.

Un-heated, but temperature recordings show a reliable temperature range between 5 and 17 ºC.

10 Units of Space, plus a brick walled container traverse large enough for 1 UOS (total 11 UOS).
This ESH has a fully serviceable and working intruder alarm which links directly to the guardroom.  

ESH 1 also has a fully functioning CCTV system with a monitor in the guard room. 

ESH 2:
Unheated brick building.

No temperature records.

715mm thick brick walls, 150mm reinforced concrete roof. 

Barricaded door.  Door faces south.
40 Units of Space.

This ESH has a fully serviceable and working intruder alarm which links directly to the guardroom.  

ESH 3:

As for ESH 2.

ESH 4:

As for ESH 2.

However, door is not barricaded and faces east.

ESH 5: 

Light structure, brick walls of 220mm brick.   Protective roof of 150mm reinforced concrete. 

Traversed on 3 sides.  Door faces east (un-traversed side)
60 Units of Space.
ESH 6:

Basic ‘shed’ structure made of frangible panels.  Door faces west.
Traversed on all sides.
50 Units of Space.
ESH 7:

Basic ‘shed’ structure made of frangible materials.  Door faces south-east.
No traversing.
40 UOS.
Ammunition Process Building: 

Medium walled building, 225mm thick brick walls.  
155mm reinforced concrete roof.  
Traversed on all sides.
Truck marshalling/loading/unloading/stabling area:
An area of hard standing, 30 x 30m.  It is untraversed.  

Depot office:  

Standard office building with ‘shatter proof film’ and ‘bomb net curtains’ on windows.   

Windows to one side, pointing away from ESHs (north west).  

Occupied by no more than 19 people at any one time. 

Guard room:

Medium walled building.
150mm reinforced concrete protective roof.   

Up to 3 people present in the building, 24 hours a day. 

SURROUNDING AREA - DETAILS: 
Main road:

A main road lining to important market towns. 

Traffic is approximately 2,000 vehicles per day (medium density). 

Café and shop:

Traditionally built structure of brick in a concrete frame with a tiled roof.

A café and shop for passing drivers.  

24 hour opening.

Usually no more than 400 visitors per day and a shop staff of 3. 
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