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-Routing and Remote Access Services (RRAS): is a windows server service that allows computers to communicate between different networks and enables users to securely access a network remotely.
-Active Directory Domain Services(AD DS): Is a Microsoft windows server role that stores and manages information about users, computers, groups, and other network resources in a domain.
-DHCP(Dynamic Host Configuration Protocol): is a network device or service that automatically assigned IP address, subnet masks, default gateways, and DNS settings to devices.
-Remote Desktop Service :The use of remote desktop services on virtualized machines is a general trend to reduce the cost of desktop seats. Instead of assigning a physical machine with its operating system and software to each user, it is considerably easier to manage a light client machine that connects to a server where the instance of the user’s desktop machine actually executes. Citrix and VMware have been major suppliers of these systems in private clouds. Desktop-as-a-Service solutions such as Amazon WorkSpaces offer a similar functionality, yet in a public cloud environment. In this paper, we review the main offerings of remote desktop protocols for a cloud deployment. We evaluate the necessary network resources using a traffic model based on self-similar processes. We also evaluate the quality of experience perceived by the user, in terms of image quality and interactivity, providing values of Mean Opinion Score (MOS). The results confirm that the type of application running on the remote servers and the mix of users must be considered to determine the bandwidth requirements. Applications such as web browsing result in unexpectedly high traffic rates and long bursts, more than the case of desktop video playing, because the on-page animations are rendered on the server.
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[bookmark: _Toc237529569]		Task 1 : Screenshots of Routing remote access.
· Install Routing and Remote access Service and modify firewall rules to allow ICMP Traffic
[image: ]
· In this picture above it shows the ‘Routing and Remote access’ is configured on the server.
[image: ]
· In this picture above it shows ICMP traffic is enabled. So in your screenshot, choosing ICMP means the firewall rule is specifically controlling ping and other ICMP traffic, rather than normal TCP/UDP traffic.
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· Screenshot of Inbound IP configuration
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· Enable VPN to secure traffics between computers

2/ Domain Server


[image: ]
· Screenshot shows that Active Directory Domain Services(AD DS) has been installed.
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· This screenshot shows the Domain Name and the Records
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· This screenshot shows the Internet Information Services(IIS) Manager
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· This screenshot shows the ping process between the Client and the Server successfully pinging
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