Task -2
1. Sine wave (Channel A): measure time period using oscilloscope cursors
In Proteus, connect a Signal Generator to an Oscilloscope (Channel A). Set the generator to Sine, 1 kHz, 10 Vpp. Display the waveform and use the time cursors to measure one full cycle and determine the time period . Calculate the frequency.
	Time Period (s)
	Frequency (Hz)

	1 mS
	1000
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2. Square wave (Channel B): measure , frequency, , , and using oscilloscope cursors
In Proteus, connect a Signal Generator to an Oscilloscope (Channel B). Set the generator to Square, 2 kHz, 5 Vpp. Display the waveform and use the time cursors to measure the time period . Then use the cursors to measure (high time) and (low time). Calculate the frequency and use the voltage cursors to measure .
	Time Period (s)
	 (s)
	 (s) 
	Frequency (Hz)
	Peak-Peak Voltge (V)

	500 µS
	250 µs
	250 µs
	2000
	5V 
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3. Triangle wave (Channel C): measure time period using oscilloscope cursors
In Proteus, connect a Signal Generator to an Oscilloscope (Channel C). Set the generator to Triangle, 500 Hz, 6 Vpp. Display the waveform and use the time cursors to measure the time period between two identical points (peak-to-peak or zero-crossing to zero-crossing). Calculate the frequency and the amplitude.
	Time Period (s)
	Frequency (Hz)
	Amplitude (V)

	2 mS
	500
	6
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4. Sawtooth wave (Channel D): measure , frequency, and using oscilloscope cursors
In Proteus, connect a Signal Generator to an Oscilloscope (Channel D). Set the generator to Sawtooth, 5 kHz, 8 Vpp. Display the waveform and use the time cursors to measure the time period (between two successive resets). Calculate the frequency and use the voltage cursors to measure 
	Time Period (s)
	Frequency (Hz)
	 (V)

	200 µS
	5000
	8
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