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	UWTSD




	Name of Scheme: Prince of Wales Dock Foot Bridge construction

	Scheme Code:  
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	Scope of Works:
With the continuing development and growth of the Prince of Wales Dock and its surrounding areas, a new pedestrian bridge is to be constructed from the Langdon Road roundabout to the Prince of Wales Dock. Currently to gain access between the two points mentioned above, it means a pedestrian walk of 750m taking approximately 9 minutes. The new proposed footbridge will mean this can be reduced to 150m taking approximately 2 minutes. 
The moorings will look to further develop the area as a multi-use area and potentially bring further income into the University as the moorings can be hired out. 
The feasibility study will ascertain through several initial assessments whether the practicality of the footbridge and additional works is a viable option.  
The feasibility study will complete initial investigations which will look at the site location, any development constraints which can be linked to planning (planning consent, environmental issues, National resources Wales etc), the design specifications and initial design ideas for the client, estimates of cost of the programme, the phasing and length of the programme.  
This information will be presented to the client with all findings, with feedback to be received at this early stage on design, programme, costings, and any other requirements. The development of the project will also be in accordance with BIM Level 2 which is the national standard. 


· Phase 1 - Site establishment including set up of a welfare compound alongside in the car parking areas.
· Phase 2 - Establish the location of services through trial holes and C.A.T and Genny surveys. 
· Phase 3 - Begin the excavation of bridge structure, including foundations and abutments. 
· Phase 4 - Construct bridge RC concrete structure.
· Phase 5 - Lift and place all steel deck structure. 
· Phase 6 - Construct bridge deck and central lift system.
· Phase 7 – Finishing of bridge materials.
· Phase 8 - Commissioning and handover of bridge.
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1. [bookmark: _Toc330377718][bookmark: _Toc133938803]
Introduction
	
1.1. [bookmark: _Toc133938804]Purpose of this plan
It is the intention of Springfield Designs LTD that this scheme carried out as part of the UWTSD Swansea programme of improvements Swansea should be executed with the highest regard for safety, health, environmental and quality matters. 

This Site-Specific Plan (SSP) meets the requirements of the Construction Design and Management (CDM) Regulations 2015 regarding the construction phase plan. This plan describes how safety aspects of this individual scheme will be managed.  It is a live document that will be reviewed at regular intervals by the Project Manager to reflect progress of the works and changes in health and safety requirements.

This plan conforms to Springfield Designs LTD’s health and safety policy.

The plan is concerned with the overall management control of all health, safety and quality aspects in the execution of the scheme.  Subcontract works are also subject to this plan.

This plan is a ‘live document’ to be supplemented and/or revised as the scheme develops, by the introduction of supporting documents such as subcontractor method statements, risk assessments or any documentation relevant to the safety, health and environment of the project, which may include:

· Appropriate legislation
· Corporate governance
· SPD policies
· Customer requirements (to include stakeholders)
· Company processes and procedures (amend as necessary)
· Methodologies and programmes
· Organisational structures
· Supply chain requirements.

1.2. [bookmark: _Toc133938805]Authorisation
	This plan is authorised when the preparation, approval, authorisation and distribution section on page 1 is completed.
This SSP will be reviewed by the Project Manager at regular intervals and, if appropriate, amended and re-issued so that it reflects the requirements of the scheme. Reviews will be recorded on the front page of the current plan.
[bookmark: OLE_LINK3][bookmark: OLE_LINK13]Any changes made to personnel or circumstances shall be marked up in ink on the live site copy and initialled as such changes take place. 

This SSP shall be retained as a ‘hard copy’ on site. 

On completion of the scheme the final revision of the SSP must be returned to Document Control for filing on the server.



1.3. [bookmark: _Toc133938806]Contract details
These are described in the Project Execution Plan/Section 1/Paragraph 3 - Purpose.

2. [bookmark: _Toc133938807]Health and Safety Management
The key high-level objective of the contract, as stated in core module (Project Execution Plan Section 1), is to deliver the customer’s contract on time, to budget and without incident or complaint.
The key health and safety objective are to complete the contract having achieved the objectives of the company’s health and safety policy, the primary message of which is ‘100% Safe’.
The project will adopt the standards and guidance documentation described in the SPD IMS and this documentation will be used to effectively manage health and safety issues within all sub-projects.
	
2.1. [bookmark: _Toc133938808]Roles and responsibilities
All members of the site-specific team have responsibility for elements of health and safety appropriate to their function, experience and seniority and those designated as key personnel will be appointed as function holders. The Project Managers has overall responsibility for delivering the individual scheme objectives.

It is essential that everyone knows who oversees safety matters on site at any time. For Springfield Designs LTD direct safety matters, the responsibility will be that of the Springfield Designs LTD Project Manager. If the Project manager is not present then the appointed Senior Site Supervisor will be responsible for site safety

Site specific arrangements are provided in the following Appendices:
.
A list of all SHEQ activity related appointments along with their duties is available from the project SHEQ department.

2.2. [bookmark: _Toc133938809]Risk assessments and method statement (RAMS)
No activity will be permitted without an approved RAMS.
    
The project management team shall produce risk assessments where significant risks are identified.
    
2.3. [bookmark: _Toc133938810]Site specific RAMS
    Site specific RAMS will be carried out by appointed and competent personnel on site. A register
of method statements and associated risk assessments will be kept on site and reviewed.

Method statements will identify tasks, responsible personnel, control measures and monitoring
arrangements in line with the Springfield Designs LTD method statement tracking and content sheet.
Method statements will be assessed, tracked, and accepted by SPD prior to commencement of work. The contents of the method statement will be communicated to all those undertaking and associated with the work activity.

Where required the RAMS will be supplemented by Task Statements for additional low risk activities not fully covered in the RAMS.  Task Statements cannot be used in place of a full RAMS for high risk activities not covered in original document.

Contractors shall hold a signed copy at the work face while the works are taking place ensuring all
    operatives have read, understood and signed stating they will comply with the method
 

Change control for systems of work
A change control will have significant repercussions with respect to the prevention or control of accidents and may require changes in the measures taken to ensure that those risks remain as low as reasonably practicable.

Whether a change has significant repercussions will depend on the degree to which it:

· Introduces a new hazard
· Changes the risk from an existing hazard
· Affects control or mitigation measures (including off-site emergency plans).

Changes that have a positive impact on the risk profile are also important.


3. [bookmark: _Toc133938811]Safety and occupational health controls
3.1 [bookmark: _Toc133938812]Excavations and services
No works will commence until details of overhead and buried services likely to affect those works are either obtained from service providers or by direct investigation.  Details will be available as plans, drawings, cross sections and other information.  Prior to commencing works and when relevant throughout the work, SPD will obtain updated utility plans in accordance with the appropriate period as per the relevant guidance.

All excavations will be undertaken by following the relevant SPD process, standards and guidance. Service and cable avoidance will be carried out according to HSG47 and SPD LTD. The precautionary principle will apply where there is uncertainty about buried services. 

A permit to break ground will be used before beginning any excavation including trial holes and investigation.

If suspect material is discovered in an excavation, the supervisor will stop work, record and investigate the occurrence and agree actions before continuing. Given the location of the works, an archaeological watching brief will be in place excavation works in the dock.

The use of specialist equipment and explosives for excavations must be the subject of specific risk assessment and controls and consultation with the SHE department.
	
3.2 [bookmark: _Toc133938813]Emergency Arrangements
An emergency co-ordinator will be appointed for this scheme.

The emergency co-ordinator will be responsible for:

· Production of the fire and emergency plan.
· Ensuring that suitable individuals are appointment to fill key positions under the emergency plan
· Arrange drills and exercises to ensure the effectiveness of the plan
· Review and update the plan as conditions change
· Ensure any equipment essential to the operation of the plan is tested and maintained.
· Due to the isolated nature of the scheme, a satellite phone will be on site to alert the emergency services in case of an incident.

3.3 [bookmark: _Toc133938814]   Fire Precautions
   The project manager will appoint a fire co-ordinator for this scheme who will ensure that a fire risk
   assessment is made, that emergency preparedness against fire is adequate and that a fire safety plan is
   in place.

The fire co-ordinator will complete the emergency arrangements and review this on a regular basis referring deficiencies to the site / project manager for action.

Site inspections of emergency arrangements against fire will be carried out not less than fortnightly.

Where fire escape routes are long, involve stairs, buildings have multiple occupancy, or may be used by the disabled or the general public, fire drills will be carried out not less than annually.

3.4 [bookmark: _Toc133938815]Hand Arm Vibration Syndrome – HAVS
SPD has adopted a HAVS strategy, guidance is given in the IMS.  This strategy will be taken into consideration when using equipment that could potentially cause HAVS. 

Where prolonged use of vibrating tools or where vibration exposure is likely to regularly exceed the action level for a particular tool / activity, the additional items listed below should be considered and implemented where applicable:

· Tool selection
· Vibration control
· Maintain blood circulation
· Selection of operatives
· Training and awareness
· Health surveillance.

3.5 [bookmark: _Toc133938816]Health and safety rules
Health and Safety rules have been developed for the scheme by the project manager in conjunction with the SHE advisers.  Rules will be posted on notice boards in the project offices and will be included in site start-up packs for display in site offices, as well as being explained at induction.

Site rules will cover as a minimum:
· Policies including substance abuse
· Access and egress
· PPE
· Mandatory instructions
· Site boundaries
· Training and competence
· Authorised persons
· Safe methods of work
· Traffic management
· Waste
· Visitors

Minimum rules are contained in the SPD Safety policy.

3.6 [bookmark: _Toc133938817]Health Surveillance
Risk assessment will identify circumstances when health surveillance is required (unless already identified by existing legislation) and should it be deemed necessary, an occupational health surveillance programme will be undertaken. Occupational health surveillance for individuals undertaking high risk activities will include screening for any or all of the following:

· HAVS
· Noise induced hearing loss
· Manual handling
· Dermatitis from onsite operations
· Repetitive strain injuries.

3.7 [bookmark: _Toc133938818]Health and safety file
    In compliance with CDM Regulations, a health and safety file will be developed for this scheme in a 
    format agreed by relevant parties early in the project contract.  

The contents of a health and safety file will be produced may include:

· A brief description of the work carried out
· Residual hazards and how they have been dealt with
· Key structural principles incorporated in the design of the structure
· Any hazards associated with the materials used
· Information regarding the removal or dismantling of installed plant and equipment
· Health and safety information about equipment provided for cleaning or maintaining the structure
· The nature, location and markings of significant services, including firefighting services 
      Information and as-built drawings of the structure, it plant and equipment
		
3.8 [bookmark: _Toc133938819]Housekeeping
As far as is reasonably practicable, all works shall be planned, organised and executed to ensure that no unacceptable health, safety, fire, environmental or other hazard arises on or from the site.  All site staff will have a responsibility for good housekeeping, and the storage and distribution of materials to ensure that the site and activities are maintained in a clean, tidy and workmanlike manner that poses no unnecessary slip, trip and fall hazards and presents an acceptable visual impression to visitors and the general public. The storage of materials will be directed and monitored by the site foreman or supervisor. Failure of contractors to maintain standards may result in work being undertaken on their behalf and those contractors being recharged accordingly. The area is popular with tourists who will be sharing the existing access track with construction plant, the road will be kept clear at all times and all construction materials will be surrounded by fencing off the main access route. 

3.9 [bookmark: _Toc133938820]Interfaces with visitors, the public and others
Interfaces between site activities, visitors and the public will be considered when developing the site plan, planning points of site ingress / egress and works outside the site boundaries to ensure that site operations do not endanger visitors and the public.  Such consideration will apply to others such as the client’s personnel who may need access to or through the site.
	
Measures to protect the public from site activities will be taken and detailed in Site Specific Plans.

Detailed pre-construction consultation will take place with stakeholders and the local community affected by the works. Works vehicles will share the existing access track with the public for the duration of the works. All working areas will be segregated with Heras fencing. 
	
3.10 [bookmark: _Toc133938821]Lifting operations
All lifting operations will be planned and authorised in accordance with company processes, standards
and guidance SH PRO9. Where applicable the project manager will appoint a competent appointed
person for cranes and a crane supervisor.  All completed lift plans will be signed by two appointed persons prior to use.
	
All lifting machinery, equipment and gear must be checked prior to use and on arrival to site. This will
include the use of piling rigs.

Lifting documentation will specify safe zone locations.

Checks and inspections of lifting plant and equipment will be recorded in the site register..

3.11 [bookmark: _Toc133938822]Manual handling
Manual handling risk assessments must be carried out prior to manually lifting a load and must include
load weights and dimensions. Methods of assessing the risks of manual handling and consideration to
alternative methods will be considered where practical.
	
3.12 [bookmark: _Toc133938823]Material storage and distribution
The storage of materials will be planned before the sites is established to meet logistical and safety
requirements and to ensure that wastage of materials through poor storage, damage or theft is
minimised.

Suitable and adequate means of distributing materials about the site when needed will be planned
beforehand. There are several existing access bridges to be crossed to gain access to the working  area which have been subject to structural assessment and have designated weight limits. Materials will be transported using a telehandler, 6t dumper, or by 4 x 4 vehicle with trailer attached 


3.13 [bookmark: _Toc133938824]Mechanical plant
Site plant and equipment operated by SPD will be subject to Planned Preventative
Maintenance (PPM) scheme.
	
Records of plant inspections will be maintained on site and will be available for inspection. 
	
Plant and equipment operated by contractors must meet SPD and Client minimum   standards and be similarly maintained in line with legislation and with SPD minimum standards.

Details of plant and equipment operators shall be maintained and evidence of periodic checks from
plant hirers that the plant has been adequately maintained shall be obtained.

All dumpers, of 6T and over will be of a dual view specification.

3.14 [bookmark: _Toc133938825]Monitoring and inspection
Safety performance and compliance will be assessed regularly.  Records of audits, inspections and visits undertaken will be available on site.

3.15 [bookmark: _Toc133938826]Noise
If work environments are likely to exceed occupational action levels specific noise assessments will be
carried out prior to commencement of works.
    
3.16 [bookmark: _Toc133938827]Occupational health monitoring and surveillance
Requirements for occupational health monitoring will be assessed on a task specific basis and in line
with the SPD company policies process, standards and guidance.  Risk assessments may
identify circumstances when additional health surveillance is required (unless already identified by
existing legislation).

3.17 [bookmark: _Toc133938828]Permits to work
The use and issue of permits shall be in accordance with SPD permit to work systems and scheme specific requirements.

Risk assessments will identify operations or areas where permits to work are required as part of the control procedure. Only qualified and competent persons are to operate and be employed on ‘permit to work’ systems. These include for this scheme:

· Permit to break ground
· Permit to lift
· Hot works operations
· Work on non-isolated electrical equipment
· Work on isolated electrical equipment
· General permit (e.g. roof access / work in occupied premises)
· Permit to Load – Temporary works 
· Permit to pump 

3.18 [bookmark: _Toc133938829]Personal Protective Equipment (PPE)
SPD will supply to and ensure the use of PPE by all employees and visitors. Contractors will be required to supply PPE to their own personnel to the minimum requirement noted:
· Safety helmet
· Light eye protection (LEP)
· Gloves
· Safety footwear 
· Hi vis coat, jacket or vest (where there are plant movements or as directed by the project manager)

	Hi-Vis Sleeve Length

	Activity
	Mandatory Sleeve Length

	Working with Hazardous Substances
	Full Length Sleeves

	When ARC Resistant Clothing Required
	Full Length Sleeves

	Excavator/Crane Operators
	Short Sleeves Acceptable Subject to Above

	General Site Operations
	Short Sleeves Acceptable Subject to Above



The issue of PPE will be recorded.  

Other PPE required will be specified in activity RAMS.  

For all directly employed operatives working on cutting, grinding, drilling activities, the 3M Versaflow TR300+ powered air respirator and M-300 Headtop will be the first choice PPE.

3.19 [bookmark: _Toc133938830]Piling operations
Piling operations by an approved contractor must be managed in line with SPD company policies, process maps, standards and guidance.  
	
3.20 [bookmark: _Toc133938831]Safety training
    Specific health and safety training will be identified in the contract specific training and competence
    plan.
	
    Where required, site supervision will arrange for safety training associated with specific tasks such as
    abrasive wheel training.  Records of all task specific training whether delivered on or off site will be
    recorded.

    The Framework Director will ensure that Build UK standards of competence for persons employed on
    SPD projects are achieved, i.e. working towards 100% CSCS or equivalent.

3.21 [bookmark: _Toc133938832]Scaffolding
    The site team will ensure that scaffold is erected in accordance with BS EN 12811, the CDM
    Regulations 2015, National Access and Scaffolding Confederation (NASC) Guidance SG4:10, company
    standards and temporary works requirements.
Scaffolding to the dam wall will be as per TG:20-21 independent tied scaffold requirements, scaffold within the valve tower will be a designed scaffold system erected by Advanced scaffolders and inspected by an advanced scaffold inspector with a temporary works Permit to Load in place prior to use. 

3.22 [bookmark: _Toc133938833]Site office safety
    Site specific risk assessment for the site office and welfare facilities will be carried out, this will identify
    any specific hazards and controls to be adopted at that location. The site establishment and
    welfare will be in accordance with the SPDl minimum standards document in the IMS.

3.23 [bookmark: _Toc133938834]Site security
Site Security arrangements will be appropriate for the nature of the site (location, size, duration etc.). This may be manned out of hrs guarding or 24 hour CCTV cameras in operation. The scheme will have two manned guards out of hours and a gate man will be present at the site access during the day shift. 
	
3.24 [bookmark: _Toc133938835]Smoking
SPDl does not allow smoking in any building or vehicle, this includes the use of electronic cigarettes. Dedicated smoking areas on site will be identified for use by cigarette smokers. Site specific no smoking areas may be established in the vicinity of high risk activities where there is the potential for fire or explosion. 
	
3.25 [bookmark: _Toc133938836]Statutory notices
SPD will obtain the F10 notification from the CDM Manager. 
  
The project manager will arrange for a copy of the following to be posted on the site notice board (as a minimum).

· F10 notification to HSE
· Health and safety law - what you should know poster
· Employers liability insurance certificate
· Fire action notice
· First aid notice
· Site specific safety rules

3.26 [bookmark: _Toc133938837]Steel erection
    Steel erection will be carried out by a specialist contractor approved via our contractor approval process
    and will be subject to an acceptable RAMS and to proper supervision and control.  

3.27 [bookmark: _Toc133938838]Supervision
An Appointed Supervisor will always be present on site.  If the person in control leaves site, the designated deputy will be formally handed over control of the site.  If an Appointed Supervisor is not present all work will cease until supervision is available.

3.28 [bookmark: _Toc133938839]Temporary works
    Site temporary works will be co-ordinated by an appointed Temporary Works Co-ordinator (TWC) who
    will be responsible for ensuring that the planning, erection, use, maintenance and dismantling of
    temporary works is undertaken in line with SPD temporary works process and as agreed with
    the relevant Temporary Works Manager (TWM). A temporary works schedule produced at tender stage
    will be reviewed and updated at regular intervals.

    Details shall be listed in the appropriate method statements.

    A detailed RAMS including calculations and designs, and pre and post loading checks will form the
    control measures for all defined temporary works which are required for the execution of permanent
    works or temporary structures i.e. not directly connected with the permanent works.

3.29 [bookmark: _Toc133938840]Traffic management 
    All areas of work on site that involve vehicle movements and the interface with personnel will have a
    Traffic Management Plan (TMP). The TMP will be managed by an appointed person who will act as the
    Traffic Management Co-ordinator (TMC).
	
    The layout of the site will be planned to provide safe segregation between plant, vehicles and
    pedestrians wherever practical. The reversing of site plant, vans and lorries will be avoided if possible
    but where this is necessary will be under the supervision of a vehicle banksman / controller. 
    Car parking arrangements and access routes will be clearly identified, particular consideration will be
    given to the delivery, loading and offloading of materials.

Visitors, public protection and interface with others

Measures will be developed as required to ensure the protection of the public / client staff at the site which will be continually reviewed as work progresses. Security and public protection will be achieved as follows:
· Fencing or hoarding and signage in accordance with client / SPD standard requirements
· Traffic management ‘best practice’
· Security arrangements.

3.30 [bookmark: _Toc133938841]Welfare and first aid
SPD will provide welfare and first aid that exceed the minimum standards of welfare set by legislation in line with IMS Standards and Guidance.  

Sites welfare provision will generally include: offices, drying rooms, male and female toilets, canteen unit, hot water to wash hands, drinking water, means of boiling water and facilities for warming food.

SPD  will ensure that adequate numbers of first aid trained personnel and first aid kits are available at:

· All site locations
· In vehicles where this has been identified as necessary or good practice
· In strategic locations within office setups.

Posters are displayed stating location of first aid boxes, first aiders, appointed persons and action to be taken in case of an incident.

3.31 [bookmark: _Toc133938842]Working at height
    SPD  will ensure that all areas that can be deemed as working at height has a suitable risk
    assessment and method statement in place. Working at height may include working from platforms,
    structures and or above excavations, shafts, manholes and voids. 

3.32 [bookmark: _Toc133938843]Working over or adjacent to water
Any work over or adjacent to a body of water (e.g. river, stream, reservoir, pond, estuary or sea) will be subject to specific risk assessment and in accordance with IMS standards and guidance. Life buoys will be present alongside the reservoir embankments. Where works over / within water are required they will be subject to a full risk assessment and method statement. 


[bookmark: _Toc133938844]4.0     Environmental Management
The detailed SSP for the environmental management of this scheme is provided in a separate dedicated Environmental Management Plan for the scheme.  Environmental management will be in accordance with the project Environmental Management Plan and Register of Environmental Effects therein.
[bookmark: _Hlk30593035]
[bookmark: _Toc133938845]5.0     Quality Management
The key scheme objective is to deliver the customer’s contract on time, to budget and without incident or complaint. Quality management will be in accordance with the SPD quality policy MS POL 02 and IMS process QPRO which ensures efficient and effective arrangements are in place for quality management and assurance. 
		All members of the site team have responsibility for elements of quality appropriate to their function, experience and seniority.  
Quality Control will be achieved through self-certification by means of inspection, testing and monitoring.  Materials and works will undergo interim and final inspections or tests against design drawings, specifications or other requirements.  The company’s commitment to perfect delivery seeks to gain customer approvals and acceptance for materials and works which forms part of the scheme.
	The quality control arrangements are defined within QPRO1 on the company IMS.

The key documents to plan and manage quality activities will be Inspection and Test Plans (ITPs) which the site team will develop for the scheme. The scope of tests and their frequencies will conform to the specification explicit or implicit requirements.  ITPs will show hold points where physical inspection or written approval to proceed is required (PM FRM26). A copy of the Inspection and Test Plan is included in Appendix O.  This will be completed to identify inspection and testing required for this specific scheme.
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Appendix D
Pre-construction Information
(CDM Regulations)
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Appendix E
Emergency Action Checklist








































Emergency Action Checklist   (Note: To be completed during the project for each designated place of construction)

	
	
	YES
	
	NO
	
	N/A

	1. 
	Has an emergency assembly point been established
	
	
	
	
	

	2. 
	Has an emergency incident risk assessment been carried out
	
	
	
	
	

	3. 
	Have appropriate fire, first aid and spill response points been established
	
	
	
	
	

	4. 
	Is a means of raising the alarm available
	
	
	
	
	

	5. 
	Have the relevant Fire Wardens/Incident Controllers been appointed
	
	
	
	
	

	6. 
	Have they received appropriate training/instruction
	
	
	
	
	

	7. 
	Has a suitable monitoring and maintenance regime for emergency equipment been established for all working areas
	
	
	
	
	

	8. 
	Are electrical instalation details available including relevant isolation points etc
	
	
	
	
	

	9. 
	Have designated storage areas been identified for flammable liquids/materials
	
	
	
	
	

	10. 
	Are there appropriate fire/safety signs posted at the relevant positions
	
	
	
	
	

	11. 
	Have relevant incident reporting procedures been established for the project
	
	
	
	
	

	12. 
	Have designated Smoking or No Smoking areas been established where appropriate
	
	
	
	
	

	13. 
	Is there a permit to work procedure required for any activity
	
	
	
	
	

	14. 
	If yes, is there a procedure in place
	
	
	
	
	

	15. 
	Are fire and emergency precautions detailed in the site induction
	
	
	
	
	

	16. 
	Has/Is there liaison with the relevant emergency services or enforcing authority ie. Fire Brigade, EA etc.
	
	
	
	
	

	17. 
	Are all maintenance, inspection details recorded and available for inspection
	
	
	
	
	

	18. 
	Are regular fire/emergency drills carried out
	
	
	
	
	

	19. 
	Have they been recorded
	
	
	
	
	

	20. 
	Is there appropriate First Aid cover (consider also 24 hour working).
	
	
	
	
	





















Appendix F
Table of Contact Numbers, Emergency Service Details and Emergency Telephone Numbers

































SSP Appendix F
Table of Contact Numbers, Emergency Service Details                                                 and Emergency Telephone Numbers
	Welsh Water (UU) 
	Control Room
	08000520130 (24hrs)

	Enforcing Authorities

	Natural Resources Wales (see Appendix A for site specific NRW)
Health & Safety Executive
	
	0300 065 3000 

02920 263000

	[bookmark: _Toc459796107]Emergency Services

	Police
	Emergency Service
	999 or 112

	Ambulance
	Emergency Service
	999 or 112

	Local & Regional Hospital
	 (see Appendix A for site specific hospital)

	Gas
	Gas Leak
	0800 111999

	Electricity
	Power Cut
	0800 052 0400

	Other 

	Occupational Health Service

	Provided by Hampton Knight

	Contact Nicola Rowlands 07808905464 (M) 


























Appendix G
Site Specific Layout Plan





























Appendix H
Site Specific Hospital Location Map
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Project Specific Information


























Appendix J
Permits to Work Required










































Appendix K
F10
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Appendix L
Additional Site Specific Information















































Appendix M
Site First Aid Assessment











































	Issue Date:
	 03.05.2023
	Review Date:
	03.05.2024

	Assessors:
	Sarah Eynon 

	Name of Scheme:
	Prince of Wales Dock  

	Site Address:
	Prince of Wales Dock, SA1

	Access Route:
	Langdon Road Via A483/ Kings Road near UWTSD Swansea Campus

	Nearest Hospital:
	Morriston Hospital, Swansea 

	Distance to Hospital:
	6 Miles 
	Estimated Travel Time:
	25 hour 

	Location of Accident Book:
	SPD SHEQ Tracker (Info Exchange)

	Emergency Numbers:
	Ambulance/Police
	999

	

	

	

	

	

	

	

	

	Activity Risk:
	High

	

	Specific Hazards on Site
	Potential Injuries
	Tick

	Working at Height
	Major Injuries, Lacerations, Fractures, Head Trauma, Blood Loss
	

	Hazardous Substances
	Burns, Skin Contamination, Asphyxiation, Eye Splashes, Ingestion
	

	Working in Excavations
	Fractures, Lacerations, Crush Injuries, Exhaustion, Shock
	

	Manual Handling
	Fractures, Lacerations, Strains, Sprains, Spinal Injuries, Blood Loss
	

	Moving Plant
	Crush Injuries, Fractures, Lacerations, Head Trauma, Blood Loss
	

	Working with Electricity
	Electric Shock, Burns, Shock, Full Body Trauma, Cardiac Trauma, 
	

	Working with Sewage
	Asphyxiation, Skin Contamination, Eye Splashes, Ingestion
	n/a 

	Slips, Trips and Falls
	Fractures, Lacerations, Head Trauma, Shock, Blood Loss
	

	Use of Hand Tools
	Electric Shock, Lacerations, Eye Injuries, Fractures, Bruising
	

	Working Near Water
	Unconsciousness, Shock, Hypothermia, Head Injuries, Laceratio7ns
	

	Fire / Hot Works
	Burns, Shock, Eye Injuries
	

	Lifting Operations
	Crush Injuries, Fractures, Head Trauma, Lacerations, Bruising
	

	Violence at Work
	Shock, Head Injuries, Fractures, Bruising, Blood Loss
	



	
	SITE SPECIFIC CONTROL MEASURES.

	1. 
	First aiders will be indicated on site by posters which contain a photograph and the name of the appointed first aider/s for the given work area/site.

	2. 
	The duty of the first aider is to provide basic first aid without putting themselves at risk until the arrival of the emergency services, until the casualty is taken to hospital or the injured party returns to work or leaves site.

	3. 
	First aiders are not to provide first aid outside of working hours on behalf of SPD Plc.

	4. 
	First aiders will ensure that all incidents that require them to administer first aid are reported to the HSE department at Nelson. They are to ensure that all details of treated persons are forwarded to the HSE department at the earliest opportunity.

	5. 
	First aiders are to ensure that all first aid facilities are clearly identified and appropriate signage is in place to identify the appointed first aiders.

	6. 
	First aiders are not permitted to administer prescribed or non-prescribed medicines to any employee.

	7. 
	All welfare facilities are to be equipped with first aid facilities and located in a prominent position to allow easy access and immediate identification. These are to be inspected and maintained by the appointed first aiders for that site or location.

	8. 
	First aiders will protect themselves against blood born infections whilst administering first aid. First aid kits contain protective gloves for use whilst administering first aid. These are to be worn whilst first aid is being administered.

	9. 
	First aiders are to inform the HSE department of any illness, which would affect their ability to perform first aid functions or any illness they believe has resulted from administering first aid.

	10. 
	In the event of an emergency that requires first aid attention the designated first aider for the site is to attend immediately and administer first aid to the affected party and record the details of any treatment administered. The designated first aider will seek assistance should they feel it necessary this may be from additional first aiders or from the emergency services by dialling 999. In cases of severe injury consideration must be made to call the emergency services to convey a casualty to the nearest hospital.

	11. 
	In the event of any incident requiring the attendance of the Emergency services, raise the alarm by dialling 999. The caller should be prepared to give their name, location and nature of the emergency. A satellite phone will be available on site for use in case of an emergency.

	12. 
	Suitable bio hazard disposable bags (yellow) will be available on the site, these are to be used for the disposal of biologically contaminated items i.e. blood soiled. It is the responsibility of the first aider to arrange disposal of contaminated items at a convenient hospital incinerator unit, or alternatively if an ambulance is in attendance the contaminated items can be passed to the ambulance crew for disposal.




	
REVIEW & MONITORING.

1. Maintain current controls as listed above.
2. Ensure first aid boxes and eye wash stations are located at the points indicated by signage.
3. Maintain system of ensuring first aid boxes are fully stocked at all times.
4. Ensure training and competence is kept at a suitable standard for all first aiders.
5. Ensure all instances of first aid administration are reported to the SHEQ department.
6. Review this risk assessment template to ensure its suitability to reflect current working practices and trends.
7. All personnel on site to sign that they have read and understood this assessment.

	APPENDIX

	Risk Level
	Type of Workplace
	No of First Aiders Required

	Lower Ris
	Shops, offices, libraries and similar workplaces.
	Fewer than 50 employed at any location; at least one appointed person.

50-100; at least one first aider.

More than 100; one additional first aider for every 100 employed.

	Medium Risk
	Light engineering, assembly work, food processing, warehousing and similar workplaces.
	Less than 20: at least one appointed person

20-100: at least one first aider for every 50 employed (or part thereof).

More than 100: one additional first-aider for every 100 employed.

	Higher Risk
	Most construction, slaughter-houses, chemical manufacture, extensive work with dangerous machinery or sharp instruments and similar workplaces

	Fewer than 5: at least one appointed person

5-50: At least one first aider.

More than 50: one additional first-aider for every 50 employed.






	WE THE UNDERSIGNED HAVE RECEIVED, READ AND UNDERSTOOD THE RISKS AND THE
SPECIFIC PRECAUTIONS LISTED ABOVE:

	NAME (Print)
	COMPANY IF OTHER EMPLOYEES AFFECTED
	SIGNATURE
	DATE
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