Networking Lab 2

Step 1
Why were the pings not successful?
The pings were unsuccessful because the interface ports on the router were not activated for the ping tests

Step 2 
Were the pings successful? Why?
The pings were successful this time because the two interface ports on the router had been activated and configured 

Part 3 Display device information
Step 1
Router
a. Use the show version command to answer the following questions about the router.
What is the name of the IOS image that the router is running?
Cisco IOS software, C1900 Software (C1900-UNIVERSALK9-M), Version 15.1(4) M4, release software (fc2)

How much DRAM memory does the router have?
491520KB/32768KB

How much NVRAM memory does the router have?
255KB

How much Flash memory does the router have?
249856KB 

Switch 
What is the name of the IOS image that the switch is running?
C2960 Software (C2960-LANBASE-M), Version 12.2(25)FX

How much dynamic random access memory (DRAM) does the switch have?
21039KB 

How much nonvolatile random-access memory (NVRAM) does the switch have?
[bookmark: _GoBack]63488KB 





