	

	METHOD STATEMENT 
PLUMBING WORKS
	
               Effective: 08/02/2022



	PERSON COMPLETING
	Adam George

	PROJECT TITLE
	
POBL-SA1, Swansea

	SUPERVISOR
	Adam George
	OPERATIVES.
	

	EMERGENCY CONTACT
	Adam George - 07432469686
	SERVICES - 999

	START DATE
	23/05/2022
	COMPLETION DATE
	10/08/2022

	METHOD OF WORK
Deliveries
Where practicable arrange deliveries of materials to times where other traffic is at lowest level. Establish unloading point and control access to ensure non-construction personnel/visitors and residents of the site are excluded from vehicle movement, unloading and storage points.
Inspect load before unloading from vehicle and ensure only necessary site personnel are in vicinity of unloading. Ensure all joists and decking boards are stored in a dry area away from sources of potential damage.

Set-up
Remove all debris from work areas. Dispose of debris in designated areas.
Remove unnecessary obstructions and debris from plot and deposit in waste receptacles or designated storage. Ensure that concrete floor has been swept and all rubble cleaned from the area.
Ensure working environment is free from any materials or tools that will not be used.

Plumbing work
Liaise with site manager/supervisor for approval to isolate water supplies.
Isolate Hot & cold water pipes where necessary. Tag isolation points to warn against turning supply back on. Drain down the water system where necessary.
Carry out replacement of parts or repairs.
Ensure waste pipes and other plastic pipe work are connected correctly.
Where plastic pipe is connected with solvents, operatives will follow all safe use instructions. Where solder work has to be carried out, prepare pipe work for solder joints.
Obtain the appropriate hot work permit from the site manager/supervisor. Ensure the correct type of fire extinguisher is on hand during hot work.
Protect surrounding area with heat shields. Ensure adequate ventilation for solder work. Connect and solder all necessary joints.
Check all joints.
Liaise with site manager/supervisor for approval to turn water supplies back. Carry out further checks for water tightness and quality of finish.

Fitting A Kitchen Or Utility Sink
Use all equipment according to manufacturer’s instruction and perform a visual check.
Ensure correct PPE is worn.
Fit the sink in worktop and secure with clips provided. Connect the trap, waste, hot and cold feeds.
Copper pipework to be installed, take care to prevent fire during hot work. Ensure the correct type of fire extinguisher is on hand during hot work.
Protect surrounding area with heat shields.
Ensure adequate natural ventilation to remove fume during solder work. Prepare all fittings, apply flux, connect and solder all joints.
Seal around the sink ware with clear mastic to work top surface. Test for correct operation, i.e. HOT (left), COLD (Right).
Visually inspect pipe work and joints for leaks and damage.
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[bookmark: _Hlk92788253]Fitting Radiators
Measure up wall for radiator brackets and mark out. Inspect the walls for live services.
Inspect all tools for damage etc. prior to use. Protect floor area from dust created while drilling. Wear correct PPE as specified.
If no live services found drill wall, install proprietary fixings and mount brackets. Screw brackets into place.
Prepare radiator valves, bleed valve and plug using PTFE tape to seal threads and secure. Mount radiator onto the brackets.
Once piping is installed offer up pipe to valves and tightens. Complete installation of all radiators and check system is connected. Fill with water and pressurise.
Bleed all radiators.
Visually inspect system pipe work and joints for leaks and damage. Flush and drain system prior to refill with inhibitor.
Reinstate system.

Fitting Sanitary Wear
Mark out the position of all sanitary wear.
Fit the bath or shower base as per the manufacturer instruction. Ensure feet are mounted on robust floor, or add pattress blocks. Secure to wall using suitable proprietary fixings.
Drill, plug and fix the supports for the sink, toilet and bidet (if applicable) using suitable proprietary fixings. Fit the sink and pedestal (if applicable).
Fabricate and install waste pipes and traps.
Where a plastic pipe is connected with solvents, staff will follow all safe use instructions. Connect the waste pipes to traps and check for leaks.
Position WC and connect to soil pipe ensuring seal is aligned correctly. Make up plastic pipework and connect to hot and cold water feeds.
Where water feeds are made up in copper, care must be taken to prevent fire during hot work. Ensure the correct type of fire extinguisher is on hand during hot work.
Protect surrounding area with heat shields.
Ensure adequate natural ventilation to remove fume during solder work. Prepare all fittings, apply flux, connect and solder all joints.
Fit the shower enclosure as per the manufacturer instruction.
Seal around the sanitary wear using a sanitary silicone in either white or clear. Drill, plug and fix any accessories.
Ensure all plugs, handles taps and other ancillaries are correctly fitted to sanitary ware.
Test for correct operation including WC cistern capacity, float valve adjustment, flushing of toilet and emptying of water through plugs and overflows.
Visually inspect pipe work and joints for leaks and damage both internally and externally.


Clean up.
Ensure all debris is removed at the completion of work period and deposit into waste receptacles provided. At end of task clean tools. Leave all areas in clean condition.




	Document Approved by: (Print)
Adam George
	Signature:
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	Position:

Site Manager
	Date:



	I understand the information presented in this document and will work in line with the stated method
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