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Lab - Building an Ethernet Crossover Cable

Lab – Understanding Ethernet Cable Standards 
Topology
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Addressing Table
	Device
	Interface
	IP Address
	Subnet Mask
	Default Gateway

	PC-A
	NIC
	192.168.10.1
	255.255.255.0
	N/A

	PC-B
	NIC
	192.168.10.2
	255.255.255.0
	N/A


Objectives
Part 1: Analyze Ethernet Cabling Standards and Pinouts
Part 2: Build an Ethernet Crossover Cable
Part 3: Test an Ethernet Crossover Cable
Background / Scenario
In this lab, you will build and terminate an Ethernet crossover cable and test it by connecting two PCs together and pinging between them. You will first analyze the Telecommunications Industry Association/Electronic Industries Association (TIA/EIA) 568-A and 568-B standards and how they apply to Ethernet cables. You will then construct an Ethernet crossover cable and test it. Finally, you will use the cable you just constructed to connect two PCs together and test it by pinging between them.
Note: With autosensing capabilities available on many devices, such as the Cisco 1941 Integrated Services Router (ISR) switch, you may see straight-through cables connecting like devices.
Required Resources
One length of cable, either Category 5 or 5e. Cable length should be 0.6 to 0.9m (2 to 3 ft.)
2 RJ-45 connectors
RJ-45 crimping tool
Wire cutter
Wire stripper
Ethernet cable tester (optional)
2 PCs (Windows 7 or 8)
Analyze Ethernet Cabling Standards and Pinouts
The TIA/EIA has specified unshielded twisted pair (UTP) cabling standards for use in LAN cabling environments. TIA/EIA 568-A and 568-B stipulates the commercial cabling standards for LAN installations; these are the standards most commonly used in LAN cabling for organizations and they determine which color wire is used on each pin.
With a crossover cable, the second and third pairs on the RJ-45 connector at one end of the cable are reversed at the other end, which reverses the send and receive pairs. The cable pinouts are the 568-A standard on one end and the 568-B standard on the other end. Crossover cables are normally used to connect hubs to hubs or switches to switches, but they can also be used to directly connect two hosts to create a simple network.
Reflection: 
Write a research report (Max word count 600) on Cat 5e and 6 Ethernet cable standards.  
Report at bottom of the document.
Analyze diagrams and tables for the TIA/EIA 568-A standard Ethernet cable.
The following table and diagrams display the color scheme and pinouts, as well as the function of the four pairs of wires used for the 568-A standard. 
Note: In LAN installations using 100Base-T (100 Mb/s), only two pairs out of the four are used.
568-A 10/100/1000Base-TX Ethernet
	Pin Number
	Pair Number
	Wire Color
	10Base-T Signal
100Base-TX Signal
	1000Base-T Signal

	1
	2
	White/Green
	Transmit
	BI_DA+

	2
	2
	Green
	Transmit
	BI_DA-

	3
	3
	White/Orange
	Receive
	BI_DB+

	4
	1
	Blue
	Not Used
	BI_DC+

	5
	1
	White/Blue
	Not Used
	BI_DC-

	6
	3
	Orange
	Receive
	BI_DB-

	7
	4
	White/Brown
	Not Used
	BI_DD+

	8
	4
	Brown
	Not Used
	BI_DD-




The following diagrams display how the wire color and pinouts align with an RJ-45 jack for the 568-A standard.
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Analyze diagrams and tables for the TIA/EIA 568-B standard Ethernet cable.
The following table and diagram display the color scheme and pinouts for the 568-B standard.
568-B 10/100/1000-BaseTX Ethernet
	Pin Number
	Pair Number
	Wire Color
	10Base-T Signal
100Base-TX Signal
	1000Base-T Signal

	1
	2
	White/Orange
	Transmit
	BI_DA+

	2
	2
	Orange
	Transmit
	BI_DA-

	3
	3
	White/Green
	Receive
	BI_DB+

	4
	1
	Blue
	Not Used
	BI_DC+

	5
	1
	White/Blue
	Not Used
	BI_DC-

	6
	3
	Green
	Receive
	BI_DB-

	7
	4
	White/Brown
	Not Used
	BI_DD+

	8
	4
	Brown
	Not Used
	BI_DD-
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Build an Ethernet Crossover Cable
A crossover cable has the second and third pairs on the RJ-45 connector at one end, reversed at the other end (refer to the table in Part 1, Step 2). The cable pinouts are the 568-A standard on one end and the 568-B standard on the other end. The two following diagrams illustrate this concept.
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Build and terminate a TIA/EIA 568-A cable end.
Determine the cable length required. (Your instructor will let you know the cable length you should make.)
Note: If you were making a cable in a production environment, the general guideline is to add another 12 in. (30.48 cm) to the length.
Cut off a piece of cable to the desired length and using your wire stripper, remove 5.08 cm (2 in.) of the cable jacket from both ends.
Hold the four pairs of twisted cables tightly where the jacket was cut away. Reorganize the cable pairs into the order of the 568-A wiring standard. Refer to the diagrams, if necessary. Take as much care as possible to maintain the twists in the cable; this provides noise cancellation.
Flatten, straighten, and line up the wires using your thumb and forefinger.
Ensure that the cable wires are still in the correct order for the 568-A standard. Using your wire cutters, trim the four pairs in a straight line to within 1.25 to 1.9 cm (1/2 to 3/4 in.).
Place an RJ-45 connector on the end of your cable, with the prong on the underside pointing downward. Firmly insert the wires into the RJ-45 connector. All wires should be seen at the end of the connector in their proper positions. If the wires are not extending to the end of the connector, take the cable out, rearrange the wires as necessary, and reinsert the wires back into the RJ-45 connector.
If everything is correct, insert the RJ-45 connector with cable into the crimper. Crimp down hard enough to force the contacts on the RJ-45 connector through the insulation on the wires, thus completing the conducting path. See the following diagram for an example.
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Build and terminate a TIA/EIA 568-B cable end.
Repeat steps 1a to 1g using the 568-B color wiring scheme for the other end.
Test an Ethernet Crossover Cable
Test the cable.
Many cable testers will test for length and mapping of wires. If the cable tester has a wire map feature, it verifies which pins on one end of the cable are connected to which pins on the other end.
If your instructor has a cable tester, test the crossover cable for functionality. If it fails, check with your instructor first as to whether you should re-cable the ends and re-test.
Connect two PCs together via NICs using your Ethernet crossover cable.
Working with a lab partner, set your PC to one of the IP addresses shown in the Addressing Table (see page 1). For example, if your PC is PC-A, your IP address should be set to 192.168.10.1 with a 24-bit subnet mask. You partner’s IP address should be 192.168.10.2. The default gateway address can be left empty.
Using the crossover cable you made, connect the two PCs together via their NICs.
On the PC-A command prompt, ping the PC-B IP address.
Note: The Windows firewall may have to be temporarily disabled for pings to be successful. If the firewall is disabled, make sure you re-enable it at the conclusion of this lab.
Repeat the process and ping from PC-B to PC-A.
Assuming IP addressing and firewall are not issues, your pings should be successful if the cables were properly made.
Reflection
Which part of making cables did you find the most difficult?
The part I had the most trouble with was fitting the cables into the modular plugs (RJ45) 

Why do you have to learn how to make a cable if you can easily buy pre-made cables?
We have to learn how to make the cables as it should be known by everyone who studies networking how to make a simple ethernet cable. Being able to make the cables is also a lot cheaper than buying them from shops. The cables can also be at a customized length if you were to build them on your own.
Ethernet cable Standards
Cat 5e
Cat 5e stands for category 5 Enhanced cabling. Cat 5e cables are typically 24 gauge twisted pair wires which can produce a gigabit network speed at distances from up to 328ft which would included patch cables at each end. A lot of people will still use Cat 5e cables as networks will be on the cloud in most cases. What this means for the cable is that there really isn’t any need for higher demands on the internal speeds. The cat 5e cables will also be used at smaller distances in comparison to the Cat 6 cables. Cat 5e cables are also roughly 30% cheaper than the Cat 6 cables which is somewhat useful in a situation where money is a big factor [1]. While category 5e was being standardized there was already proposals of Category 6 cables as a new specification. What these different specifications were, were higher frequency ranges from 100 up to 200and lower attenuation. Attenuation being the loss of signal power as a signal propagates from one transmitter at one end of the cable toward a receiving device located at the end of the cable [2]. You would also use Cat 5e cables for data transmission as it can support up to 1000Mbps but it is not recommended to use it for the maximum speed that it can reach as it may cause some crosstalk within the wire causing some minor data loss [3].
Cat 6
[bookmark: _GoBack]The Cat 6 standard cable can sometimes be 23gauge and sometimes Cat 6 will have a piece of plastic in the middle of the cable that splits the pairs apart. This is done to supposedly further the limit of crosstalk. Crosstalk means the amount of noise that is made when the cable is working and having more of it will slow down the speed of the network [1]. The frequency that this cable type can vary from are 0-500 which would be the maximum. The cable can also theoretically reach speeds of up to 10Gbps over 33 to 55 meters of cable. It is argued that having to pay the small price is worth when it comes to buying the cable as eventually all hardware gets upgraded and having to pay such a small difference is worth it especially due to the higher speeds the cable can reach [4]. After you compare these two standards you wouldn’t necessarily consider Cat 5e to be useless as you would still use it in most day to day situations such as a home network or anything on a smaller scale. If you were in a big office building that needed high speed networks you would probably make use of the Cat 6 cables as it’d be a lot more efficient. Like previously mentioned for Cat 5e you would use Cat 6 cables for data transmission more than any other cable. There is also a separator added between each pair of wires allowing it to function at higher speeds [3]. In general the Cat6 cable will overall statistically be a improved version of Cat5 as that’s how you’d expect the evolution of the cables to go.
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