Packet tracer – Trouble shooting GRE

Part 1:     Find and Correct All Network Errors.
	Device
	Error
	Correction

	 RA
	The IP address for Tunnel 0 and G0/0 is swapped. 
 
 
	 The tunnel 0 ip address is supposed to be 192.168.1.1 255.255.255.252.

The IP address for G0/0 is supposed to be 172.31.0.1 255.255.255.0

	 RA
	The route for the private IP address was configured wrong for the next hop address
 
 
 
	The route for private ip address next hop 172.31.1.0 255.255.255.0 192.168.1.2

	 RB
	 The source interface is incorrect and the destination address is a private IP
 
 
 
	Change source interface to s0/0/0 and the destination address to 209.165.122.2



