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Building configuration...

Current configuration : 2305 bytes
!
version 12.2
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname S1
!
!
!
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
interface FastEthernet0/1
switchport mode trunk
!
interface FastEthernet0/2
switchport access vlan 5
switchport mode trunk
!
interface FastEthernet0/3
switchport access vlan 5
switchport mode access
!
interface FastEthernet0/4
switchport access vlan 5
switchport mode access
!
interface FastEthernet0/5
switchport access vlan 5
switchport mode access
!
interface FastEthernet0/6
switchport access vlan 21
switchport mode access
!
interface FastEthernet0/7
switchport access vlan 5
switchport mode access
!
interface FastEthernet0/8
switchport access vlan 6
switchport mode access
!
interface FastEthernet0/9
switchport access vlan 6
switchport mode access
!
interface FastEthernet0/10
switchport access vlan 6
switchport mode access
!
interface FastEthernet0/11
switchport access vlan 6
switchport mode access
!
interface FastEthernet0/12
switchport access vlan 6
switchport mode access
!
interface FastEthernet0/13
switchport access vlan 6
switchport mode access
!
interface FastEthernet0/14
switchport access vlan 6
switchport mode access
!
interface FastEthernet0/15
switchport access vlan 7
switchport mode access
!
interface FastEthernet0/16
switchport access vlan 7
switchport mode access
!
interface FastEthernet0/17
switchport access vlan 7
switchport mode access
!
interface FastEthernet0/18
switchport access vlan 7
switchport mode access
!
interface FastEthernet0/19
switchport access vlan 7
switchport mode access
!
interface FastEthernet0/20
switchport access vlan 7
switchport mode access
!
interface FastEthernet0/21
switchport access vlan 8
switchport mode access
!
interface FastEthernet0/22
switchport access vlan 8
switchport mode access
!
interface FastEthernet0/23
switchport access vlan 8
switchport mode access
!
interface FastEthernet0/24
switchport access vlan 8
switchport mode access
!
interface GigabitEthernet0/1
!
interface GigabitEthernet0/2
!
interface Vlan1
ip address 192.168.1.3 255.255.255.0
shutdown
!
ip default-gateway 192.168.1.1
!
!
!
!
line con 0
!
line vty 0 4
login
line vty 5 15
login
!
!
!
!
end
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Building configuration...

Current configuration : 2326 bytes
!
version 12.2
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname S2
!
!
!
no ip domain-lookup
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
interface FastEthernet0/1
switchport mode trunk
!
interface FastEthernet0/2
switchport access vlan 5
switchport mode access
!
interface FastEthernet0/3
switchport access vlan 5
switchport mode access
!
interface FastEthernet0/4
switchport access vlan 5
switchport mode access
!
interface FastEthernet0/5
switchport access vlan 5
switchport mode access
!
interface FastEthernet0/6
switchport access vlan 5
switchport mode access
!
interface FastEthernet0/7
switchport access vlan 5
switchport mode access
!
interface FastEthernet0/8
switchport access vlan 6
switchport mode access
!
interface FastEthernet0/9
switchport access vlan 6
switchport mode access
!
interface FastEthernet0/10
switchport access vlan 6
switchport mode access
!
interface FastEthernet0/11
switchport access vlan 6
switchport mode access
!
interface FastEthernet0/12
switchport access vlan 6
switchport mode access
!
interface FastEthernet0/13
switchport access vlan 6
switchport mode access
!
interface FastEthernet0/14
switchport access vlan 6
switchport mode access
!
interface FastEthernet0/15
switchport access vlan 7
switchport mode access
!
interface FastEthernet0/16
switchport access vlan 7
switchport mode access
!
interface FastEthernet0/17
switchport access vlan 7
switchport mode access
!
interface FastEthernet0/18
switchport access vlan 23
switchport mode access
!
interface FastEthernet0/19
switchport access vlan 7
switchport mode access
!
interface FastEthernet0/20
switchport access vlan 7
switchport mode access
!
interface FastEthernet0/21
switchport access vlan 8
switchport mode access
!
interface FastEthernet0/22
switchport access vlan 8
switchport mode access
!
interface FastEthernet0/23
switchport access vlan 8
switchport mode access
!
interface FastEthernet0/24
switchport access vlan 8
switchport mode access
!
interface GigabitEthernet0/1
!
interface GigabitEthernet0/2
!
interface Vlan1
ip address 192.168.1.2 255.255.255.0
shutdown
!
ip default-gateway 192.168.1.1
!
!
!
!
line con 0
!
line vty 0 4
login
line vty 5 15
login
!
!
!
!
end
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Building configuration...

Current configuration : 2521 bytes
!
version 12.2
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname Branch1
!
!
!
!
ip dhcp excluded-address 192.168.5.1 192.168.5.10
ip dhcp excluded-address 192.168.6.1 192.168.6.10
ip dhcp excluded-address 192.168.7.1 192.168.7.10
ip dhcp excluded-address 192.168.8.1 192.168.8.10
!
ip dhcp pool vlan5
network 192.168.5.0 255.255.255.0
default-router 192.168.5.1
dns-server 209.165.200.25
ip dhcp pool vlan6
network 192.168.6.0 255.255.255.0
default-router 192.168.6.1
dns-server 209.165.200.25
ip dhcp pool vlan7
network 192.168.7.0 255.255.255.0
default-router 192.168.7.1
dns-server 209.165.200.25
ip dhcp pool vlan8
network 192.168.8.0 255.255.255.0
default-router 192.168.8.1
dns-server 209.165.200.25
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
!
!
!
!
!
!
no ip domain-lookup
!
!
!
!
!
!
!
!
interface Loopback2
ip address 192.168.2.1 255.255.255.252
!
interface Loopback3
ip address 192.168.3.1 255.255.255.252
!
interface Loopback4
ip address 192.168.4.1 255.255.255.252
!
interface Loopback5
no ip address
!
interface Loopback6
no ip address
!
interface FastEthernet0/0
no ip address
duplex auto
speed auto
shutdown
!
interface FastEthernet1/0
no ip address
duplex auto
speed auto
shutdown
!
interface Serial2/0
ip address 10.10.4.1 255.255.255.252
!
interface Serial3/0
no ip address
clock rate 2000000
shutdown
!
interface FastEthernet4/0
no ip address
shutdown
!
interface FastEthernet5/0
no ip address
shutdown
!
interface GigabitEthernet6/0
no ip address
duplex auto
speed auto
!
interface GigabitEthernet6/0.1
encapsulation dot1Q 1 native
ip address 192.168.1.1 255.255.255.0
!
interface GigabitEthernet6/0.5
encapsulation dot1Q 5
ip address 192.168.5.1 255.255.255.0
!
interface GigabitEthernet6/0.6
encapsulation dot1Q 6
ip address 192.168.6.1 255.255.255.0
!
interface GigabitEthernet6/0.7
encapsulation dot1Q 7
ip address 192.168.7.1 255.255.255.0
!
interface GigabitEthernet6/0.8
encapsulation dot1Q 8
ip address 192.168.8.1 255.255.255.0
!
interface GigabitEthernet6/0.9
encapsulation dot1Q 9
ip address 192.168.9.1 255.255.255.0
!
interface GigabitEthernet7/0
no ip address
duplex auto
speed auto
shutdown
!
router rip
network 10.0.0.0
network 192.168.1.0
network 192.168.5.0
network 192.168.6.0
network 192.168.7.0
network 192.168.8.0
network 209.165.200.0
!
ip classless
!
ip flow-export version 9
!
!
!
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
login
!
!
!
End
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Building configuration...

Current configuration : 1066 bytes
!
version 12.2
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname HQ
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
!
!
!
!
!
!
no ip domain-lookup
!
!
!
!
!
!
!
!
interface Loopback1
ip address 1.1.1.1 255.255.255.0
!
interface FastEthernet0/0
no ip address
duplex auto
speed auto
shutdown
!
interface FastEthernet1/0
no ip address
duplex auto
speed auto
shutdown
!
interface Serial2/0
ip address 10.10.4.2 255.255.255.252
clock rate 2000000
!
interface Serial3/0
ip address 10.10.10.2 255.255.255.252
!
interface FastEthernet4/0
no ip address
shutdown
!
interface FastEthernet5/0
no ip address
shutdown
!
interface GigabitEthernet6/0
ip address 209.165.200.30 255.255.255.248
duplex auto
speed auto
!
router rip
network 10.0.0.0
network 192.168.1.0
network 192.168.5.0
network 192.168.6.0
network 192.168.7.0
network 192.168.8.0
network 209.165.200.0
!
ip classless
!
ip flow-export version 9
!
!
!
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
login
!
!
!
end
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Building configuration...

Current configuration : 920 bytes
!
version 12.2
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname Branch2
!
!
!
!
!
!
!
!
ip cef
no ipv6 cef
!
!
!
!
!
!
!
!
!
!
no ip domain-lookup
!
!
!
!
!
!
!
!
interface FastEthernet0/0
no ip address
duplex auto
speed auto
shutdown
!
interface FastEthernet1/0
no ip address
duplex auto
speed auto
shutdown
!
interface Serial2/0
ip address 10.10.10.1 255.255.255.252
clock rate 2000000
!
interface Serial3/0
no ip address
clock rate 2000000
shutdown
!
interface FastEthernet4/0
no ip address
shutdown
!
interface FastEthernet5/0
no ip address
shutdown
!
router rip
network 10.0.0.0
network 192.168.1.0
network 192.168.5.0
network 192.168.6.0
network 192.168.7.0
network 192.168.8.0
network 209.165.200.0
!
ip classless
!
ip flow-export version 9
!
!
!
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
login
!
!
!
End

