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	Site Specific Activity and Control Measures        
                                     (This section must be completed)

	Method
	

	
	Location
	Carpark and access road

	
	Duration
	Various stages during contract duration

	
	Control
	Assessment included in RA/MP’s briefing

	Exposure Limits


	Asphalt, petroleum fumes 5mg/m3 8hr TWA
Hydrogen sulphide 10ppm 8hr TWA


	Physical Properties
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	Bitumen is a hydrocarbon derived from the distillation of petroleum crude oil.

Black solid at ambient temperature supplied in cardboard or metal kegs, which gradually softens, becomes liquid when heated. 

	Hazard
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	Burns from contact with hot bitumen
Bitumen presents no acute health hazards to the skin other than burning when handled at elevated temperatures

	
	
	Inhalation of vapour in confined spaces may cause irritation to respiratory tract, eyes can lead to headaches and dizziness.

	Work Procedures/PPE
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	Heavy duty, heat resistant gloves (BS EN 374, 388 & 511), footwear and overalls.
Wear full face visor to protect against splashes.
Ensure adequate ventilation during heating / application.
Avoid water contact when heating in suitable bitumen boiler – causes splatter / rapid ejection of hot bitumen. 
Restrict public access during application and until set

	First Aid/Fire
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	Skin Contact:	Flush with cold water, DO NOT ATTEMPT TO REMOVE BITUMEN, cover with sterile dressing, seek immediate medical attention
Inhalation: 	Remove to fresh air and rest, seek medical attention
Ingestion: 	Ensure airways are not obstructed, treat as for Skin.
Eye Contact: 	See and treat as for Skin. 
Fire: 	Use dry powder/foam/CO2 – Do not use water.

	Storage/Disposal
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	Hot bitumen – store in suitable tank / container at correct storage temperature. Keep water away from hot bitumen. Do not overheat. Avoid sources of ignition.
Kegged bitumen – keep dry, 

Disposal: in accordance with legislative and company requirements

	Environmental
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	Spillage: bund using sand or earth to prevent from entering mains drain, sewers, watercourses etc.  Shut off source of spillage and allow to cool. Shovel into suitably marked containers for disposal.
Inform authorities if bitumen enters mains drain, sewers, watercourses.
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