Part 1

1. Take off tyre using tyre leavers
2. Identify area of puncture
3. Assess probability of fixing
4. Clean area and rough surface using both sandpapers provided
5. Evenly apply glue to area
6. Wait one minute
7. Peel packaging of repair patch
8. Press patch and retain pressure onto area
9. Wait for several minutes until glue dries
10. Replace tyre
11. Pump tyre up to see if tyre retains pressure


Part 2
1. Tyre levers too brittle and snap 
2. Tyre leaves bend and do not remove tyre
3. Tyre leavers damage rim
4. Sandpaper not adequate size
5. Sandpaper not adequate grit size
6. Glue not spreading properly
7. Glue not solidifying enough
8. Patch tearing
9. Patch not bonding to glue
10. Patch not allowing tyre to retain pressure
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