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“Rhyd-y-car Terrace”. Are a small row of terrace houses which were built by Richard Crawshay around 1795 to provide housing for the workers in his iron-ore mine, which is now situated in St Fagans National Museum of History. Each dwelling contains a small living room with one bedroom above, accessed by a steep narrow circular staircase next to the fireplace. A second bedroom and small pantry are located at the rear of the houses. The six houses are purposely intended to display different time periods of their history, namely 1805, 1855, 1895, 1925, 1955 and 1985. In this way the changes in the buildings, their contents and their gardens can be shown.


House 1 1805
The windows of house 1 are made from wood with 20 small single paned glass with wooden cross sections, the glass is held in with putty, and the wooden frame is painted, and has a stone cill and brick lintel above the window. The upstairs window is smaller with only 16 panes, one of the panes is a bullseye glass pane which was usually cheaper than a flat piece of glass. The external door is made of wood with a wooden frame with a latch, this seems to be the same with the internal door.
The external wall is constructed from stone, it has a stone cill and external brick lintel. The external is painted with what looks to be lime whitewash, and the internal walls are plastered and painted in white. This is incorporated with an open fire
The roof on property one is covered with rectangle stone, the chimney is constructed of brick and has a stone cowl.
The eves are constructed flush to the property with minimal overhang to the front but has a larger overhang to the rear of the property, the rainwater collection e.g. Guttering is made from cast iron and has a cast iron downpipe.
The internal floor covering is made from stone flags with no carpet coverings, and the external front path is made from cobbled stones.
The internal joinery shows the upstairs joists with solid wooden floorboards, flush door frame with no architrave, wooden shelf above the fireplace and has a round narrow steep staircase that leads to the first floor. There is also deep wooden internal window cill.  

House 2 1855  
Like house 1, the windows are made from wood with 20 small single paned glass with wooden cross sections, the glass is held in with putty, and the wooden frame is painted, it has a stone cill and brick lintel above the window. The upstairs window is smaller with only 16 panes. Same as house 1 there are minimal changes with the external door that is made of wood with a wooden frame with a latch and lock, this seems to be the same with the internal door, in this house there is a door at the bottom of the stairs 
The external wall is constructed of stone, it has a stone cill and external brick lintel. The external looks to have been painted with lime whitewash at some point but has never been re-applied, and the internal walls are plastered and painted in white. This is incorporated with an open fire which has a small oven to the side.
The roof on property two is the same as property one and is covered with rectangle stone, the chimney is constructed of brick and has a stone cowl.
Again, as house 1 the eves are constructed flush to the property with minimal overhang to the front but have a larger overhang to the rear of the property, the guttering is made from cast iron.
The internal floor covering is made from stone flags with a small rug in front of the fire, the external front path is made from cobbled stones.
Same as house 1 the internal joinery shows the upstairs joists with solid wooden floorboards, flush door frame with no architrave, wooden shelf above the fireplace and has a round narrow steep staircase that leads to the first floor. There is also deep wooden internal window cill.  

House 3 1895
The windows on house 3 are different to the first two, the windows on this house are known as sash windows which can open to increase ventilation, they are built with internal weights and are recessed into the building. These windows have larger panes of glass and again have stone cill and brick arched lintel. Same as the first two houses there are minimal changes, the external door is made of wood with a wooden frame with a latch and lock, this seems to be the same with the internal door, and the same as house 2 there is a door to bottom of the stairs. 
The external walls are built using stone and this time the walls have not been painted. Again, the internal walls are plastered and painted white, and a fireplace with an oven to the side of it.
The roof on the property is covered with rectangle stone, the chimney is shared with house 2 and is constructed of brick and has a stone cowl.
Again, the eves are constructed flush to the property with minimal overhang on the front, to the rear there is larger overhang of eves, the guttering is the same as the first two houses which is made from cast iron. 
The internal floors are again the same as the first two houses, made from stone flags but with a slightly higher step into the property. The front path this time has brick laid path and a stone flag at the threshold.
The internal joinery consists of a large timber fireplace surround, upstairs joists with solid wooden floorboards and consists of a narrow staircase and large wooden window cill’s to the inside.

House 4 1925
On this property the windows are known as sash windows which have 9 panes of glass, it also has stone cill’s and an arched brick lintel. The external door is made from wood and with this property the door frame has a bottom threshold and a seal to it, also it has a doorknob rather than a latch.
The external wall is constructed from stone and has more of a natural bare stone construction, the internal décor on this property has wallpaper on the internal wall with pictures hung on the wall.
The roof on the property is covered with rectangle stone, again the chimney is constructed from bricks and with a slate cowl.
The eves are constructed flush to the property with minimal overhang, and the guttering is made from cast iron. 
The floor covering in this property is slightly more raised than the other 3 properties and is constructed of stone slabs, but on one side of the property it looks like it has some kind of Lino material. The external floor is laid with stone slabs.
The internal joinery includes Wooden joists to the first floor and solid wooden floorboards, it has a narrow wooden staircase a wooden fireplace and has skirting boards.

House 5 1955
The windows on this property are more recessed in to the walls and are constructed of wood and are known as sash windows, but this time they only have 2 panes of glass one small pane at the top of the window and one larger pane at the bottom, this time the windows external cill is made of concrete and protrudes out from the property, the lintel above the window is now covered and not on show. The door of this property is constructed of wood but different to the other 4 is that it has a window to increase the lighting into the property, on the door there is also a brass letter box and a door knocker. 
The external walls on this property have been plastered with a rough finish and is painted with what looks like masonry paint, also around the windows and doors have been plastered with some decorative detail. There are also some electrical wires running along the external wall of the property. The internal décor consists of wallpaper in the main room, and the back room is painted two-toned with a tiled section around the sink, the celling is covered in what looks to be Artex and is painted in white paint. The internal joinery is painted in white gloss paint, and there are also some electrical switches in the property. 
The roof on the property is covered with slate possibly Welsh slate. The chimney is shared with house 4 and is constructed of brick and has no cowl but a terracotta chimney pot.
Again, the eves are constructed flush to the property with minimal overhang on the front, to the rear there is larger overhang of eves, the guttering is the same as the other houses which are made from cast iron and includes a cast iron downpipe, but this time it is painted in green paint.
The floor covering in this property is covered with wooden parquet style wooden floor with a large rug to the center of the room, in the front room the floor is covered in red Lino and in the room to the side the floor is covered in a patterned carpet. 
The internal joinery includes Wooden joists and solid wooden floorboards which this time are not as visible due to have been covered with Artex, it has a narrow wooden staircase which this time is missing a door, a wooden fireplace painted in gloss white and has some skirting boards around the main room. 

House 6 1985
The windows on this property are made from steel and painted with white gloss and have a hinge which allows the window to open outwards to allow ventilation, and a latch to close it tight. The Cill’s are also flush with the external walls, The external door on this property is recessed into the property which gives some shelter when unlocking the door. The door is made from wood and as house 5 the door has half round glass to allow natural light into the property. 
The external wall on the final property is covered in a possible sand cement plaster mix and is painted in pink masonry paint, it has also electric cables running along the wall, and on the corner there is a light fitted to the wall. As this is an end of terrace house the pine end is rough plastered and painted with masonry paint. The internal wall coverings are covered in decorative wallpaper, at the rear of the property in the kitchen the walls are smoothly plastered and painted blue, also there are some tiled sections in front of the sink and at the cooking and prepping area. 
With this property the roof covering is made of tile. The chimney is constructed of bricks and has two chimney pots but no cowls.
The eves on this property are the same as all the other properties but one thing that does stand out is that it has what looks to be either an asbestos sheet or a concrete fiber sheet at the end of the roof as a weather board (pine end side). The guttering on this property is made from gray plastic.
The floor in this property is covered in carpet at the front and the stairs with a section by the door which looks rougher than the rest so you can wipe your feet on entry, also on the threshold of the property there are some concrete polished tiles, in the kitchen the floor is covered with decorative Lino material.  
The internal joinery on this property has skirting boards at the bottom of the walls and some architrave around the doors, it has a wooden fireplace top and a wooden surround around the fire hearth, there are wooden upstairs floor joists on show, but the floorboards are covered with Artex. 
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