R1
Current configuration : 3584 bytes
!
! Last configuration change at 18:32:07 UTC Sun Apr 7 2013
!
version 16.9
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
platform qfp utilization monitor load 80
no platform punt-keepalive disable-kernel-core
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
enable password 7 094F471A1A0A
!
no aaa new-model
!
no ip domain lookup
ip admission watch-list expiry-time 0
!
!
!
!
!
!
!
!
!
!
subscriber templating
multilink bundle-name authenticated
!
!
!
crypto pki trustpoint TP-self-signed-1783363698
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-1783363698
 revocation-check none
 rsakeypair TP-self-signed-1783363698
!
!
crypto pki certificate chain TP-self-signed-1783363698
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 31373833 33363336 3938301E 170D3133 30343037 31373436
  30395A17 0D333030 31303130 30303030 305A3031 312F302D 06035504 03132649
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D31 37383333
  36333639 38308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
  0A028201 0100AE05 DFB2B6E3 4671F904 BCF54793 DB2A5024 62F67F4F 0CFC1CAE
  77166387 BCE5455A EC19D160 D857AA9B 1C24FEA9 9E757592 41019E4C 91AC943B
  E3A11DD8 70561C56 07AFD6B9 EB2F0BAF 98F53982 423821E7 0E012C85 91ABF614
  0D18ADAA 1551E247 909D93B4 8665EA61 B091DE83 8BC335F1 C18E73BE 338B12C5
  FE796EB1 FA9C60B6 9EAF0125 8A590EA6 C2008C03 4CDEFD7F 3D1F0B80 9068426D
  B7410565 2E378DEF 994AD135 DDA7D3C1 D5774F7E 68D77484 1F93D878 6805CD1C
  4BBC7ECA B87E3550 0DDB5083 3D17635C 55F73522 F098B941 D79048F4 4E9F1D2E
  6C3A87A0 DA8E25DF E00080B0 6A378C85 8457EBCB B5A074FE 5C5DF486 6A3FA102
  012F9D37 33010203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
  301F0603 551D2304 18301680 1431E11B 78CE290C 6EB334FD 1D2D9466 54995288
  E9301D06 03551D0E 04160414 31E11B78 CE290C6E B334FD1D 2D946654 995288E9
  300D0609 2A864886 F70D0101 05050003 82010100 93105B4D 031A1986 7E804F90
  267A47CC 3EF799A1 D6553915 B5EDB7ED 6AF6F964 EB88815F F8FCB231 CF539DCC
  8DFE05EF 0370191C 1534995E F9954190 3871345C 40DFC1C2 4D37D77E BD6306E9
  E7CAE40E 2ED7C007 47045EF8 2B709821 517C1221 0F80EB28 6BE49D0F FC922491
  653A3C89 9F230939 D640BF4B 0840ABE1 8F346316 B3EF7798 DB88C724 D04B3CCF
  7C82C96D C3B85B2E F70E4A30 6F020620 334E5F90 59FC2B80 246A3B2B B0B699F1
  909CA4A9 1B997622 274B791E 546BA45D 32382A32 27381482 75283549 AE6D935F
  D0B54931 1126C075 21D8B95C 9B09705C F2272E7C B056CA7C D93A08F8 CF41CAFE
  F7845B22 057BCECB 36042F2E F244D1DF 2D1DE457
        quit
!
license udi pid ISR4221/K9 sn FGL2235928E
no license smart enable
diagnostic bootup level minimal
!
spanning-tree extend system-id
!
!
!
!
redundancy
 mode none
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0/0
 description PC-B to R1 d.gateway for PC-B
 ip address 172.16.10.1 255.255.255.0
 negotiation auto
!
interface GigabitEthernet0/0/1
 description R1 to S1 d.gateway for PC-A
 ip address 172.16.11.1 255.255.255.0
 negotiation auto
!
interface Serial0/1/0
 no ip address
 shutdown
!
interface Serial0/1/1
 no ip address
 shutdown
!
ip forward-protocol nd
ip http server
ip http authentication local
ip http secure-server
!
!
!
!
!
!
control-plane
!
banner motd ^Cunauthorized access is prohibited^C
!
line con 0
 password 7 060503205F5D
 login
 transport input none
 stopbits 1
line vty 0
 password 7 060506324F41
 login
line vty 1 4
 login
!
!
!
!
!
!
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R1#show ip int brief

Interface              IP-Address      OK? Method Status                Protocol
GigabitEthernet0/0/0   172.16.10.1     YES manual up                    up
GigabitEthernet0/0/1   172.16.11.1     YES manual up                    up
Serial0/1/0            unassigned      YES unset  administratively down down
Serial0/1/1            unassigned      YES unset  administratively down down

R1#


S1
Current configuration : 1476 bytes
!
! Last configuration change at 03:51:12 UTC Mon Mar 1 1993
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
system mtu routing 1500
!
!
!
!
!
!
!
no ip domain-lookup
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface FastEthernet0/1
!
interface FastEthernet0/2
!
interface FastEthernet0/3
!
interface FastEthernet0/4
!
interface FastEthernet0/5
!
interface FastEthernet0/6
!
interface FastEthernet0/7
!
interface FastEthernet0/8
!
interface FastEthernet0/9
!
interface FastEthernet0/10
!
interface FastEthernet0/11
!
interface FastEthernet0/12
!
interface FastEthernet0/13
!
interface FastEthernet0/14
!
interface FastEthernet0/15
!
interface FastEthernet0/16
!
interface FastEthernet0/17
!
interface FastEthernet0/18
!
interface FastEthernet0/19
!
interface FastEthernet0/20
!
interface FastEthernet0/21
!
interface FastEthernet0/22
!
interface FastEthernet0/23
!
interface FastEthernet0/24
!
interface GigabitEthernet0/1
!
interface GigabitEthernet0/2
!
interface Vlan1
 ip address 172.16.11.10 255.255.255.0
!
ip default-gateway 172.16.11.1
ip http server
ip http secure-server
!
no vstack
banner motd ^C unauthorized access is prohibited ^C
!
line con 0
line vty 0
 password telnet
 login
line vty 1 4
 login
line vty 5 15
 login
!
end

S1#

S1# show ip int brief
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  172.16.11.10    YES manual up                    up
FastEthernet0/1        unassigned      YES unset  down                  down
FastEthernet0/2        unassigned      YES unset  down                  down
FastEthernet0/3        unassigned      YES unset  down                  down
FastEthernet0/4        unassigned      YES unset  down                  down
FastEthernet0/5        unassigned      YES unset  up                    up
FastEthernet0/6        unassigned      YES unset  up                    up
FastEthernet0/7        unassigned      YES unset  down                  down
FastEthernet0/8        unassigned      YES unset  down                  down
FastEthernet0/9        unassigned      YES unset  down                  down
FastEthernet0/10       unassigned      YES unset  down                  down
FastEthernet0/11       unassigned      YES unset  down                  down
FastEthernet0/12       unassigned      YES unset  down                  down
FastEthernet0/13       unassigned      YES unset  down                  down
FastEthernet0/14       unassigned      YES unset  down                  down
FastEthernet0/15       unassigned      YES unset  down                  down
FastEthernet0/16       unassigned      YES unset  down                  down
FastEthernet0/17       unassigned      YES unset  down                  down
FastEthernet0/18       unassigned      YES unset  down                  down
FastEthernet0/19       unassigned      YES unset  down                  down
FastEthernet0/20       unassigned      YES unset  down                  down
FastEthernet0/21       unassigned      YES unset  down                  down
FastEthernet0/22       unassigned      YES unset  down                  down
FastEthernet0/23       unassigned      YES unset  down                  down
FastEthernet0/24       unassigned      YES unset  down                  down
GigabitEthernet0/1     unassigned      YES unset  down                  down
GigabitEthernet0/2     unassigned      YES unset  down                  down
S1#
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>ipconfig /all
Windows IP Configuration

Host Name .
Primary Dns Suffix’
Node Type . . .

Ip Routing Enabled.
WINS Proxy Enabled.

Ethernet adapter Ethernet:

Connection-specific DNS Suffix
Description .

Physical Address.

DHCP Enabled.
Autoconfiguration Enabled .
Link-local IPv6 Address .
1Pv4 Address.

Subnet Mask .

Default Gateway .

DHCPV6 TAID .

DHCPV6 Client DUID.

DNS Servers .

NetBIOS over Tcpip.

: feco

Intel(R) Ethernet Connection (2) 1219-1M
C-9D-92-BF-B9-33

No

Yes

e80: :d160:77F6: cfe9:808%2 (Preferred)
172.16.11.254(Preferred)

255.255.255.6

172.16.11.1

34381262
00-61-60-61-23-4E-79-A7-6C-9D-92-BF -89-33
FEFFL %1

feco
feco

: Enabled
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C:\>ping 172.16.10.254

pinging 172.16.
Reply from 172.
Reply from 172.
Reply from 172.
Reply from 172.

10.254 with 32 bytes of data:
16.10.254: bytes=32 time<ims
16.10.254: bytes=32 time<ims
16.10.254: bytes=32 time<ims
16.10.254: bytes=32 time<ims

ping statistics for 172.16.16.254:
Packets: Sent - 4, Received = 4, Lost = © (8% loss),
pproximate round trip times in milli-seconds:
Minimum = ems, Maximum - ems, Average = 6ms

c:\>




image3.JPG
818 show ip int brief
Interface
Ulani
FastEthernet8/1
FastEthernetd, 2
FastEChornota,3
FastEthernetd, 4
FastEChornot,/s
FastEthernetd &
FastEChornota, 7
FastEthernetd, 8
FastEChornota 9
FastEthernetd, 10
FastEChornota 11
FastEthernetd, 12
FastEChornota 13
FastEthernetd, 14
FastEChornota 15
FastEthernetd, 16
FastEChornota 17
FastEthernetd, 18
FastEChornota 19
FastEthernetd, 20
FastEChornot, 21
FastEthernetd, 22
FastEChornota,/23
FastEChornot, 24
faabicEchernetd 1

IP-fddress

172.16.11.18

ned
ned
ned
ned
ned
ned
ned
ned
ned
ned
ned
ned
ned
ned
ned
ned
ned
ned
ned
ned
ned
ned
ned
ned
ned

unassigned

oK?
YES
YES
YES
YES
YES
YES
YES
YES
YES
YES
YES
YES
YES
YES
YES
YES
YES
YES
YES
YES
YES
YES
YES
YES
YES
YES
YES

Method Status

manual up

unset
unset
unset
unset
unset
unset
unset
unset
unset
unset
unset
unset
unset
unset
unset
unset
unset
unset
unset
unset
unset
unset
unset
unset
unset
unset

doun
doun
doun
doun
up

up

doun
doun
doun
doun
doun
doun
doun
doun
doun
doun
doun
doun
doun
doun
doun
doun
doun
doun
doun
doun

Protocol
up
doun
doun
doun
doun
up
up
doun
doun
doun
doun
doun
doun
doun
doun
doun
doun
doun
doun
doun
doun
doun
doun
doun
doun
doun
doun
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>ipconfig /all

iindows I Configuration

Host Name . LN272-NETLAB
Primary Dns Suffix’

Node Type . . . Hybrid

Ip Routing Enabled. No

WINS Proxy Enabled. : No

thernet adapter Ethernet:

Connection-specific DNS Suffix
Description .
Physical Address.

Intel(R) Ethernet Connection (2) I219-LM
: 6C-9D-92-BF-B9-BF

DHCP Enabled. . No
Autoconfiguration Enabled . Yes
Link-local IPvé Address . : fe80::a051:e2eb:2a25: 2ecck7 (Preferred)

1Pv4 Address.
Subnet Mask .
Default Gateway .
DHCPV6 TAID .
DHCPY6 Client DUID.
DNS Servers .

172.16.16.254(Preferred)
255.255.255.6

: 172.16.10.1

34381262

00-61-60-61-23-4F -BE-EA-0C-9D-02-BF -B9-BF
: fec8:0:0:FFFF::1%1

NetBIOS over Tcpip.

>





