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/* Main.c file generated by New Project wizard

* Created:  Tue May 13 2025
* Processor: PICI6FE774

* Compiler: CCs for PIC

o

#include <16F877A.h>
int main (void)

1 {

] (if(outpug igh(pin_c1))
output_b(exFf);

else

{
output_b(ex20) ;

P
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main.c @
/% Main.c file generated by New Project wizard
* Created:  Tue May 13 2025

1

2

s

4 * Processor: PICIGFE774
5 * Compiler: CCS for PIC
B

7

5

B

R4

#include <16F877A.h>
000000)

suse delay(cloc
10
11 unsigned int count[] - {0xco,0x79,0xa4,0xb0,0x99, 0x92, 0x52, 0xTS, OB, 0x30} 5
2

13 int main (void)

148 ¢

15 output_d(oxco);

16 delay_ms(2000);

17 output d(oxts);

15 delay_ms(2000);

13 output d(oxad);

20 delay_ms(2000);

21 output_d(oxbo);

22 delay_ms(2000);

2 output d(0x99);

2 delay_ms(2000);

25 output d(0x92);

26 delay_ms(2000);

27 output_d(0x52);

26 delay_ms(2000);

29 output_d(ox7s);

30 delay_ms(2000);

31 output d(oxso);

32 delay_ms(2000);

33 output d(oxs0);

34 delay_ms(2000);

3}

36




