[bookmark: _Hlk134002394]IP Construction
Take-off
Jack Rees
Centre Lines
Based on a wall thickness of 400mm
External corners – 17no.
Internal corners – 9no.
17 – 9 = 8
Internal Girth
8/ 2/ .400 = 6.40
428.20 (external wall) – 6.40 = 421.80 internal girth
Centre Line
8/ 2/ 0.5/ .400 = 3.20
428.20 – 3.20 = 425.00 Centre Line
Centre line of external girth (external girth thickness – 100mm)
8/ 2/ 0.5/ 0.100 = 0.800
428.2 – 0.80 = 427.40 external girth centre line
Centre line of internal girth (internal girth thickness – 150mm)
8/ 2/ 0.5/ 0.150 = 1.20
421.80 (internal girth) + 1.20 = 423.00 internal girth centre line
