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12. Answer this question in a Word Document with a screenshot of Evidence.
· Is DHCP successful in Ha1 and Ha2? 
NO
· 
Should be successful. If not Troubleshoot!
· From Ha1, ping Ha2. Is it successful? 
[image: ]



· From Ha2, ping Ra1. Is it successful?
[image: Text
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60% completion screenshot
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· Kept saying invalid login, used the correct password form the setup but not sure why it wasn’t working

· Connect 209.165.201.1 from Hc1 using SSH. Is it reachable? [image: ]
· Connect 209.165.201.1 from Hc2 using SSH. Is it reachable? 

· Connect 209.165.201.1 from Ha1 using SSH. Is it reachable? 

· Connect 209.165.201.1 from Ha2 using SSH. Is it reachable? 



· 
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fcommana prompt

Packet Tracer PC Command Line 1.0
C:\>ping 165 254 12¢.132

Pinging 165.254.126.132 with 32 byres of data:

Reply from 165.254.12¢.132 cime<lms
Reply from 165 254 126132 “ime<lms
Reply from 165 254 126132 “ime<lms
Reply from 165254126 132: byces=32 cime<lms TTL=128

Ping stavistics for 165.254.12¢.132
Packets: Sent = 3, Received = 4, Lost = 0 (0% loss),
Bpprosimate round trip vimes in milli-seconds

Minimm = 0ms, Maximm = 0ms, Average = Oms

e
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fcommana prompt

Packet Tracer BC Command Line 1.0
C:\>ping 152.1€5.10.1

Pinging 152.168.10.1 with 32 bytes of data:
Request cimed out.
Request cimed out.
Request cimed out.

Request cimed out.

Ping scavistics for 152.168.10.1
Packets: Sent = 4, Received = 0, Lost = 4 (100%

e
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Configure Company C (Rc1, Sc1 and Rc2, Sc2)

13. On Router Rl and Re2, configure IP Address and activate all the interfaces (including loopback).

14. Configure Management Interface (SVI) for Vian 1 with IP Address and Default Gateways on switches Sc1 and Sc2 as per the Vlan Table details. Shut down all unused ports.

15. On Router Rc1 and Rc2, configure OSPF routing protocol based on the following information.

process id 15, Area 0

Router Id for Rc1 with 1.1.1.1 and Rc2 with 5.5.5.5

Configure the network statement for each locally attached networks using a wild card mask matching the network’s subnet mask.
Configure appropriate interfaces as passive.

Configure the reference bandwidth to 1Gigabit.

16. Configure DHCP relay (IP - Helper address) at the appropriate Interface enabling Hc2 for DHCP Configuration.

17. Configure Hel

approj

e 1P address, subnet mask and default gateway as per the addressing table.

18. Test your configuration (Before ACL) Answer this question in a Word Document with a screenshot of Evidence.

All the PC's must Ping Successfully:

If not Troubleshoot!
Connect 209.165.201.1 from Hcl using SSH. Is it reachable?

Should be reachable. If not Troubleshoot!
Connect 209.165.201.1 from Hc2 using SSH. Is it reachable?

Should be reachable. If not Troubleshoot!
Connect 209.165.201.1 from Hal using SSH. Is it reachable?

Should be reachable. If not Troubleshoot!
Connect 209.165.201.1 from Ha2 using SSH. Is it reachable?

Should be reachable. If not Troubleshoot!

Restrictions and Modifications: Access Control Lists and NAT

19. Create an access control list

Time Elapsed: 01

(] Top.

Check Results| | Reset Activity

Completion: 60%

73
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fcommana prompt

[E—
* Login invalia

Erem—

(Connection to 205.1€5.201.1 closed by foreign hostl
Ci\>ssh -1 sdminl 205.165.201.1

Erm—
* Login invalia

Erm—
* Login invalia

Erm—
§ Passvord: vimeout expired!
* Login invalid

(Connection to 205.1€5.201.1 closed by foreign hostl
Ci\>ssh -1 sdmin 205.165.201.1

Erm—
§ Passvord: vimeout expired!
* Login invalid

(Connection to 205.1€5.201.1 closed by foreign hostl
Ci\>ssh -1 sdminl 205.165.201.1





