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:\Users\Admin>netstat
Active Connections

Proto Local Address Foreign Address state

:\Users\Admin>ping 141.246.11.254

Pinging 141.246.11.254 with 32 bytes of data:
Reply from 153.99.16.254: Destination host unreachable.
Reply from 153.99.10.254: Destination host unreachable.
Reply from 153.99.16.254: Destination host unreachable.
Reply from 153.99.10.254: Destination host unreachable.

Ping statistics for 141.246.11.254:
Packets: Sent = 4, Received = 4, Lost = © (8% loss),

Users\Admin>
Users\Admin>
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Command Prompt
+\Users\Admin>netstat

\ctive Connections

Proto Local Address Foreign Address state

:\Users\Admin>ping 141.240.11.254

binging 141.248.11.254 with 32 bytes of data:
Reply from 153.99.16.254: Destination host unreachable.
Reply from 153.99.16.254: Destination host unreachable.
Reply from 153.99.16.254: Destination host unreachable.
Reply from 153.99.16.254: Destination host unreachable.

ping statistics for 141.246.11.25
Packets: Sent = 4, Received = 4, Lost = © (8% loss),

\Users\Admin>
:\Users\Admin>ping 141.246.16.254

binging 141.240.10.254 with 32 bytes of data:
Reply from 153.99.16.254: Destination host unreachable.
Reply from 153.99.16.254: Destination host unreachable.
Reply from 153.99.16.254: Destination host unreachable.
Reply from 153.99.16.254: Destination host unreachable.

ping statistics for 141.246.16.25
Packets: Sent = 4, Received = 4, Lost = © (8% loss),
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