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PC to Server
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PC to Laptop
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Laptop to Server
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Laptop to Printer
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Laptop to PC
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Logical Topology
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Logical Topology 
	Device
	Interface
	IP Address
	Subnet Mask
	Default Gateway

	PC0
	NIC
	192.168.1.10
	255.255.255.0
	192.168.1.1

	Router0
	Gig0/0/1
Gig0/0/0
Se0/1/0
	192.168.1.1
192.168.2.1
11.0.01
	255.255.255.0
255.255.255.0
255.255.255.252
	N/A
N/A
N/A

	Printer0
	NIC
	192.168.2.5
	255.255.255.0
	192.168.2.1

	Server0
	NIC
	192.168.2.2
	255.255.255.0
	192.168.2.1

	Wireless Router0
	VLAN
	192.168.2.1
	255.255.255.0
	N/A

	Laptop
	NIC
	192.168.2.100
	255.255.255.0
	192.168.2.1
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Config _Desktop _ Programming _ Attribute

fcommana Prompt

Pinging 152.168.2.5 with 32 bytes of data:

Reply from 152168
Reply from 152168
Reply from 152168
Reply from 152168 bytes=32 vime=Tms TTL=123

Ping stavistics for 152.168.2.5
Packets: Sent = 3, Received = 4, Lost = 0 (0% loss),
Bpprosimate round trip vimes in milli-seconds

Minimum = 7ms, Maximm = 3lms, Average = 17ms
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C:\>ping 152.165.1.10

Pinging 152.168.1.10 with 32 byres of data:

Reply from 152.168.1.10
Reply from 152.1€5.1.10
Reply from 152.1€5.1.10
Reply from 152.1€5.1.10

Ping scavistics for 152.168.1.10
Packets: Sent = 3, Received = 4, Lost = 0 (0% loss),
Bpproximate round trip times in milli-seconds
Minimm = 1lms, Maximm = léms, Average = lims
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Programming  Attribute

C:\>ping 152.165.2.5

Pinging 152.168.2.5 with 32 byres of data:

Reply from 152168 “ime<lms TTL=127
Reply from 152168 “ime<lms TTL=127
Reply from 152168 “ime<lms TTL=127
Reply from 152168 “ime<lms TTL=127

Ping stavistics for 152.168.2.5
Packets: Sent = 3, Received = 4, Lost = 0 (0% loss),
Bpprosimate round trip vimes in milli-seconds
Minimm = 0ms, Maximm = 0ms, Average = Oms
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0p_ Programming

fcommana Prompt

C:\>ping 152.165.2.2
Pinging 152.168.2.2 with 32 byres of data:

Reply from 152168 bytes=32 cime<lms
Reply from 152168 bytes=32 cime<lms
Reply from 152168 bytes=32 cime<lms
Reply from 152168 bytes=32 vime<lms TTL-127

Ping stavistics for 152.168.2.2

Packets: Sent = 3, . Tost = 0 (0% loss),
Bpprosimate round trip vimes in milli-seconds

Minimm = 0ms, Maximm = 0ms, Average = Oms

Received = 4
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Config _Desktop _ Programming _ Attribute

fcommana Prompt

C:\>ping 152.165.2.100
Pinging 152.168.2.100 with 32 byres of data.

Reply from 152.168.2.100: byres=32
Reply from 152.1¢8.2.100: byres=32
Reply from 152.1¢8.2.100: byres=32
Reply from 152.1¢8.2.100: byres=32

Ping stavistics for 152.1€8.2.100

Packets: Sent = 3, . 0 (0% 1oss),
Bpprosimate round trip vimes in milli-seconds

Minimum = Sms, Maximm = léms, Average = llms

Received = 4
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0p  Programming  Attributes

fcommana Prompt

Packet Tracer BC Command Line 1.0
C:\>ping 152.165.2.2

Pinging 152.168.2.2 with 32 byres of data:

Reply from 152168 bytes=32 vime=3ems TTL=123
Reply from 152168 bytes=32 vime=lims TTL=123
Reply from 152168 byces=32 Tri-128
Reply from 152168 byves=32 Tri-128

Ping stavistics for 152.168.2.2

Packets: Sent = 3, . Tost = 0 (0% loss),
Bpproximate round trip times in milli-seconds

Minimm = l4ms, Maximm = 3éms, Average = 2lms

Received = 4





