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R1#show run
Building configuration...


Current configuration : 3652 bytes
!
! Last configuration change at 15:18:55 UTC Tue Jan 14 2020
!
version 16.9
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
platform qfp utilization monitor load 80
no platform punt-keepalive disable-kernel-core
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$1M20$XSN/GOX/j401gz0wEWOKv.
!
no aaa new-model
!
no ip domain lookup
ip admission watch-list expiry-time 0
!
!
!
!
!
!
!
!
!
!
subscriber templating
multilink bundle-name authenticated
!
!
!
crypto pki trustpoint TP-self-signed-1227001095
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-1227001095
 revocation-check none
 rsakeypair TP-self-signed-1227001095
!
!
crypto pki certificate chain TP-self-signed-1227001095
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 31323237 30303130 3935301E 170D3230 30313134 31343235
  35375A17 0D333030 31303130 30303030 305A3031 312F302D 06035504 03132649
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D31 32323730
  30313039 35308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
  0A028201 0100AA33 FB331090 0753C465 2E2465B9 8C940ACD 7428701D F754E69A
  1AEDB9DB C3BFA669 17AB484C 6268517A 9A1533F2 D0FB144D B111B895 8470218B
  D30F0D68 E7587F10 70B339CA 0DAA81BF EBD9EE8D 56094593 8A667B01 F431A736
  BE5BAF14 38E7F4E7 82B8ED92 46FA8EA5 CCB557D1 3A9777DC 865D231B DFB7E55D
  EE66E8C4 751B5BF5 7135B402 7B3ADCBF 7CEC9F3F 1C540C61 D0952599 7E28FA02
  4610E77E 4EC09F21 7009C356 D4F5A6A2 B2DCBE53 A348A2FB 80E2ECF1 895AE7D6
  4F1A98EA 558AA42F D53AB2D4 8FDFC47B 96EB5016 94785156 07CC9FC3 A387DE30
  94ED6B7F 85BE4D92 DE6FD885 474B03BB 4611DEA3 E5460E98 013479E0 C55F72AD
  CA6EFFFD C5E30203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
  301F0603 551D2304 18301680 142751CC B6734B7F 4AA6BB9B C4EA3B67 8B67A77D
  A4301D06 03551D0E 04160414 2751CCB6 734B7F4A A6BB9BC4 EA3B678B 67A77DA4
  300D0609 2A864886 F70D0101 05050003 82010100 7F22052B 918A8E4A 528EC1FB
  199AD1A8 09ABA833 45A5B8E2 645C21D3 43524BDC C0EB1C92 96344CDB FB992634
  4D059709 2C6C421B BAD2CD7C F5F2E101 0A2E8957 D852AE1B 534DFC33 190C17B9
  1D4A0153 360A867B D3782DDF 9356F932 8CEB44CA 218AC696 70184CD8 8FEFB099
  EDCB2537 6B167698 51D1A2C0 23C4A536 1614749D EDDEF3F8 ED2ED0C0 759FE8BB
  C596D2FA DD89BC3C A74983D5 DB23BE25 7CCB4404 B313C692 C6F72842 2515ADD5
  35A389B4 3188168A 8FF429A9 45BBAFF4 EDC659A1 4FFA5D80 0A392329 9374CDB5
  B848C31E 3750FCC5 1EA7FEF7 47D94A30 247E503C 50D488A0 3BA1C3D5 F3CA34E9
  98174F54 CD853657 5DF05AA9 4663F31C 4E0791AA
        quit
!
license udi pid ISR4221/K9 sn FGL224190DV
no license smart enable
diagnostic bootup level minimal
!
spanning-tree extend system-id
!
!
!
!
redundancy
 mode none
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0/0
 ip address 141.240.10.1 255.255.255.0
 negotiation auto
!
interface GigabitEthernet0/0/1
 ip address 141.240.11.1 255.255.255.0
 negotiation auto
!
interface Serial0/1/0
 no ip address
 shutdown
!
interface Serial0/1/1
 no ip address
 shutdown
!
ip forward-protocol nd
ip http server
ip http authentication local
ip http secure-server
!
!
!
!
!
!
control-plane
!
banner motd ^Cwarning unauthorised acces prohibiterd^C
!
line con 0
 exec-timeout 5 0
 password 7 060503205F5D
 login
 transport input none
 stopbits 1
line vty 0 4
 exec-timeout 5 0
 password 7 05080F1C22430E
 logging synchronous
 login
line vty 5 15
 exec-timeout 5 0
 password 7 05080F1C22430E
 logging synchronous
 login
!
!
!
!
!
!
end
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Rlfchou 1o
lon 14 15:16:55.003: 1845-5-CONFIG L Configured fron console by console

Uirtual Service Elobal State and Virtualizat lon Linits:

Infrastructure version : 1.7
Total virtual services installed : 0
Total virtual services activated ¢ 1

Hachire tupes supported < KUK, LIC
Hachire tpes disabled  : nons

Hasirun CPUS por virtua] service : 2
Rasaurce virtualizaton Linits:

Hare Uots  Comitted  Ruailable
Systen 03U (1) 3 0 3
rerory (16) 1024 0 1024
bootlash (1) 1000 0 1000

10+ Infrastructure Survary;

0 service (CAF)
10 service ()

10 service (Iiran)
Libvivtd + Runing

Rifhos ip route
Codes: L - local, € - comected, § - static, & - RIP, H - robile, & - BiP
1§ - EIGRP) 4 - EIGR exiomal, 0 - O, 4 © OSPF inter area
1 - O5PF HSA extemnal tupe 1, 2 - OSPF HSSR external tupe 2
EA - O5PF extemal tupe 1, €2~ OSPF extemal tupe 2
§- 188, su - 1516 sumary, L1 - 515 lowel-d, 12 - 18-15 lovel-2
Is - 1818 inter ares, * - cardidate default, U - par-user static route
o 0, P - periodic donloadad static routs, H - MRF, 1 - LIS
a - application route
* - replicated route, 1 - next hop override, p - overrides fron PR

Gateuay of last resort s ot se

Rifishou ip interface bris

Interface Tr-fddress  OK? Hthod Status Protocal
GlgsbitEtherret0/0/)  141.240.10.1  VES ranual doun doun
GlgsbitEthoret0/0/1  141240.1171  YES ranual down doun
Sariall/1/0 nassiored VES unset advinistrat ively doun down
ool wassigned  VES unset advinistrat vely doun down
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-r count Record route for count hops (IPvd-only). ~
count. Timestamp for count hops (IPv4-only).
host-list  Loose source route along host-list (IPvd-only).
host-list  Strict source route along host-list (IPv-only).
-w timeout  Timeout in milliseconds to wait for each reply.
R Use routing header to test reverse route also (IPv6-only).
Per RFC 5605 the use of this routing header has been
deprecated. Some systems may drop echo requests if
this header is used.

-S srcaddr  Source address to use.
-C compartment Routing compartment identifier.

- Ping a Hyper-V Network Virtualization provider address.
-4 Force using IPva.

-6 Force using IPV6.

C:\Users\Admin>ping 141.246.16.254

Pinging 141.246.10.254 with 32 bytes of data:
Reply from 141.240.16.254: bytes-32 time<ims TTL-127
Reply from 141.240.16.254: bytes=32 time<ims TTL-127
Reply from 141.240.16.254: bytes=32 time<ims TTL-127
Reply from 141.246.16.254: bytes-32 time<ims TTL-127

Ping statistics for 141.246.16.254:
Packets: Sent = 4, Received = 4, Lost = © (6% loss),
Approximate round trip times in milli-seconds:
Minimum = @ms, Maximum - ems, Average = 6ms

:\Users\Admin>
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