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R1
R1>en
R1#show run
Building configuration...

Current configuration : 1407 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R1
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX15248S4V-
!
!
!
!
!
!
!
!
!
no ip domain-lookup
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
ip address 185.95.1.1 255.255.255.0
ip ospf priority 200
duplex auto
speed auto
!
interface GigabitEthernet0/1
no ip address
duplex auto
speed auto
shutdown
!
interface GigabitEthernet0/2
no ip address
duplex auto
speed auto
shutdown
!
interface Serial0/0/0
ip address 185.95.12.1 255.255.255.252
ip ospf priority 200
clock rate 2000000
!
interface Serial0/0/1
ip address 185.95.13.1 255.255.255.252
clock rate 2000000
!
interface Serial0/3/0
no ip address
clock rate 2000000
shutdown
!
interface Serial0/3/1
no ip address
clock rate 2000000
shutdown
!
interface Vlan1
no ip address
shutdown
!
router ospf 1
router-id 1.1.1.1
log-adjacency-changes
passive-interface GigabitEthernet0/0
auto-cost reference-bandwidth 1000
network 0.0.0.0 255.255.255.255 area 0
network 185.95.1.0 0.0.0.255 area 0
network 185.95.1.1 0.0.0.0 area 0
network 185.95.12.0 0.0.0.3 area 0
network 195.95.13.0 0.0.0.3 area 0
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CGTFO^C
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
login
!
!
!
end


R1#
R1#sho
R1#show ip int brief
Interface IP-Address OK? Method Status Protocol 
GigabitEthernet0/0 185.95.1.1 YES manual up up 
GigabitEthernet0/1 unassigned YES unset administratively down down 
GigabitEthernet0/2 unassigned YES unset administratively down down 
Serial0/0/0 185.95.12.1 YES manual up up 
Serial0/0/1 185.95.13.1 YES manual up up 
Serial0/3/0 unassigned YES unset administratively down down 
Serial0/3/1 unassigned YES unset administratively down down 
Vlan1 unassigned YES unset administratively down down
R1#show ip route
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
* - candidate default, U - per-user static route, o - ODR
P - periodic downloaded static route

Gateway of last resort is not set

185.95.0.0/16 is variably subnetted, 9 subnets, 3 masks
C 185.95.1.0/24 is directly connected, GigabitEthernet0/0
L 185.95.1.1/32 is directly connected, GigabitEthernet0/0
O 185.95.2.0/24 [110/65] via 185.95.12.2, 00:08:50, Serial0/0/0
O 185.95.3.0/24 [110/65] via 185.95.13.2, 00:08:50, Serial0/0/1
C 185.95.12.0/30 is directly connected, Serial0/0/0
L 185.95.12.1/32 is directly connected, Serial0/0/0
C 185.95.13.0/30 is directly connected, Serial0/0/1
L 185.95.13.1/32 is directly connected, Serial0/0/1
O 185.95.23.0/30 [110/128] via 185.95.12.2, 00:08:50, Serial0/0/0
[110/128] via 185.95.13.2, 00:08:50, Serial0/0/1

R1#show ip ospf ne
R1#show ip ospf neighbor 


Neighbor ID Pri State Dead Time Address Interface
3.3.3.3 0 FULL/ - 00:00:37 185.95.13.2 Serial0/0/1
2.2.2.2 0 FULL/ - 00:00:33 185.95.12.2 Serial0/0/0
R1#show ip ospf da
R1#show ip ospf database 
OSPF Router with ID (1.1.1.1) (Process ID 1)

Router Link States (Area 0)

Link ID ADV Router Age Seq# Checksum Link count
2.2.2.2 2.2.2.2 544 0x80000005 0x005cd3 5
1.1.1.1 1.1.1.1 542 0x80000005 0x00af9a 5
3.3.3.3 3.3.3.3 542 0x80000005 0x00d255 5
R1#

R2>en
R2#show run
Building configuration...

Current configuration : 1185 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R2
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX1524JJ6O-
!
!
!
!
!
!
!
!
!
no ip domain-lookup
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
ip address 185.95.2.1 255.255.255.0
duplex auto
speed auto
!
interface GigabitEthernet0/1
no ip address
duplex auto
speed auto
shutdown
!
interface GigabitEthernet0/2
no ip address
duplex auto
speed auto
shutdown
!
interface Serial0/0/0
ip address 185.95.12.2 255.255.255.252
!
interface Serial0/0/1
ip address 185.95.23.1 255.255.255.252
!
interface Vlan1
no ip address
shutdown
!
router ospf 1
router-id 2.2.2.2
log-adjacency-changes
passive-interface GigabitEthernet0/0
auto-cost reference-bandwidth 1000
network 0.0.0.0 255.255.255.255 area 0
network 185.95.2.0 0.0.0.255 area 0
network 185.95.2.1 0.0.0.0 area 0
network 185.95.12.0 0.0.0.3 area 0
network 185.95.23.0 0.0.0.3 area 0
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CGTFO^C
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
login
!
!
!
end


R2#show ip int brief
Interface IP-Address OK? Method Status Protocol 
GigabitEthernet0/0 185.95.2.1 YES manual up up 
GigabitEthernet0/1 unassigned YES unset administratively down down 
GigabitEthernet0/2 unassigned YES unset administratively down down 
Serial0/0/0 185.95.12.2 YES manual up up 
Serial0/0/1 185.95.23.1 YES manual up up 
Vlan1 unassigned YES unset administratively down down
R2#show ip route
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
* - candidate default, U - per-user static route, o - ODR
P - periodic downloaded static route

Gateway of last resort is not set

185.95.0.0/16 is variably subnetted, 9 subnets, 3 masks
O 185.95.1.0/24 [110/65] via 185.95.12.1, 00:09:42, Serial0/0/0
C 185.95.2.0/24 is directly connected, GigabitEthernet0/0
L 185.95.2.1/32 is directly connected, GigabitEthernet0/0
O 185.95.3.0/24 [110/65] via 185.95.23.2, 00:09:42, Serial0/0/1
C 185.95.12.0/30 is directly connected, Serial0/0/0
L 185.95.12.2/32 is directly connected, Serial0/0/0
O 185.95.13.0/30 [110/128] via 185.95.12.1, 00:09:42, Serial0/0/0
[110/128] via 185.95.23.2, 00:09:42, Serial0/0/1
C 185.95.23.0/30 is directly connected, Serial0/0/1
L 185.95.23.1/32 is directly connected, Serial0/0/1

R2#show ip ospf nei
R2#show ip ospf neighbor 


Neighbor ID Pri State Dead Time Address Interface
3.3.3.3 0 FULL/ - 00:00:37 185.95.23.2 Serial0/0/1
1.1.1.1 200 FULL/ - 00:00:39 185.95.12.1 Serial0/0/0
R2#show ip ospf dat
R2#show ip ospf database 
OSPF Router with ID (2.2.2.2) (Process ID 1)

Router Link States (Area 0)

Link ID ADV Router Age Seq# Checksum Link count
2.2.2.2 2.2.2.2 595 0x80000005 0x005cd3 5
1.1.1.1 1.1.1.1 593 0x80000005 0x00af9a 5
3.3.3.3 3.3.3.3 593 0x80000005 0x00d255 5
R2#

R3>en
R3#show run
Building configuration...

Current configuration : 1205 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R3
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX1524A4ZP-
!
!
!
!
!
!
!
!
!
no ip domain-lookup
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
ip address 185.95.3.1 255.255.255.0
duplex auto
speed auto
!
interface GigabitEthernet0/1
no ip address
duplex auto
speed auto
shutdown
!
interface GigabitEthernet0/2
no ip address
duplex auto
speed auto
shutdown
!
interface Serial0/0/0
ip address 185.95.13.2 255.255.255.252
!
interface Serial0/0/1
ip address 185.95.23.2 255.255.255.252
clock rate 2000000
!
interface Vlan1
no ip address
shutdown
!
router ospf 1
router-id 3.3.3.3
log-adjacency-changes
passive-interface GigabitEthernet0/0
auto-cost reference-bandwidth 1000
network 0.0.0.0 255.255.255.255 area 0
network 185.95.3.0 0.0.0.255 area 0
network 185.95.3.1 0.0.0.0 area 0
network 185.95.13.0 0.0.0.3 area 0
network 185.95.23.0 0.0.0.3 area 0
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CGTFO^C
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
login
!
!
!
end


R3#show ip int brief
Interface IP-Address OK? Method Status Protocol 
GigabitEthernet0/0 185.95.3.1 YES manual up up 
GigabitEthernet0/1 unassigned YES unset administratively down down 
GigabitEthernet0/2 unassigned YES unset administratively down down 
Serial0/0/0 185.95.13.2 YES manual up up 
Serial0/0/1 185.95.23.2 YES manual up up 
Vlan1 unassigned YES unset administratively down down
R3#show ip route
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
* - candidate default, U - per-user static route, o - ODR
P - periodic downloaded static route

Gateway of last resort is not set

185.95.0.0/16 is variably subnetted, 9 subnets, 3 masks
O 185.95.1.0/24 [110/65] via 185.95.13.1, 00:10:17, Serial0/0/0
O 185.95.2.0/24 [110/65] via 185.95.23.1, 00:10:17, Serial0/0/1
C 185.95.3.0/24 is directly connected, GigabitEthernet0/0
L 185.95.3.1/32 is directly connected, GigabitEthernet0/0
O 185.95.12.0/30 [110/128] via 185.95.13.1, 00:10:17, Serial0/0/0
[110/128] via 185.95.23.1, 00:10:17, Serial0/0/1
C 185.95.13.0/30 is directly connected, Serial0/0/0
L 185.95.13.2/32 is directly connected, Serial0/0/0
C 185.95.23.0/30 is directly connected, Serial0/0/1
L 185.95.23.2/32 is directly connected, Serial0/0/1

R3#show ip osp
R3#show ip ospf ne
R3#show ip ospf neighbor 


Neighbor ID Pri State Dead Time Address Interface
2.2.2.2 0 FULL/ - 00:00:38 185.95.23.1 Serial0/0/1
1.1.1.1 0 FULL/ - 00:00:34 185.95.13.1 Serial0/0/0
R3#show ip os
R3#show ip ospf da
R3#show ip ospf database 
OSPF Router with ID (3.3.3.3) (Process ID 1)

Router Link States (Area 0)

Link ID ADV Router Age Seq# Checksum Link count
2.2.2.2 2.2.2.2 629 0x80000005 0x005cd3 5
3.3.3.3 3.3.3.3 627 0x80000005 0x00d255 5
1.1.1.1 1.1.1.1 627 0x80000005 0x00af9a 5
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