Networks and Cybersecurity Essentials (ACCA4024)
Lab 1 : Design and Connect a Simple Network and determine IP Address
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Task 1.
7.
	a)	What is the IP address of the computer?
		192.168.1.10
	What is the subnet mask of the computer?
	255.255.255.0
b)	Was the ping successful?
	Yes, 4/4 packets returned
8.
	a)	What is the IP address of the computer?
		192.168.1.11
	What is the subnet mask of the computer?
	255.255.255.0
b)	Was the ping successful?
	Yes, 4/4 packets returned

Task 2.
5.		IP address is manually configured
8.		Yes, ping was successful
9.		The trace completed in 8 hops. 
First hop involves the default gateway of my machine. 
Second hop involves my DNS server, not sure what ttrouter means.
I’m guessing the hops are the steps through the network from me to Google.
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