Packet Tracer – Troubleshoot Enterprise Networks

Part 1 – 
C: Currently assigned to VLAN 10 are ports F0/3 and F0/4.
D: PC1 does not have an assigned IP address only an Automatic Private IP Addressing (APIPA) address. 
F:  PC1 now has the IP address 192.168.10.10
G: One problem was highlighted when running the command on S3, S3 shows Po1 as down. 
I: On S2, G0/1 is showing VLAN 1 as the Native VLAN. 

Part 2 – 
A: checking Ips on PC 3 & 4, I can see the incorrect Gateway IP on both. They’re current Gateway IP’s are 192.168.30.1. 
B: I can see in both LAN40 and LAN50 Pools the Default router settings are incorrect. 
C: I could ping all IPv4 addresses in the R3 DHCP pool.

Part 3 – 
A: All of the networks appear in the routing tables. 
B: The ping failed. This should have been successful. 

Part 4 – 
A: in the routing table for R1 I can see the 192.168.20.0 network is using S0/1/0. Also the default route is using the serial link. 
D: Ping to TFTP server was successful but the Outside Host ping failed. This could be an issue with R2. 

