Was ping successful? Yes
	Description
	Physical Address

	Intel(R) Ethernet Connection
	2C-4D-54-4C-BE-26

	Bluetooth Device
	BC-A8-A6-F4-95-88

	Microsoft Wi-fi Direct Virtual Adapter
	Bc-A8-A6-F4-95-85



How many MAC addresses did you discover in your PC? 3
	Manufacturer OUI
	Unique Identifier for the Interface
	Vendor Name

	2C:4D:54
	4C-BE-26
	ASUSTek COMPUTER INC

	BC-A8-A6
	F4-95-88
	Intel Corporate

	BC-A8-A6
	F4-95-85
	Intel Corporate



How many different vendors did you discover? 2
Record your Reflection 
1. Why might a computer have more than one MAC address? 
PC’s have multiple NIC (Network Interface Cards), with each have their own MAC addresses. 
2. Try connecting and disconnecting the network cable(s) to your network adapter(s) and use the ipconfig /all again. What changes do you see? Does the MAC address still display? Will the MAC address ever change? 
No, the MAC address will never change as it is permanently assigned to a device. It will not change under any circumstances. 
3. What are other names for the MAC address?
Another name for a MAC address is a physical address. 

Task 3:
What is the Service Set Identifier (SSID) for the wireless router of your connection?
SKY74B84
What is the speed of your wireless connection?
52Mbps
What is the MAC address of your wireless NIC?
BC-A8-A6-F4-95-84
Why would you activate more than one NIC on a PC?
In the case where one NIC fails, it is still possible to connect to a network. 

Task4:
Does the Source MAC address match your PC’s interface? 
Yes
What is the result of executing the arp –a command on your PC? 
The ARP command located another 7 devices situate on the same network
Which option deletes an entry from the ARP cache? 
Arp –d
What would be the result of issuing the arp –d * command?
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What is a benefit of keeping ARP cache entries in memory on the source computer?
Prevents needlessly broadcasting ARP requests, as it is possible to reference the local cache saved on the device.  
If the destination IPv4 address is not located on the same network as the source host, what MAC address will be used as the destination target MAC address in the frame?
The device will use the MAC address of the default gateway
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Deletes the host specified by inet_addr. inet_addr may be
Wildcarded with * vo delete all hoses.




