Hydraulic geometry

	Channel width
	Use a tape measure held across the channel just above the water level

	Bank-full width
	Use a tape measure held across the channel at the break of slope on each side

	Channel depth
	Use a meter rule. Take readings at regular interval across the channel

	Bank-full depth
	Use a meter rule to measure the vertical distance between the water level and the line of bank-full width

	Wetted perimeter
	Use a tape measure or chain to measure the total distance that the water is in contact with the bed and the banks

	Cross-sectional area
	[bookmark: _GoBack]Channel width x average water depth
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