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R3gsho run
Building configuration...

Curzent configuravion : 1589 byves
version 15.4

no service vimestamps log davevime msec
no service vimestamps debug davecime msec

service password-encryprion

hostnsme 23

enable secrec § 313mERrsy/Ce71zaULOROUIQUGWE/

no ip cef
ipve unicasc-rousing

no ipve cef

interface GigabitZthernesd/o/0
descripoion 23 to BCL

ip address 152.163.2.1 255.255.255.0
aquplex auco

speed auto

ipve address FE80::3 link-local
ipve address 2001:2222:ABCD: €521
interface GigabitEthernesd/o/1
no ip address

duplex auco

speed auto
=hucdoun

ses
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interface GigabitZthernet0/0/2
no ip address
duplex auco

speed auto
=hucdoun

interface Serialo/2/o
no ip address

Clack rate 2000000
shucdown

interface Serialo/2/1
descripoion 23 to AL

bandwiden S12

ip address 152.163.4.2 255255255252
ipve address FE80::3 link-local

ipve address 2001:4444:ABCD: €34

interface Viaal

no ip address
shucdoun

ses

classiess
zouce 152.163.1.0 255.255.255.0 Serialo/2/1

route 172.16.1.33 255.255.255.255 152.163-4.1
zouce 152.163.3.0 255 255 255 252 Serialo/2/1

ip flow-expors version 3

ipve route 2001:ABCD:BCDE:1€10::/64 2001:4444:ABCD: €340
ipve route 2001:1111:ABCD:€310::/64 Serialo/2/1

ipve route 2001:3333:ABCD:€330:1/64 Serialo/2/1

no cdp run
banner motd ~C unsuchorized access prohibited AT

ine con 0
password 7 082945420516544541
logging synchronous
login

line sux 0

Line vey 0 1
password 7 082949420516514244
login local
cranspors inpuc telnet

Line vey 2 4
1ogin
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Rlgsho run
Building configuravion

Current configuravion : 1827 byves
version 15.4

no service vimestamps log davevime msec
no service vimestamps debug davecime msec

service password-encryprion

hostnsme A1

enable secrec § 313mERrsy/Ce71zaULOROUIQUGWE/

ip cer
ipve unicasc-rousing

interface Losphackl
description A1 loopback

ip address 172.16.1.33 255.255.255.255
ipve address FE80::1 link-local

interface Losphacks
descripoion A1 loopback 2

no ip address

ipve address FE80::1 link-local

ipvé address 2001-ABCD:BCDE:1€10::33/€4
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interface GigabitEthernesd/o/0
no ip address

duplex auco

speed auto

=hucdoun
interface GigabitEthernesd/o/1
no ip address

duplex auco

speed auto
=hucdoun

interface GigabitEthernetd/0/2
no ip address

duplex auco

speed auto

=hucdoun
interface Serialo/2/o

descripoion A1 to 22

bandwideh S12

ip address 152.163.3.1 255255255252
ipve address FE80::1 link-local

ipve address 2001:3333:ABCD: €330

interface Serialo/2/1
descripoion A1 to 23

bandwideh S12

ip address 152.163.4.1 255255255252
ipve address FE80::1 link-local

ipve address 2001:4444:ABCD: €340
pe———
interface Viaal

no ip address

shucdoun

1768

1768

ip classless
ip rouce 152.163.1.0 255.255.255.0 Serialo/2/0
ip rouce 152163 2.0 255,255 2550 Serialo/2/1

ip flow-expors version 3
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1line con 0
password 7 082945420516544541
logging synchronous
login

line sux 0
Line vey 0 1

password 7 082949420516514244
login local

cranspors inpuc telnet

Line vey 2 4

1ogin
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R2(config)#do sho run
Building configuracion.

Curzent configuravion : 1657 byves
version 15.4

no service vimestamps log davevime msec
no service vimestamps debug davecime msec

service password-encryprion

hostnsme 22

enable secrec § 313mERrsy/Ce71zaULOROUIQUGWE/

no ip cef
ipve unicasc-rousing

descripoion 22 to BC 2
ip address 152 1€3.1.1 255.255.255.0
aquplex auco

speed auto

ipve address ¥E30

interface GigabitEthernesd/o/1
no ip address
duplex auco

speed auto
<hutdown
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interface GigabitEthernetd/0/2
no ip address
duplex auco
speed auto
=hucdoun

interface Serialo/1/o
descripoion 22 ©o AL
bandwideh S12
ip address 152.163.3.2 255.255.255.252
ipve address FE80::2 link-local
ipve address 2001:3333:ABCD: €330

pe———

interface Serialo/1/1
no ip address

Clack rate 2000000
shucdown

interface Viaal
no ip address

shucdoun

ip classless

ip rouce 172.16.1.33 255.255.255.255 152 163.3.1
ip rouce 152.163.2.0 255,255 2550 Serialo/1/0
ip rouce 152.163 4.0 255 255 255 252 Serialo/1/0
ip rouce 152.163.3.0 255 255 255 252 Serialo/1/0

ip flow-expors version 3

ipve route 2001:ABCDIBCDE:1€10::/64 2001:3333:ABCD: €330
ipve zoute 200. /€4 serialo/i/o
/€4 seriatoriso

ine con 0
password 7 082945420516544541
logging synchronous
login

line sux 0

Line vey 0 1
password 7 082949420516514244
login local
cranspors inpuc telnet

Line vey 2 4
login
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