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	Assume ‘g’  =  9.81 m/s2.

	








ANSWER 4 QUESTIONS FROM 5

QUESTION ONE (SUSPENSION AND CHASSIS SYSTEMS)

Define the following terms (use diagrams where appropriate) and explain how these effect the performance of a suspension system

i) Camber			(2 marks)						
ii) Caster Angle		(2 marks)
iii) Instant centre		(3 marks)
iv) Roll centre			(3 marks)

QUESTION TWO (TYRES AND WEIGHT TRANSFER)

A vehicle of mass 915Kg drives around a 130m radii corner at 25m/s. If the vehicle has a centre of gravity height of 0.375m an average track of 1.16m and a wheelbase of 2.65m. 

i) Show that the lateral acceleration of the vehicle is 4.81m/s2. 		(2 marks)
ii) Calculate the lateral load transfer which would be experienced by the vehicle during the turn. 								(3 marks)
iii) Explain why load transfer has a detrimental impact on the overall available grip for a vehicle.								(3 marks)
iv) With the aid of a diagram explain what is meant by the term ‘Slip Angle’
(2 marks)


QUESTION THREE (SPRINGS AND DAMPING)

The front suspension for a Dakar Rally vehicle may be modelled as a system of springs in series and parallel as shown below. 
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Ms             Sprung Mass = 215 Kg
K1             Helper Spring Rate = 13 000 N/m
K2             Main Spring Rate = 28 000 N/m


i) Calculate the overall spring rate of the suspension system.  		(3 Marks)
ii) Calculate the natural frequency of the suspension system.		(2 Marks)
iii) Comment on the natural frequency of the suspension system with reference to its suitability to an off road vehicle.						
(2 Marks)

iv) Draw a diagram to show the response of a spring mass damper system when undamped, overdamped and underdamped.
(3 Marks)


QUESTION FOUR (BRAKES)

A vehicle of total mass 875 kg must decelerate at 7.5 m/s2 when it’s disc brakes are applied. If as a worst case scenario of 100% longitudinal weight transfer is assumed, calculate;

i) The deceleration force required to be produced by the front brake system.

(2 Marks)
ii) The pedal force required if the brake system specification is as follows;

(8 Marks)

Pedal Ratio					4:1
Master Cylinder Piston Diameter		15.875 mm
Slave Cylinder Piston Area Diameter		44.45 mm
Number of Slave Cylinders			2
Effective Pad Radius				0.15m
Pad Coefficient of Friction			0.42
Rolling Radius 				0.285m


QUESTION FIVE (AERODYNAMICS)

A single seater race car with frontal area 1.1m2 is tested in the wind tunnel at 35 m/s2 and found to produce aerodynamic forces measured at the wheels as shown below. Take the density of air to be 1.223 Kg/m3
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i) Explain how the velocity of air around the vehicle relates to the pressure acting on the vehicle surface.
(3 Marks)

ii) Calculate the total downforce produced and the corresponding coefficient of lift for the car.
(3 Marks)

iii) Calculate the drag force which would be produced if the coefficient of drag for the vehicle is 0.67
(2 Marks)

iv) Calculate the centre of pressure (%) for the vehicle. 
(2 Marks)
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