Lab 4
Network Diagrams
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Addressing Table
	Device 
	Interface 
	IP Address 
	Subnet Mask 
	Default Gateway 

	R1
	Gig0/0/1
	192.168.2.1
	255.255.255.0
	

	R1
	Gig0/0/0
	192.168.1.1
	255.255.255.0
	

	R1
	Se0/1/0
	11.0.0.1
	255.255.255.252
	

	S0 
	SVI Interface
	192.168.2.9
	255.255.255.0
	192.168.2.1

	S1 
	SVI Interface
	192.168.1.9
	255.255.255.0
	192.168.1.1

	WirelessRouter1
	Ethernet 1
	192.168.1.11
	255.255.255.0
	

	PC0
	Fa0
	192.168.1.10
	255.255.255.0
	192.168.1.1

	Server0
	Fa0
	192.168.2.2
	255.255.255.0
	192.168.2.1

	Printer0
	Fa0
	192.168.2.5
	255.255.255.0
	192.168.2.1

	Laptop0
	Wireless0
	192.168.1.100 (DHCP)
	255.255.255.0
	192.168.1.11




Router / Switch Credentials
	Device
	User Exec Mode Password
	Privileged EXEC Mode Password

	R1
	cisco
	class123

	S1
	cisco
	class123

	S0
	cisco
	class123



	Device
	Connection Type
	Username
	Password

	R1
	SSH
	admin
	ciscovty

	S1
	SSH
	admin
	ciscovty

	S0
	SSH
	admin
	ciscovty



Wireless PSK Pass Phrase: wireless123




Connectivity ICMP tests
Laptop0
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Connectivity SSH tests
PC0
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Tracert
PC0 -> server0
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Server0 -> PC0
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Server0 -> Laptop0
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Laptop0 -> Server0
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