Task 1 – Network Test

Windows Server
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Linux Server
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Mindows TP Configuration

Host Name .
Primary Dns Suffix’
Node Type . . .

Ip Routing Enabled.
WINS Proxy Enabled.

DNS Suffix Search List.

Ethernet adapter Intswa:

Connection-specific DNS Suffix
Description .

Physical Address.

DHCP Enabled. .
Autoconfiguration Enabled .
Link-local IPv6 Address .
1Pv4 Address.

Subnet Mask .

Default Gateway .

DHCPYV6 TATD . .

DHCPYV6 Client DUID.

DNS Servers .

NetBIOS over Tcpip.
Ethernet adapter External:

Connection-specific DNS Suffix
Description .

Physical Address.

DHCP Enabled. .
Autoconfiguration Enabled .
Link-local IPv6 Address .
1Pv4 Address.

Subnet Mask .

Default Gateway .

DHCPYV6 TATD . .

DHCPYV6 Client DUID.

DNS Servers .

NetBIOS over Tcpip.
PS C:\Users\Administrator>

s-DC
swansea.acca

: swansea.acca

Intel(R) PRO/1066 MT Desktop Adapter #2
08-00-27-41-14-F7

No

Yes

Fego: :4be3:4d1d: 3a0e: 5e44%13 (Preferred)
192.168.1.1(Preferred)

255.255.255.6

168296487
00-01-00-01-30-66-31-06-08-00-27-1A-80-9D

127.6.0.1

: Enabled

Intel(R) PRO/1066 MT Desktop Adapter #3

08-06-27-26-88-9C
No

Yes

Fego: :f421:4636:8514:3a18%15 (Preferred)
20.6.0.1(Preferred)

255.255.255.252

185073703
00-01-00-01-30-66-31-06-08-00-27-1A-80-9D

192.168.1.1

w0
~ 8% g0
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PS C:\Users\Administrator> ping 192.168.1.16

Pinging 192.168.1.10 with 32 bytes of data:
Reply from 192.168.1.10: bytes=32 time<ims TTL-128
Reply from 192.168.1.16: bytes=32 time<ims
Reply from 192.168.1.16: bytes=32 time<ims
Reply from 192.168.1.16: bytes=32 time<ims

Ping statistics for 192.168.1.1
Packets: Sent = 4, Received = 4, Lost = © (8% loss),
Approximate round trip times in milli-seconds:
Minimun = @ms, Maximum - ems, Average = 6ms
PS C:\Users\Administrator> ping 192.168.2.1

Pinging 192.168.2.1 with 32 bytes of data:
Reply from 192.168.2.1: bytes=32 time<ims TTL-64
Reply from 192.168.2.1 2 time<ins
Reply from 192.168.2.1
Reply from 192.168.2.1:

2 timecims TTL=64

Ping statistics for 192.168.2.1
Packets: Sent = 4, Received = 4, Lost = © (8% loss),
Approximate round trip times in milli-seconds:
Minimun = ems, Maximum - ems, Average = 6ms
PS C:\Users\Administrator> o
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Debian GNU/Linux 13 L-CD ttyl

L-CD login: Notebook@i2s
Passuord:
Login incorrect

L-CD login: landonlogin
Passuord:

Linux L-CD 6.12.48+deb13-amd6d #1 SMP PREEMPT_DYNAMIC Debian 6.12.48-1 (2025-09-20) x86_64

The programs included with the Debian GNU/Linux system are free sof tuare;
the exact distribution terms for each program are described in the
individual files in /usr/share/doc/+/copyright.

Debian GNU/Linux comes with ABSOLUTELY NO WARRANTY, to the extent
permitted by applicable law.
Londonlogin@L-CD: ™8 ip a
+ 1o <LOOPBACK,UP,LOMER_UP> mtu 65536 gdisc nogueue state UNKNOWN group default glen 1000
Link/loophack 00:00:00:00:00:00 brd 00:00:00:00:00:00
inet 127.0.0.1/8 scope host lo
! valid_Lft forever preferred_lft forever
ineté /128 scope host noprefixroute
valid_Lft forever preferred_lft forever
2: enpos9: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 odisc fo_codel state U group default glen 1008
Link/ether 08:00:27:fc:ge:dc brd £1:F1:Ff it
altname enxo80027fceede
- inet 20.0.0.2/30 brd 20.0.0.3 scope global enposd
valid_Lft forever preferred_lft forever
ineté -~ oo oo /64 scope link proto kernel 11
valid_Lft forever preferred_lft forever
: enposio: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 odisc fo_codel state U group default glen 1008
Link/ether 08:00:27:34:10:15 brd ff:ff:ff:ff:ffff
altname enxo80027341015
inet 192.168.2.1724 brd 192.165.2.255 scope global enposie
valid_Lft forever preferred_lft forever
inete oo o0 /64 scope link proto kernel 11
valid_Ift forever preferred_lft forever
Londonlog in@L-CD: ™%
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Londonlogin@L-CD:™$ ping 192.168.1.

PING 192.166.1.1 (192.168.1.1) 56(84) butes of data
b4 bytes from 192.168.1. _: .753 ms
b4 butes from 192.168.1. .35¢ ms
b4 butes from 192.168.1. _: 657 ms
b4 butes from 192.168.1 469 ms
C

-- 192.168.1.1 ping statistics ---

4 packets transmitted, 4 received, 0% packet loss, time 3095ms
rtt min/ave/max/mdev = ©.354/0.558/0.753/0.156 ms
LondonloginL-CD: ™% ping 192.168.1.10

PING 192.166.1.10 (192.168.1.10) 56(84) bytes of data

b4 butes from 192.168.1.10: icmp_seq=1 tt1=127 time=1.06 ms
b4 bytes from 192.168.1.18: icmp_seq=2 tt1=127 time=0.346 ms
b4 bytes from 192.168.1.18: icmp_seq=3 tt1=127 time=0.747 ms
B4 bytes from 192.168.1.10: icnp_seq=4 tt1=127 time=2.25 ms

C
-- 192.168.1.10 ping statistics ---

4 packets transmitted, 4 received, 0% packet loss, time 3053ms
rtt min/ave/max/miev = ©.747/1.243/2.246/0.586 ms

Londonlog inL-CD: ™%





