
	
	METHOD STATEMENT
PLASTERBOARDING
	
Effective: 08/02/2022


	PERSON COMPLETING
	Adam George

	LOCATION
	POBL-SA1, Swansea

	SUPERVISOR
	Adam George
	OPERATIVES.
	

	EMERGENCY CONTACT
	Adam George - 07432469686
	SERVICES – 999


	START DATE
	07/06/2022
	COMPLETION DATE
	21/06/2022


	METHOD OF WORK
Deliveries
Where practicable arrange deliveries of materials to times where other traffic is at lowest level. Establish unloading point and control access to ensure non-construction personnel/visitors and residents of the site are excluded from vehicle movement, unloading and storage points.

Inspect load before unloading from vehicle and ensure only necessary site personnel are in vicinity of unloading. Ensure all cement bags are stored in stable dry conditions and that sand piles are strategically deposited near to designated mixing area to reduce congestion on site and ease of access to the working area.

Distribution to Site
Plaster boards are to be handled by mechanical means where practicable. Ground conditions/stacking point are to be firm and level with debris and waste materials cleared away. Access to work area must be planned for in the design of scaffolding.
Ensure all loads are stable before lifting.

Plan loading out of work platform to enable the plaster spots to be placed appropriately and reduce the need for twisting and lifting. Ensure that all unnecessary site personnel are excluded from the work area.

Set-up
Remove all debris from work areas. Dispose of debris in designated areas.
Remove unnecessary obstructions and debris from plot and deposit in waste receptacles or designated storage. Ensure that scaffold is complete before entering platform.
Ensure that any scaffold required is erected to facilitate safe working and report any defects to site controller. Do Not remove any scaffolding parts/ties or boards this is a will place the operative in breach of legislative requirements and make the scaffold unfit for access.

Plasterboard Fixing
Measure and cut plasterboard using a suitable hand tool as required for size and area of wall/ceiling where application is required. Lift plaster board into place ensuring good posture throughout and avoid over reaching.
For plasterboards being secured above 1.5 metres as secure platform is to be used.
For plasterboards secured to ceilings mechanical means of support are to be used prior to fixing.
Plaster boards are to be fixed in place using nails or screws, ensuring there is enough fixing for next board where multiple boards are required to be secured.

Clean up.
Ensure all debris is removed at the completion of work period and deposit into waste receptacles provided. All boards from scaffolded areas are to be replaced immediately to ensure safety of other site personnel. Do not drop debris from height, use chutes or containers. Ensure only authorised persons are in the vicinity.
At end of task clean tools. Leave all areas in clean condition.









	Document Approved by: (Print)
Adam George
	Signature:

A.George
	Position:

Site Manager
	Date:



	I understand the information presented in this document and will work in line with the stated method

	Name
	Company
	Signature
	Date

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	




