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Lab - Building an Ethernet Crossover Cable

Lab – Understanding Ethernet Cable Standards 
Topology
[image: ]
Addressing Table
	Device
	Interface
	IP Address
	Subnet Mask
	Default Gateway

	PC-A
	NIC
	192.168.10.1
	255.255.255.0
	N/A

	PC-B
	NIC
	192.168.10.2
	255.255.255.0
	N/A


Objectives
Part 1: Analyze Ethernet Cabling Standards and Pinouts
Part 2: Build an Ethernet Crossover Cable
Part 3: Test an Ethernet Crossover Cable
Background / Scenario
In this lab, you will build and terminate an Ethernet crossover cable and test it by connecting two PCs together and pinging between them. You will first analyze the Telecommunications Industry Association/Electronic Industries Association (TIA/EIA) 568-A and 568-B standards and how they apply to Ethernet cables. You will then construct an Ethernet crossover cable and test it. Finally, you will use the cable you just constructed to connect two PCs together and test it by pinging between them.
Note: With autosensing capabilities available on many devices, such as the Cisco 1941 Integrated Services Router (ISR) switch, you may see straight-through cables connecting like devices.
Required Resources
One length of cable, either Category 5 or 5e. Cable length should be 0.6 to 0.9m (2 to 3 ft.)
2 RJ-45 connectors
RJ-45 crimping tool
Wire cutter
Wire stripper
Ethernet cable tester (optional)
2 PCs (Windows 7 or 8)
Analyze Ethernet Cabling Standards and Pinouts
The TIA/EIA has specified unshielded twisted pair (UTP) cabling standards for use in LAN cabling environments. TIA/EIA 568-A and 568-B stipulates the commercial cabling standards for LAN installations; these are the standards most commonly used in LAN cabling for organizations and they determine which color wire is used on each pin.
With a crossover cable, the second and third pairs on the RJ-45 connector at one end of the cable are reversed at the other end, which reverses the send and receive pairs. The cable pinouts are the 568-A standard on one end and the 568-B standard on the other end. Crossover cables are normally used to connect hubs to hubs or switches to switches, but they can also be used to directly connect two hosts to create a simple network.
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Research report on cat5e and cat6 ethernet cable standards

Introduction:
This report will be talking about cat5e and cat6 ethernet cable standards and the differences between them. 

Cat5e:
Cat5e cables are simply Cat5 cables but the e in Cat5e stands for enhanced, which means that this is an upgraded version of Cat5 cables which can only support up to 100 Megabits per second. Cat5e cables are a commonly used cable due to its flexibility when it comes to data speed over distances. Cat5e can reach up to 1Gigabit per second network speed but still has 100-Megahertz bandwidth usage. [1] 
Cat5e cables were designed to limit the amount of cross talk on a network to be able to reach network speeds up to 1Gbps. These cables are also much more cost effective which plays a big role in why Cat5e cables are so common. [5]

Cat6:
Cat6 ethernet cables are a newer type of ethernet cable that aren’t as cost effective as your standard cat5 or cat5e cables, but these cables do have a lot of potential when it comes to network speed Cat6 cables are also backwards compatible with Cat5 and Cat5e cables, these cables can also come shielded or unshielded unlike Cat5 or Cat5e cables. Cat6 cables can support up to 10 Gigabits per second on a network but data speed starts to drop after a certain distance, these cables are usually used in homes or businesses and are usually used in the router since Cat6 cables are capable reaching 10 Gigabit per second speeds. [2] [1]


The difference between cat5e and cat6 cables:
When it comes to comparing these types of cables, they only have 1 thing in common visually and that is the RJ45 connector since this allows this cable to be plugged into anything that has an ethernet port.
For over all better performance and best possible speeds generally you would use a Cat6 but as mentioned before these cables do have a drop off at a certain distance and once that drop of hits the cable has the same speed as a Cat5e cable however when it comes to cross talk on the network a Cat6 cable is better for reducing the noise within the network.
When looking at a price range and the differences between these 2 cables generally most would go for the Cat5e cable due to the fact that its cheaper and the performance can usually be seen as negligible when it comes to the network speed between the 2 since the Cat5e cable can maintain its 1Gbps speed over greater distances where as Cat6 cables loses its 10gbps over a shorter distance in comparison to the Cat5e cable so that way Cat5e and Cat6 cables will have the same speed of 1 Gbps speed and choosing a cable really depends on the price range of a buyer.
The last differences between the 2 really is that Cat6 is backwards compatible with Cat5e, Cat5 and up to even Cat3 cables where as Cat5e is only backwards compatible with Cat5 cables and below it. [3] [4]
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Write a research report (Max word count 600) on Cat 5e and 6 Ethernet cable standards.  
Analyze diagrams and tables for the TIA/EIA 568-A standard Ethernet cable.
The following table and diagrams display the color scheme and pinouts, as well as the function of the four pairs of wires used for the 568-A standard. 
Note: In LAN installations using 100Base-T (100 Mb/s), only two pairs out of the four are used.
568-A 10/100/1000Base-TX Ethernet
	Pin Number
	Pair Number
	Wire Color
	10Base-T Signal
100Base-TX Signal
	1000Base-T Signal

	1
	2
	White/Green
	Transmit
	BI_DA+

	2
	2
	Green
	Transmit
	BI_DA-

	3
	3
	White/Orange
	Receive
	BI_DB+

	4
	1
	Blue
	Not Used
	BI_DC+

	5
	1
	White/Blue
	Not Used
	BI_DC-

	6
	3
	Orange
	Receive
	BI_DB-

	7
	4
	White/Brown
	Not Used
	BI_DD+

	8
	4
	Brown
	Not Used
	BI_DD-




The following diagrams display how the wire color and pinouts align with an RJ-45 jack for the 568-A standard.
[image: T-568A]
[image: RJ-45 Jack]
Analyze diagrams and tables for the TIA/EIA 568-B standard Ethernet cable.
The following table and diagram display the color scheme and pinouts for the 568-B standard.
568-B 10/100/1000-BaseTX Ethernet
	Pin Number
	Pair Number
	Wire Color
	10Base-T Signal
100Base-TX Signal
	1000Base-T Signal

	1
	2
	White/Orange
	Transmit
	BI_DA+

	2
	2
	Orange
	Transmit
	BI_DA-

	3
	3
	White/Green
	Receive
	BI_DB+

	4
	1
	Blue
	Not Used
	BI_DC+

	5
	1
	White/Blue
	Not Used
	BI_DC-

	6
	3
	Green
	Receive
	BI_DB-

	7
	4
	White/Brown
	Not Used
	BI_DD+

	8
	4
	Brown
	Not Used
	BI_DD-


[image: T568B_ColorPinout_AndRJ45Jack]


Build an Ethernet Crossover Cable
A crossover cable has the second and third pairs on the RJ-45 connector at one end, reversed at the other end (refer to the table in Part 1, Step 2). The cable pinouts are the 568-A standard on one end and the 568-B standard on the other end. The two following diagrams illustrate this concept.
[image: Cross_over_CableRJ45Connectors_1]
Build and terminate a TIA/EIA 568-A cable end.
Determine the cable length required. (Your instructor will let you know the cable length you should make.)
Note: If you were making a cable in a production environment, the general guideline is to add another 12 in. (30.48 cm) to the length.
Cut off a piece of cable to the desired length and using your wire stripper, remove 5.08 cm (2 in.) of the cable jacket from both ends.
Hold the four pairs of twisted cables tightly where the jacket was cut away. Reorganize the cable pairs into the order of the 568-A wiring standard. Refer to the diagrams, if necessary. Take as much care as possible to maintain the twists in the cable; this provides noise cancellation.
Flatten, straighten, and line up the wires using your thumb and forefinger.
Ensure that the cable wires are still in the correct order for the 568-A standard. Using your wire cutters, trim the four pairs in a straight line to within 1.25 to 1.9 cm (1/2 to 3/4 in.).
Place an RJ-45 connector on the end of your cable, with the prong on the underside pointing downward. Firmly insert the wires into the RJ-45 connector. All wires should be seen at the end of the connector in their proper positions. If the wires are not extending to the end of the connector, take the cable out, rearrange the wires as necessary, and reinsert the wires back into the RJ-45 connector.
If everything is correct, insert the RJ-45 connector with cable into the crimper. Crimp down hard enough to force the contacts on the RJ-45 connector through the insulation on the wires, thus completing the conducting path. See the following diagram for an example.
[image: crimp_Pic]
Build and terminate a TIA/EIA 568-B cable end.
Repeat steps 1a to 1g using the 568-B color wiring scheme for the other end.
Test an Ethernet Crossover Cable
Test the cable.
Many cable testers will test for length and mapping of wires. If the cable tester has a wire map feature, it verifies which pins on one end of the cable are connected to which pins on the other end.
If your instructor has a cable tester, test the crossover cable for functionality. If it fails, check with your instructor first as to whether you should re-cable the ends and re-test.
Connect two PCs together via NICs using your Ethernet crossover cable.
Working with a lab partner, set your PC to one of the IP addresses shown in the Addressing Table (see page 1). For example, if your PC is PC-A, your IP address should be set to 192.168.10.1 with a 24-bit subnet mask. You partner’s IP address should be 192.168.10.2. The default gateway address can be left empty.
Using the crossover cable you made, connect the two PCs together via their NICs.
On the PC-A command prompt, ping the PC-B IP address.
Note: The Windows firewall may have to be temporarily disabled for pings to be successful. If the firewall is disabled, make sure you re-enable it at the conclusion of this lab.
Repeat the process and ping from PC-B to PC-A.
Assuming IP addressing and firewall are not issues, your pings should be successful if the cables were properly made.
Reflection
Which part of making cables did you find the most difficult?
During this task I had found it difficult to keep the wires straight when putting them into each terminal and I couldn’t make an ethernet cable work due to this.


Why do you have to learn how to make a cable if you can easily buy pre-made cables?
[bookmark: _GoBack]The reason we must learn how to make ethernet cables is due to that if everyone just bought premade cables there would be no one left to make these ethernet cables also it is much more expensive to buy premade cables than it is to make one yourself.
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