S1#show ip interface brief
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  153.99.11.10    YES manual up                    up
FastEthernet0/1        unassigned      YES unset  down                  down
FastEthernet0/2        unassigned      YES unset  down                  down
FastEthernet0/3        unassigned      YES unset  down                  down
FastEthernet0/4        unassigned      YES unset  down                  down
FastEthernet0/5        unassigned      YES unset  down                  down
FastEthernet0/6        unassigned      YES unset  up                    up
FastEthernet0/7        unassigned      YES unset  down                  down
FastEthernet0/8        unassigned      YES unset  down                  down
FastEthernet0/9        unassigned      YES unset  down                  down
FastEthernet0/10       unassigned      YES unset  down                  down
FastEthernet0/11       unassigned      YES unset  down                  down
FastEthernet0/12       unassigned      YES unset  down                  down
FastEthernet0/13       unassigned      YES unset  down                  down
FastEthernet0/14       unassigned      YES unset  down                  down
FastEthernet0/15       unassigned      YES unset  down                  down
FastEthernet0/16       unassigned      YES unset  down                  down
FastEthernet0/17       unassigned      YES unset  down                  down
FastEthernet0/18       unassigned      YES unset  down                  down
FastEthernet0/19       unassigned      YES unset  down                  down
FastEthernet0/20       unassigned      YES unset  down                  down
 --More--
FastEthernet0/21       unassigned      YES unset  down                  down
FastEthernet0/22       unassigned      YES unset  down                  down
FastEthernet0/23       unassigned      YES unset  down                  down
FastEthernet0/24       unassigned      YES unset  down                  down
GigabitEthernet0/1     unassigned      YES unset  down                  down
GigabitEthernet0/2     unassigned      YES unset  down                  down

S1#show running-config
Building configuration...

Current configuration : 1511 bytes
!
! Last configuration change at 01:34:29 UTC Mon Mar 1 1993
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
enable password class
!
no aaa new-model
system mtu routing 1500
!
!
!
!
!
!
!
no ip domain-lookup
!

Router1#show running-config
Building configuration...


Current configuration : 1303 bytes
!
! Last configuration change at 13:13:32 UTC Tue Jan 14 2020
!
version 16.9
service timestamps debug datetime msec
service timestamps log datetime msec
platform qfp utilization monitor load 80
no platform punt-keepalive disable-kernel-core
!
hostname Router1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$DRvi$wgE30ARtQyfph1bs5O4kb1
enable password class
!
no aaa new-model
!
no ip domain lookup
ip admission watch-list expiry-time 0
!
!
!
!
!
!
!
!
!
!
subscriber templating
multilink bundle-name authenticated
!
!
!
!
!
license udi pid ISR4221/K9 sn FGL22359289
no license smart enable
diagnostic bootup level minimal
!
spanning-tree extend system-id
!
!
!
!
redundancy
 mode none
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0/0
 description Router-PC-B connection
 ip address 153.99.10.1 255.255.255.0
 negotiation auto
!
interface GigabitEthernet0/0/1
 description Router-Switch connection
 ip address 153.99.11.1 255.255.255.0
 negotiation auto
!
interface Serial0/1/0
 no ip address
!
interface Serial0/1/1
 no ip address
!
ip forward-protocol nd
no ip http server
ip http secure-server
!
!
!
!
!
 --More--
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:\Users\Student>ipconfig/all

windows TP Configuration

Host Name . . . C 2T
Primary Dns Suffix’
Node Type . . . C ... .. Hybrid
Ip Routing Enabled. . . . . . . . : Mo
WINS Proxy Enabled. . . . . . . . : No
Ethernet adapter Ethernet:
Media State . . . . : Media disconnected
Connection-specific DS Suffix’
Description . Intel(R) Ethernet Connection (2) I219-1M
Physical Address. ... ... :8C-9D-92-BF-B9-DF
DHCP Enabled. . . . St Yes
Autoconfiguration Enabled . . . . : Yes

Ethernet adapter VirtualBox Host-Only Network:

Connection-specific DNS Suffix

Description . . . . . .. ... .: VirtualBox Host-Only Ethernet Adapter
Physical Address. ©A-00-27-00-00-6D

DHCP Enabled. .
Autoconfiguration Enabled .
Link-local IPv6 Address . 562:d480:504%13 (Preferred)
1Pv4 Address. © .. .. ... :192.168.56.1(Preferred)

Subnet Mask . . . . . .. ....: 255.255.255.6

Default Gateway .
DHCPYV6 TATD . s .. ... .. :ae3308583

DHCPV6 Client DUID. . . . . . . . : ©0-81-80-61-25-4D-BO-A2-0C-9D-92-BF-B9-DF
DNS Servers . 1%

91

Fece:0:0: FFFF::3%1
NetBIOS over Tcpip. . . . . . . . : Enabled

C:\Users\Student>

12:48
AR 100
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