Risk Assessment





	Site
	University of Wales - Single Two Storey Detached Domestic Building With Loft Room
	Assessment Number
	002

	Task / Activity
	Manual Fixing and Positioning of Roof Trusses

	Date Conducted
	10.04.2020
	Date Reviewed
	
	
	

	Assessment Team 
	Assessors
	

	1

Hazard
	2

Hazard

Effect
	3  At Risk 


	4 Severity


	5 Probability


	6 Risk Rating
	7

Required Control Measures

(minimum requirements)
	8 Severity
	9 Probability
	10 Risk Rating
	11 Acceptable?  
	12

Further site/job specific controls
	13 Completed

	Falls from height - Scaffolding
	Death, broken bones etc.
	E
	5
	4
	20
	· Ensure scaffold is erected by competent person to relevant standards and view hand-over certificate (see separate RA for scaffolding)

· Ensure scaffolding is inspected by competent person at designated intervals.

· Ensure employees are instructed not to tamper with or alter scaffold and to report any defects.

· Ensure employees are trained and competent.
· Ensure access ladders are suitable, inspected and clamped off.
· Ensure employees use tool belts to carry hand tools.

· Ensure lifting equipment is used to transport any heavier items of work equipment/materials.
· Ensure scaffold staircase is provided.
· Provide soft landing systems in voids.
· Ensure employees are equipped with suitable safety boots.

· NEVER use additional items (steps etc.) to gain extra height on working platform.

· Report any suspected scaffold defects immediately to the Site Manager.

· Ensure that carpenters are trained in banksman duties for roof works.

· Ensure working platform or boarding is provided for bracing trusses etc.
	
	
	
	
	· Reinforce with tool-box talks.

· Scaffold to be provided and managed by *********.

· Scaffold must be fully enclosed with hand rail, intermediate rail, toe board and gates.

· Weather and wind speed to be checked daily and no work undertaken if site manager feels weather conditions affect the safety of the workforce.

· Ongoing scaffold inspections to be carried out by *********.
· No work from trusses etc.
	

	Falls from height – Soft landing system
	Death, broken bones
	E
	5
	4
	20
	· Soft landing system to be installed by *********.

· Soft landing system must be suitable for the construction and fitted by a competent person. 

· Only use soft landing system where enclosed scaffold work is not possible or reasonably practical.

· Ensure that competent person undertakes necessary inspections and checks of soft landing system.

· Ensure minimal height of fall from working area to soft landing.
	
	
	
	
	· Ensure competence of operatives is checked.

· Employees must be instructed not to tamper with or adjust soft landing system.
	

	Falls From Height – Handling Trusses
	Death, broken bones etc.
	E
	5
	4
	20
	· Only handle trusses where there is absolutely no safe option to use a crane or other mechanical handling.
· Ensure a wide staircase is fitted to walk the trusses up – this should be positioned in front of each property.

· Scaffolding must be totally enclosed and no sections removed.

· The internal areas must be filled with a suitable soft landing system. 

· Each property must have an enclosed scaffold platform to walk the trusses across and lower into fixing positions.

· Handling aids must be used to stabilise truss whilst lowering into position.

· Minimum four operatives must be available for operation.
	
	
	
	
	
	

	Falling material and objects
	Head injuries
	A
	3
	3
	9
	· Ensure that only the minimum amount of tools and equipment are stored on the working platform.

· Place barriers in areas where falling material may injure other workers or the public.

· Instruct employees not to throw items from the scaffold – ensure waste is removed using purpose constructed enclosed waste chutes.
· Site is enclosed with hoardings.
· Ensure employees wear suitable PPE (Steel toe cap safety boots, hard hats, impact eye protection etc.)

· Never leave waste on the scaffold deck.

· Ensure that tool belts are worn as wherever practical.
· Hard hats to be worn at all times.

· Ensure trusses are stabilised and guided into position with wooden supports.
	
	
	
	
	
	

	Use of hand tools
	Cuts, bruises etc.
	E
	2
	2
	4
	· Ensure hand tools are fit for purpose and well maintained.
· Ensure tools are visually inspected prior to use and that any defective equipment is withdrawn from service.

· Ensure tools are kept clean and sharp.

· Ensure employees are equipped with and wear suitable gloves, impact eye protection, steel toe capped safety boots and hard hats.

· Ensure tools are not left unattended at any time.

· Ensure tools are transported in a tool belt or box, never in pockets.
	
	
	
	
	Reinforce with tool-box talks.
	

	Use of power tools
	Entanglement, electric shock etc.
	
	
	
	
	· Ensure that tools supplied are suitable and adequate for the job.

· Ensure employees are trained and competent in the use of the equipment.

· Ensure all equipment is visually checked prior to use and defects reported before use.

· Ensure only battery rechargeable or 110v equipment used.

· Ensure electrical equipment is PAT tested.

· Ensure all guards and safety devices are in place before use.

· Ensure no loose clothing / jewellery / long hair is worn.

· Ensure drill bits are sharp and of the correct size.

· Ensure employees wear suitable safety boots, hard hat, impact eye protection, ear defenders and an approved respirator.

· See vibration, noise categories.
	
	
	
	
	
	

	Hazardous substances including dust
	Broken bones, cuts, bruises
	A
	3
	3
	9
	· Ensure material safety data sheets are obtained for substances used etc.
· Ensure COSHH Risk assessment is carried out for using hazardous substances.

· Ensure employees trained in safe use of chemicals.

· Ensure employees are issued with, and use suitable approved chemical resistant gloves, respirator and goggles.

· Ensure good hygiene practices are maintained and hand washes / wipes are available on site.

· Ensure first aid kit is available.

· Ensure no substances are left unattended on site at any time.

· Ensure employees use suitable respirators when creating wood dust.
	
	
	
	
	Reinforce with tool-box talks.
	

	Manual Handling
	Sprains, strains, broken bones etc.
	E
	3
	3
	9
	· Only handle trusses where there is absolutely no safe possibility of utilising a crane or other lifting equipment.
· Four workers must be available to lift trusses.

· All operatives to wear suitable approved gloves.

· The scaffold must be fitted with a wide staircase to lift the trusses into position. This must be moved per dwelling to ensure a straight lift onto the deck.

· All operatives to be trained in manual handling techniques.

· Suitable working platform decks must be provided to ensure that the trusses can be lifted into position safely.
· Ensure handling aids are used to stabilise trusses whilst positioning and securing into position.
	
	
	
	
	
	

	Authorised by

The Responsible Manager
	Signed:
	Dated:


	At Risk
	Severity
	Probability
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	E - Employees
	1
	No Injury
	1
	Very Unlikely
	1 – 5
	LO W
	A - Acceptable
	

	C - Contractors
	2
	Minor Injury
	2
	Unlikely
	6 - 14
	MEDIUM
	M - More Analysis Required
	

	V - Visitors
	3
	+3 Day Absence
	3
	Likely
	15 - 25
	HIGH
	U – Unacceptable Risk
	

	P - Public
	4
	Major Injury 
	4
	Very Likely
	
	
	
	

	A - All
	5
	Death
	5
	Virtually Certain
	
	
	
	



