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R3#sh run
Building configuravion

Cuzzent configurscien

1323 byces

version 15.4
no service vimestamps log davevime msec
no service vimestamps debug davecime msec

service password-encryprion

hostnsme 23

enable secrec § $13mERrsS.a€PATGBNAMKDLusTEkS/

ip cer
ipve cer

e

ip address 205 1€.20.225 255255255248
ipve address FE80::1 link-local
ipve address 2001:CEED:DBS:205::225/64

interface GigabitEthernesd/o/0
no ip address
duplex auco

speed auto
=hucdoun

interface GigabitEthernesd/o/1
no ip address
e s
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interface GigabitEthernesd/o/1
no ip address
duplex auco

speed auto
=hucdoun

interface GigabitEthernetd/0/2
no ip address
duplex auco

speed auto
=hucdoun
interface Serialo/2/o
no ip address
Clock rate €4000
shucdown

inverface Serialo/2/1
bandwidch S12

ip address 152.163.35.5 255255255252
ipve address FEs!

ip classless

ip zoute 0.0.0.0 0.0.0.0 209.1€.20.224

ip flow-expors version 3

cdp run

e

banner motd ~C Auchorized Ussrs Only ~C

ine con 0
password 7 0822455DUALEDELSIC
logging synchronous
login

line sux 0

Line vey 0 2
password 7 0822455DUALE130308
login local
cranspore inpuc ssh

line vey 3 4
no login

Line vey 5 15
no login
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Rlgsh run
Building configuration...

Curzent configuravion : 1533 byves
version 15.4

no service vimestamps log davevime msec
no service vimestamps debug davecime msec

service password-encryprion

hostnsme A1

enable secrec § $13mERrsS.a€PATGBNAMKDLusTEkS/

interface GigabitEthernesd/o/0
ip address 152.163.1.1 255.255.255.0
aquplex auco
speed auto
ipve address FE80::1 link-local

ipve address 2001:ABCD:CEED:

1/es

interface GigabitEthernesd/o/1
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™ ip sdaress
duplex auco
speed auto
=hucdoun

interface GigabitEthernetd/0/2
no ip address
duplex auco

speed auto
=hucdoun

interface Serialo/2/o
bandwidch S12

ip address 152.163.55.2 255255255252
ipve address FE80::1 link-local

ipve address 2001:ABCD:BEEF:10:

inverface Serialo/2/1
bandwidch S12

ip address 152 16335 ¢ 255255255252
ipve address FE80::1 link-local

ipve address 2001:ABCD:BEEF:2

Clock rate €4000

interface Viaal
no ip address
shucdoun

ip classless
ip rouce 172.16.1.0 255.255.255.0 Serialo/2/0
ip zoute 0.0.0.0 0.0.0.0 209.1€.20.224

ip flow-expors version 3

ipve zouse

0 2001:Cz2D:DB8:205:

no cdp run
banner motd ~C Auchorized Ussrs Only ~C

ine con 0
password 7 0822455DUALEDELSIC
logging synchronous
login

line sux 0

Line vey 0 2
password 7 0822455DUALE130308
login local
cranspors inpuc ssh

line vey 3 4
no login

Line vey 5 15
no login
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version 15.4
no service vimestamps log davevime msec
no service vimestamps debug davecime msec

service password-encryprion

hostnsme 22

enable secrec § $13mERrsS.a€PATGBNAMKDLusTEkS/

o ip domain-lookup

spanning-tree mode pust

interface Loopbackl
ip address 172.16.1.1 255.285.255.0
interface Loopback2

ip address 172.1€.2.1 255.285.255.0
interface Loopbacken

no ip address

ipve address FESO::1 link-local

ipve address 2001:DB8:CAFE:€0::1/64
interface Loopbackel

no ip address

ipve address FESO::1 link-local

ipve address 2001:DB8:CAFE:EL::1/e4
interface GigabicEchernet0/0/0

ip address 152.1¢5.25 €5 255.255 255 224
aquplex auco

speed auto

ipve address FEso

1 link-local
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interface GigabitEthernesd/o/1
no ip address

duplex auco

speed auto

=hucdoun

interface GigabitEthernetd/0/2
no ip address
duplex auco

speed auto
=hucdoun

interface Serialo/1/o
bandwidch S12

ip address 152.163.35.1 255255255252
ipve address FE80::2 link-local

ipve address 2001:ABCD:EEEF:10

Clock rate €4000

interface Serialo/1/1
no ip address

Clack rate 2000000
shucdown

interface Viaal
no ip address
shucdoun

no cdp run

banner motd ~C Auchorized Ussrs Only ~C

ine con 0
password 7 0822455DUALEDELSIC
logging synchronous
login

line sux 0

Line vey 0 2
password 7 0822455DUALE130308
login local
cranspors inpuc ssh

line vey 3 4
no login

Line vey 5 15
no login
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