Basic river mapping using the “tape off-set method”

· Establish a base line and note its compass bearing.
· Establish perpendiculars and measure distance to both banks.
· The number of perpendiculars will determine the accuracy of your drawing afterwards.
· Using the “dumpy” level, work-out the cross-sectional area of at least 4 sections.
· At each section students will study the substrate looking for size (texture) and angularity (or roundness)
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