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S1(config)# vlan vian_id

S1(config-vlan)# name vian_name

S1(config)# end Activy Resuts Time Elapsed: 022349
S1(config)# config terminal

S1(config)# interface interface_id
S1(config-if)# switchport mode access You did not complete the activity. Please close this window and try again.

S1(config-if)# suitchport access vlan vian_id OverallFeedback _ Assessment tems  Connectivty Tests
NOTE [ExpandiColapse Al |Show Incorrect tems| Seore 280100
Physical  Config _CLL_ Alrbutes tem Count 26
‘The SV for VLAN 99 will not appear as “up/up” until VLAN 99 is created, ‘Assessment tems. 7 [status Points Component(s) | Feedback s
the IP adaress assigned to the SV, the no shutdown command entered, 105 Commend ) ok Component ltemsfTotal  Score.
and either (1) a device is connected to an access port associated with =t orce 0 Other » 1809 1829
'VLAN 99 (not a best practice) or (2) a trunk link (covered in the VLAN = Ports. 0 Other Other 21 821
chapter) connects to another network device such as a switch = Fastetemeto o Otner Prysical e one
cess RETURN to get starsed. "o DHCP clent enabe Correct 1 ® =
Step 2. Configure the Default Gateway. Fress 2 = “ £ Haz: DHCP o otner oo o
& Poris o Other
« The switch should be configured with a default gateway f the switch will = FastEinemeto H Other
be managed remtely from networks not directly connected. The default 7o OHCP cient enaee Correct 1 »
gateway is the first Layer 3 device (such as a router) on the same & Het: 192.168.1.1124 0 Other
management VLAN network to which the switch connects. The switch & Ports o Other
will forward IP packets with estination IP addresses outside the local = Fastetemeto o Otner
NEWOrk 10 the default gateway. AS shown in Table 2-3 and Figure 2-5, o Padiress Comect 1 ®
R1 s the default gateway for S1. The interface on R1 connected to the 5 Hez DHCP o Otrer
switch has IP address 172.17.99.1. This address Is the default gateway & Poris o Other
address for S1 5 FastEthemeto o Otner
o DHCP clent enabe Correct 1 ®
Table 2-3 Commands to Configure a Switch Default Gateway Bushorized psexs oniyt - Rat
X Bamerom ncorrect 1 Otner
s = Console Line 0 Otrer
Enter global configuration mode. 514 configure terminal Selsconti « o gogsing Syneh neerreet ! Prysical
Enter configurstion comands, one 1= DHCP Server
9 (Bt ‘Excluded Addresses
el (config) taesaulc-gatevay 152,160 e ri10 oot \ i
Configure the switch default S1(config)# ip default-gateuay -
» Invalid inpue devacved ab *=* marid X 152168101 192.168.10.10 Incorrect 1 ®
gateway. 172.17.99.1 & Pocs
Sel(confi) ¢ip defaulc-gatevay 152.1 & PoolC2
Ret leged EXEC mod 1 d Sellcentigs X DefautGateway Incorrect 1 ®
um to privilege mode.  S1(config)# en Ux Name Incarrest 4 v
CireFS t ext CLi focus & Poollid
X NS senver ncorrect 1 ®
Save the running config to the S1¢ copy running-config startup-
startup conf. config
Owp
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Figure 2-5 Configuring the Switch Default Gateway

« To configure the default gateway for the switch, use the ip default-
gateway command. Enter the IP adaress of the default gateway. The
default gateway is the IP address of the fouter interface to which the
switch connects. Use the following command to backup the
configuration: copy running-config startup-config
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