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	Steel Purlins
(Division) – based on 1800mm centres

With the Ridge length at 51.70m, we will require more than the 15no worked out. Basing the steel purlins on 10m lengths (can be comfortably manufactured to this length), we will require the following:
Division
Multiply

78no Steel Purlins required.

Rafters (steel)

No detail received showing the rafter spacing, therefore, have based this on the pillar spacing shown on the elevation drawings.

Spacing between are as follows:

4922mm – 1nr

3055mm – 1nr

5410mm – 6nr

9nr pillars each side

Providing steel rafters can be made in 13m lengths.
Roof Trusses

Again, based on the same details is the Rafters due to lack of detail.
Building width – 21.00m

If Steel Trusses can’t be used at this length, we will require more based on the length of each truss.

(NA to the proposed UWTSD Library as trusses are not required).
	
	
	
	



UWTSD Library – Roof Structure









