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Package L = PLCC

 

P = PDIP (standard plastic package)

 

SO = SOIC (small outline IC)

 

PQ = MQFP

 

JW = Windowed device (CERDIP)
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PART No.    

–

XX 

   

 

X  

 

/XX

 



Package L = PLCC


P = PDIP (standard plastic package)


SO = SOIC (small outline IC)


PQ = MQFP


JW = Windowed device (CERDIP)





Temperature Range	- = 0°C to +70°C


			I =  -40°C to +85°C


			E =  -40°C to +125°C





Frequency range	04 = 4MHz


			10 = 10MHz


			20 = 20MHz





Device, i.e. 16C711
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