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TASK I
1. From your previous lab (Lab 1 OSPF), DESIGN your own security policy for the networks in Area 1 and Area 2.
2. State the reason for your design. 
a. Eg: Restrict Emp network to reach the MGM network
b. Eg: Restrict MGM1 only to access ISP 
c. Etc.
d. (Note: You shall also add new devices like FTP Servers, Web Servers etc and set your access controls. Tips: Use the network 192.168.30.0/24 as it previously does not have any host machines)
3. Write down the ACL’s for your design
4. Implement them in the Topology
5. Test the ACL’s if it works as expected 
[image: ]
TASK II
Topology
[image: ]
Addressing Table
	Device
	Interface
	IP Address
	Subnet Mask 
	Default Gateway

	R1
	G0/0/1
	N/A
	N/A
	N/A

	R1
	G0/0/1.20
	10.20.0.1
	255.255.255.0
	N/A

	R1
	G0/0/1.30
	10.30.0.1
	255.255.255.0
	N/A

	R1
	G0/0/1.40
	10.40.0.1
	255.255.255.0
	N/A

	R1
	G0/0/1.1000
	N/A
	N/A
	N/A

	R1
	Loopback1
	172.16.1.1
	255.255.255.0
	N/A

	R2
	G0/0/1
	10.20.0.4
	255.255.255.0
	N/A

	S1
	VLAN 20
	10.20.0.2
	255.255.255.0
	10.20.0.1

	S2
	VLAN 20
	10.20.0.3
	255.255.255.0
	10.20.0.1

	PC-A
	NIC
	10.30.0.10
	255.255.255.0
	10.30.0.1

	PC-B
	NIC
	10.40.0.10
	255.255.255.0
	10.40.0.1


VLAN Table
	VLAN
	Name
	Interface Assigned

	20
	Management
	S2:  F0/5

	30
	Operations
	S1:  F0/6

	40
	Sales
	S2:  F0/18

	999
	ParkingLot
	S1:  F0/2-4, F0/7-24, G0/1-2
S2:  F0/2-4, F0/6-17, F0/19-24, G0/1-2

	1000
	Native
	N/A


Objectives
Part 1: Build the Network and Configure Basic Device Settings
Part 2: Configure and Verify Extended Access Control Lists
Instructions
Build the Network and Configure Basic Device Settings.
Design the network as shown in the topology.
Configure basic settings for each router.
Assign a device name to the router.
Disable DNS lookup to prevent the router from attempting to translate incorrectly entered commands as though they were host names.
Assign class as the privileged EXEC encrypted password.
Assign cisco as the console password and enable login.
Assign cisco as the VTY password and enable login.
Encrypt the plaintext passwords.
Create a banner that warns anyone accessing the device that unauthorized access is prohibited.
Save the running configuration to the startup configuration file.
Configure basic settings for each switch.
Assign a device name to the switch.
Disable DNS lookup to prevent the router from attempting to translate incorrectly entered commands as though they were host names.
Assign class as the privileged EXEC encrypted password.
Assign cisco as the console password and enable login.
Assign cisco as the VTY password and enable login.
Encrypt the plaintext passwords.
Create a banner that warns anyone accessing the device that unauthorized access is prohibited.
Save the running configuration to the startup configuration file.
Create VLANs on both switches.
Create and name the required VLANs on each switch from the table above.
Configure the management interface and default gateway on each switch using the IP address information in the Addressing Table. 
Assign all unused ports on the switch to the Parking Lot VLAN, configure them for static access mode, and administratively deactivate them.
Note: The interface range command is helpful to accomplish this task with as few commands as necessary.
Assign VLANs to the correct switch interfaces.
Assign used ports to the appropriate VLAN (specified in the VLAN table above) and configure them for static access mode.
Issue the show vlan brief command and verify that the VLANs are assigned to the correct interfaces.
Manually configure trunk interface F0/1.
Change the switchport mode on interface F0/1 to force trunking. Make sure to do this on both switches.
As a part of the trunk configuration, set the native vlan to 1000 on both switches. You may see error messages temporarily while the two interfaces are configured for different native VLANs.
As another part of trunk configuration, specify that VLANs 10, 20, 30, and 1000 are allowed to cross the trunk.
Issue the show interfaces trunk command to verify trunking ports, the Native VLAN and allowed VLANs across the trunk.
Manually configure S1’s trunk interface F0/5.
Configure S1’s interface F0/5 with the same trunk parameters as F0/1. This is the trunk to the router.
Save the running configuration to the startup configuration file.
Issue the show interfaces trunk command to verify trunking.
Configure Inter-VLAN Routing on R1.
Activate interface G0/0/1 on the router.
Configure sub-interfaces for each VLAN as specified in the IP addressing table. All sub-interfaces use 802.1Q encapsulation. Ensure the sub-interface for the native VLAN does not have an IP address assigned. Include a description for each sub-interface.
Configure interface Loopback 1 on R1 with addressing from the table above.
Use the show ip interface brief command to verify the sub-interfaces are operational.
Configure the R2 interface g0/0/1 using the address from the table and a default route with the next hop 10.20.0.1
Configure all network devices for basic SSH support.
Create a local user with the username SSHadmin and the encrypted password $cisco123!
Use ccna-lab.com as the domain name.
Generate crypto keys using a 1024-bit modulus.
Configure the first five VTY lines on each device to support SSH connections only and to authenticate to the local user database.
Enable secure, authenticated web services on R1.
Enable the HTTPS server on R1.
R1(config)# ip http secure-server
Configure R1 to authenticate users attempting to connect to the web server.
R1(config)# ip http authentication local
Configure PC hosts.
Refer to the Addressing Table for PC host address information.
Complete the following tests. All should be successful.
Note: You may have to disable the PC firewall for pings to be successful.
	From
	Protocol
	Destination

	PC-A
	Ping
	10.40.0.10

	PC-A
	Ping
	10.20.0.1

	PC-B
	Ping
	10.30.0.10

	PC-B
	Ping
	10.20.0.1

	PC-B
	Ping
	172.16.1.1

	PC-B
	HTTPS
	10.20.0.1

	PC-B
	HTTPS
	172.16.1.1

	PC-B
	SSH
	10.20.0.1

	PC-B
	SSH
	172.16.1.1


Configure and Verify Extended Access Control Lists.
When basic connectivity is verified, the company requires the following security policies to be implemented:
Policy 1: The Sales Network is not allowed to SSH to the Management Network (but other SSH is allowed).
Policy 2: The Sales Network is not allowed to access IP addresses in the Management network using any web protocol (HTTP/HTTPS). The Sales Network is also not allowed to access R1 interfaces using any web protocol. All other web traffic is allowed (note – Sales can access the Loopback 1 interface on R1).
Policy 3: The Sales Network is not allowed to send ICMP echo-requests to the Operations or Management Networks. ICMP echo requests to other destinations are allowed.
Policy 4: The Operations network is not allowed to send ICMP echo-requests to the Sales network. ICMP echo requests to other destinations are allowed.
Analyze the network and the security policy requirements to plan ACL implementation.
Develop and apply extended access lists that will meet the security policy statements.
Verify security policies are being enforced by the deployed access lists.
Run the following tests. The expected results are shown in the table:
	From
	Protocol
	Destination
	Result

	PC-A
	Ping
	10.40.0.10
	Fail

	PC-A
	Ping
	10.20.0.1
	Success

	PC-B
	Ping
	10.30.0.10
	Fail

	PC-B
	Ping
	10.20.0.1
	Fail

	PC-B
	Ping
	172.16.1.1
	Success

	PC-B
	HTTPS
	10.20.0.1
	Fail

	PC-B
	HTTPS
	172.16.1.1
	Success

	PC-B
	SSH
	10.20.0.4
	Fail

	PC-B
	SSH
	172.16.1.1
	Success


End of document

Record your Observations on this Lab (Both Task I & II)
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