Scope of Works for Dry Lining Subcontractor
Project: [Project Name]
Location: [Project Location]
Date: [Insert Date]

1. Overview
The dry lining subcontractor is responsible for supplying and installing partitions, ceilings, linings, and associated works as per project specifications. All work must comply with UK regulations and relevant British Standards.
2. Key Responsibilities
· Partitions & Wall Linings: Install metal stud partitions, plasterboard, acoustic insulation, and fire-rated partitions.
· Ceilings: Install suspended ceilings (metal grid and plasterboard) including acoustic-rated ceilings.
· Fire & Acoustic Barriers: Ensure fire-rated and acoustic systems are installed with appropriate fire stopping.
· Taping & Jointing: Complete jointing and finishing for a smooth, paint-ready surface.
· Doors, Windows, & Openings: Form and finish openings to specified tolerances.
· M&E Coordination: Collaborate with M&E trades, ensuring correct penetrations and fire stopping.
3. Materials & Standards
· Plasterboard: BS EN 520 compliant.
· Metal Studs: BS 7364 compliant.
· Fire & Acoustic Performance: Meet BS 476 and Building Regulations Part E standards.
4. Health & Safety
· Adhere to CDM Regulations and provide site-specific RAMS.
· Ensure workers are appropriately certified (CSCS cards).
5. Programme & Coordination
· Provide a detailed work schedule in line with the main contractor’s programme.
· Report progress regularly and communicate delays immediately.
6. Quality Assurance
· Comply with the main contractor’s QA procedures, ensuring high-quality workmanship.
· Conduct inspections and rectify defects as needed.
7. Site Management
· Manage material deliveries and site cleanliness.
· Follow site security and waste management protocols.
8. Payment Terms
· Payments will be made per the contract schedule, based on completed and approved work. Variations must be agreed upon in writing.
9. Exclusions
· Final painting and decoration.
· M&E installations, except for coordination and penetrations.

