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Introduction:

The purpose of this method statement is to explain the general procedures for the work involved in the construction and installation of piers & pile caps within the scheme.

Location

As per setting out drawing.

Programme

The element of works detailed in this Method Statement will commence on 06/05/2021 

Working hours are predominantly Monday – Friday 07:30 until 17:00.

Constraints

Constraints are:
· Live railway lines
· Permit to dig system implemented and followed.


Permits

The following permits must be in place before the work commences:


	Permit Requirement
	Yes
	No

	Permit to Work
	X
	

	Permit to Dig / Break Ground
	
	X

	Permit to Pump
	X
	

	Hot Work Permit
	
	X

	Confined Space Permit
	
	X

	Permit to Pump Concrete
	X
	

	Permit to load / dismantle (temporary works)
	X
	










Responsibilities:

The site team consist of the following people

	Name
	Position
	Emergency contact No.

	
Robert Davies

	
Contracts Manager
	
07777777777

	
Lee Davies
	
Project Manager
	
07777777778

	
Neil Williams
	
Site Agent
	
07777777779

	
Darrel Jones
	
Site Engineer

	
07755678940

	
Phil Brookes

	
Works Manager

	
07774444389



In addition to this, the task will involve the following:

· Workforce
· 1 Foreman
· 7 Operatives


Method/Procedure:

Prior to commencing the works:
· All personnel will undertake the New site induction with Covid-19 updates & be briefed on & understood the Social Distancing on Construction Sites Risk Assessment.
· Evaluate the requirement for a specific Method Statement.
· Provide toolbox method explanation to all employees associated with the works.
· Confirm train movements arrangements with Network Rail and phase the work accordingly.
· Obtain permit to pump (if necessary)
· Obtain permit to pump concrete (if necessary)
· Obtain permit to load
· Provide required PPE to all operatives on site.






· 2 metres Social Distancing to be maintained at all times due to current Covid-19 legislation
· Adequate signage and guarding of works areas, to be maintained as necessary.

Hold Point – Works Supervisor to inspect base of excavation.
On completion of the piling, the works to the concrete support piers may begin following the description and sequence as detailed below.
· Blinding concrete to formation around piles.
· On completion of the blinding, the site engineer shall set out the position of the piers.
· On completion of setting out works the installation of the reinforcing steel for the pile caps shall commence.
· On completion of the fixing of the reinforcing steel, carpenters may commence shuttering the pile cap.
· On completion of the shuttering concrete shall then be poured to the required level.
· Concrete will be delivered to site by the designated supplier’s concrete mixer wagon. Concrete mixer will discharge concrete into the concrete pump.
NOTE: All deliveries must be accompanied by the sites designated banksman.
· A vibration poker shall be used routinely throughout the pour to ensure no air is trapped within the concrete.
· On sufficient curing of the concrete, steel fixing may commence for the main pier having removed the shutters.
· Reinforcement bars will be fixed to the starter bars protruding from the pile cap.
· Pre formed shutters shall then be positioned for the main body of the piers
· On completion of the shuttering concrete shall then be poured to the required level.
· Concrete will be delivered to site by the designated supplier’s concrete mixer wagon. Concrete mixer will discharge concrete into the concrete pump.
NOTE: All deliveries must be accompanied by the sites designated banksman.
· A vibration poker shall be used routinely throughout the pour to ensure no air is trapped within the concrete.
· On sufficient curing of the concrete, removal of the shutters may take place.





Environmental Considerations:

· All plant and equipment to be in good working order and free of defects / leaks. Any defect or leaks found must be corrected prior to commencing / re-commencing works.
· Where possible plant to be equipped with bio oil.
· Static plant to be sited on suitable drip trays.
· Spill kits to be at hand at all times.
· Emergency response plan to be implemented should there be an incident.
· Noise level shall be minimised where possible and within the site working hours.
· Refuelling of plant to be carried out in accordance with the approved procedures and not near any watercourses.
· Any cutting of bituminous material (tarmac) Concrete or natural stone paving shall only be “wet” cut – water bottle attachment to disc cutter or reservoir on road saw.
· Debris netting to be secured to herras fencing where required / feasible.



COSHH:

Refer to main COSHH assessment file in site office for daily use materials


Specific Requirements for Risk Assessment/main hazards

· Excavations
· Working area
· Existing Services
· Use of hand-held small tools
· Transportation of materials
· Compaction of fill

Personal Protective Equipment Requirements

The PPE that must be for this activity are as per the site induction listed below
· Hard hat.
· Safety footwear.
· High visibility clothing. (incl. trousers and long sleeves)
· Gloves
· Safety Glasses
· Dust mask

Plant 

Plant associated with this activity.
· 1x Concrete pump
· 1x Compressor
· 3 x Poker Vibrator
· Fencing / Barriers / Signage
· Van / pick-up
· Small Tools



Emergency Arrangements

All incidents and accidents must be reported to the Site Management team as soon as possible. Accidents will be recorded in the site accident book
First aid will be administered on site by one of the site team’s first aiders.
If required Emergency assistance will be summoned by calling “999”
The nearest 24hr A&E Hospital is:
Neath Port Talbot Hospital
	Type of Hospital:
	Major acute 
Minor A&E - Open 24 hours

	Address:
	Neath Port Talbot Hospital, 
Baglan Way, 
Port Talbot, 
SA12 7BX.  

	Telephone:
	01639 862 000

	
	






Quality

Quality of the concrete will be sent away for testing. 

Waste Management

There are segregated waste skips labelled in the site compound.
Waste associated with this task will be treated in a controlled manner. A suitable location will be required for any surplus concrete.


Distribution of Information

As listed on the front page of the document.
All communication to the workforce will be verified via a method statement communication sheet attached to this document.
Welfare

Main compound as detailed in the overall Project Plan will be provided.

Change Management

Should any changes be required to this document, then they need to be approved before commencing by the Project Manager, Agent or Works Manager.
Changes can be made in hand to the document but must be signed for.



Appendices:

Appendix A	           Risk Assessments.
Appendix B              Site plan of Works area
Appendix C              COSHH
Appendix D              Method Statement Acceptance Form
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	Date:
	Signature:
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	KEY:
	L	=	Likelihood
	S	=	Severity
	R	=	Risk (Likelihood x Severity)

	RISK RANKING:
	3= Likely
2= Possible
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2= Major Injury
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	1 to 2  = Acceptable – Use basic control measures (PPE,supervision,tool box talks)
3 to 6 = Significant Risks, further control measures to be applied to reduce results                                                                                                  to Acceptable
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	Ref No
	Task/Element
	Potential Hazards
	Population at Risk

	Risk Rating
	Control Measures Specified
	Revised Risk Ranking

	1
	Placing of concrete
	Concrete splashes and possible burns.
	Employees
Ecology
	3
	2
	6
	Suitable PPE provided and to be worn including gloves and safety glasses while working with concrete.
Competent and experienced operatives to carry out operations in a controlled manner.
Supervision to be provided, as necessary.
Any spillage to be cleaned up immediately.
Concrete washout and surplus concrete to be placed in the designated area.
	1
	2
	2
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	Ref No
	Task/Element
	Potential Hazards
	Population at Risk

	Risk Rating
	Control Measures Specified
	Revised Risk Ranking

	
2
	
Working area
	
Trips and falls

	
Employees
Visitors
	
3
	
3
	
9
	All working areas to be kept free of debris where possible with surplus tools and materials removed.
Only those involved in the working operations to be within the area.
Provide suitable fencing, signing and guarding to the working area as necessary.


	
2
	
3
	
6

	
3
	
Services

	
Existing services may be present and overhead power lines
	
Employees
	
3
	
3
	
9
	
All known services shall be located prior to commencing operations where possible. 
Area shall be CAT scanned, with permit to dig issued.
Overhead cable goalposts to erected and maintained throughout operations as necessary.
NO MECHANICAL EXCAVATION WITHIN 500MM OF KNOWN SERIVCES
	
2
	
3
	
6
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	Ref No
	Task/Element
	Potential Hazards
	Population at Risk

	Risk Rating
	Control Measures Specified
	Revised Risk Ranking

	
	
	
	
	L
	S
	R
	
	L
	S
	R

	4
	Live railway line
	Passing rail striking persons, plant, or materials.

	Employees

	3
	3
	9
	Ensure safe route to working areas is identified. Safe system of work to be implemented. Due care and attention. Make enquiries to network rail as to when the railway siding is in use. Alert operatives to stop work when trains pass.
	2
	3
	6

	5
	Use of hand-held small tools, electric and fuel driven power tools.
	Cuts, bruises and airborne dusts

	Employees

	3
	2
	6
	All employees to be trained in use of relevant tools (i.e. Abrasive wheels etc.
PPE to be provided and worn including goggles and dust masks suitable for the operations.
Where possible operation to be carried out in open, ventilated environment (i.e. above ground)
Bed and surround materials will be offloaded in a suitable area and transported as required, with operatives maintaining a suitable distance while deposition takes place.

	2
	2
	4
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	Ref No
	Task/Element
	Potential Hazards
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	L
	S
	R
	
	L
	S
	R

	6
	Transportation of Material
	Moving Plant


	Employees
Visitors
	3

	3

	9

	All plant to be operated by trained and competent personnel only.
All plant to be checked on arrival to site and to hold all necessary test certificates.
All plant to be fitted with warning lights on top of their vehicle.
All mandatory PPE to be worn by operatives.

Licensed vehicles to be used when using the public highway.
Public highway to be kept clean at all times – sweeper.

	1

	3

	3
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	L
	S
	R
	
	L
	S
	R

	7
	
Coronavirus-Covid-19









	
Interaction when working. 
Higher risk from COVID-19 exposure when in close proximity











	
Site based workers – both AG staff, contractors & members of the public




	
3














	
3














	
9













	· Plan all work to minimise any contact between workers and activities requiring interaction within 2m. If you have to work within 2 metres, please stop work & inform your supervisor so another work method can be implemented or Risk assessment can be carried out
· Single use PPE to be disposed in bags in general waste so that it cannot be reused.
· Mandatory PPE to be cleaned in line with Public Health England after use.
maintain the strict cleaning a hygiene controls on each site.
Appointed COVID-19 Marshalls to be allocated to projects still working to ensure that social distancing control methods are policed and maintained. Covid-19 Warning Signs to be placed on perimeter fencing
	
1














	
3










	
3
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Plan of Works Area












Appendix C

COSHH


See main file
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MAX AARON (CONTRACTORS) LTD.

BAGLAN LINK BRIDGE AND ROAD



       METHOD STATEMENT EXPLANATION FORM

	Method statement
	Construction of the Piers & Pile Caps

	Method Statement No.
	MS 03 Rev 01

	Date of explanation
	

	Explanation given by
	

	Topics covered:
	Method statement explanation including toolbox talks on:







	No.
	Attendee 
	Signature
	No.
	Attendee 
	Signature

	1
	
	
	14
	
	

	2
	
	
	15
	
	

	3
	
	
	16
	
	

	4
	
	
	17
	
	

	5
	
	
	18
	
	

	6
	
	
	19
	
	

	7
	
	
	20
	
	

	8
	
	
	21
	
	

	9
	
	
	22
	
	

	10
	
	
	23
	
	

	11
	
	
	24
	
	

	12
	
	
	25
	
	

	13
	
	
	26
	
	



Signature of person giving explanation:  ………………………………………………

Signature of attendee confirms understanding of explanation given
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