Session 6: engine disassembly and measuring
Instructor: Barry 
Date: 31/10/19
Aim: To disassemble the engine with aspirations to remove the cylinder head.
Health and safety: All PPE mentioned in the first logbook entry must be warn before entering the workshop. Barrier cream should be applied on entry.
All safety procedures spoken about in session one entry must be followed throughout the workshop session.
Equipment
· 8mm ratchet set
· 10 mm ratchet set
· Breaker bar 
· 8mm spanner 
· 10 mm spanner 
Method
· Firstly, remove the spark plug leads, followed by the removal of the rocker cover. An 8mm rachet with an 8mm attachment is used for this.
· Then, using the rachet again, remove the fuel rail from the side of the cylinder head
· Next, move the exhaust manifold, there should be six 8 mm screws.
· Then remove the cam gear covers from the side of the block 
· Remove the cam belt 
· Remove all other components on the outside of the block and cylinder head.
[bookmark: _GoBack]Evaluation:
· This was a very successful session; the aim was achieved, and it was all carried out with no issues as well as no injuries. the success of the session shows that all procedures, both safety and carrying out the task were completed correctly.
· The aim of this session was accomplished efficiently with no issues or injuries. The success of this session demonstrates that all procedures were carried out accurately, including ensuring the follow the health and safety guidelines.


