Switch S1 Configurations
Unauthorised Access Is Strictly Prohibited 

User Access Verification

Password: 
[bookmark: _GoBack]S1> en
Password: 
S1#show running-config
Building configuration...

Current configuration : 1640 bytes
!
! Last configuration change at 11:13:04 UTC Tue Mar 27 2018
!
version 12.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
enable secret 5 $1$a0z1$W2.bQy.slbpSjqeRZEWkv.
!
!
!
no aaa new-model
switch 1 provision ws-c3750-24p
system mtu routing 1500
 --More--         no ip domain-lookup
!
!
!
!
!
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
interface FastEthernet1/0/1
!
interface FastEthernet1/0/2
!
interface FastEthernet1/0/3
!
 --More--         interface FastEthernet1/0/4
!
interface FastEthernet1/0/5
!
interface FastEthernet1/0/6
!
interface FastEthernet1/0/7
!
interface FastEthernet1/0/8
!
interface FastEthernet1/0/9
!
interface FastEthernet1/0/10
!
interface FastEthernet1/0/11
!
interface FastEthernet1/0/12
!
interface FastEthernet1/0/13
!
interface FastEthernet1/0/14
!
interface FastEthernet1/0/15
 --More--         !
interface FastEthernet1/0/16
!
interface FastEthernet1/0/17
!
interface FastEthernet1/0/18
!
interface FastEthernet1/0/19
!
interface FastEthernet1/0/20
!
interface FastEthernet1/0/21
!
interface FastEthernet1/0/22
!
interface FastEthernet1/0/23
!
interface FastEthernet1/0/24
!
interface GigabitEthernet1/0/1
!
interface GigabitEthernet1/0/2
!
 --More--         interface Vlan1
 ip address 172.16.2.2 255.255.255.192
!
ip default-gateway 172.16.2.1
ip classless
ip http server
ip http secure-server
!
!
!
!
banner motd ^C
Unauthorised Access Is Strictly Prohibited ^C
!
line con 0
 password 7 14141B180F0B
 login
line vty 0 4
 password 7 14141B180F0B
 login
line vty 5 15
 login
!
 --More--         end

S1#show ip interface brief
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  172.16.2.2      YES manual up                    up      
FastEthernet1/0/1      unassigned      YES unset  up                    up      
FastEthernet1/0/2      unassigned      YES unset  down                  down    
FastEthernet1/0/3      unassigned      YES unset  down                  down    
FastEthernet1/0/4      unassigned      YES unset  down                  down    
FastEthernet1/0/5      unassigned      YES unset  down                  down    
FastEthernet1/0/6      unassigned      YES unset  up                    up      
FastEthernet1/0/7      unassigned      YES unset  down                  down    
FastEthernet1/0/8      unassigned      YES unset  down                  down    
FastEthernet1/0/9      unassigned      YES unset  down                  down    
FastEthernet1/0/10     unassigned      YES unset  down                  down    
FastEthernet1/0/11     unassigned      YES unset  down                  down    
FastEthernet1/0/12     unassigned      YES unset  down                  down    
FastEthernet1/0/13     unassigned      YES unset  down                  down    
FastEthernet1/0/14     unassigned      YES unset  down                  down    
FastEthernet1/0/15     unassigned      YES unset  down                  down    
FastEthernet1/0/16     unassigned      YES unset  down                  down    
FastEthernet1/0/17     unassigned      YES unset  down                  down    
FastEthernet1/0/18     unassigned      YES unset  down                  down    
FastEthernet1/0/19     unassigned      YES unset  down                  down    
FastEthernet1/0/20     unassigned      YES unset  down                  down    
FastEthernet1/0/21     unassigned      YES unset  down                  down    
 --More--         FastEthernet1/0/22     unassigned      YES unset  down                  down    
FastEthernet1/0/23     unassigned      YES unset  down                  down    
FastEthernet1/0/24     unassigned      YES unset  down                  down    
GigabitEthernet1/0/1   unassigned      YES unset  down                  down    
GigabitEthernet1/0/2   unassigned      YES unset  down                  down    

S1#show ip route
Default gateway is 172.16.2.1

Host               Gateway           Last Use    Total Uses  Interface
ICMP redirect cache is empty
S1#
