Switch AS1
AS1#sh run
Building configuration...

Current configuration : 1889 bytes
!
version 12.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname AS1
!
boot-start-marker
boot-end-marker
!
!
!
!
no aaa new-model
system mtu routing 1500
!
!
!
!
!
!
!
!
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
spanning-tree vlan 1,10,99 priority 28672
!
vlan internal allocation policy ascending
!
!
!
interface FastEthernet0/1
 switchport access vlan 99
 switchport mode access
!
interface FastEthernet0/2
 switchport access vlan 99
 switchport mode access
!
interface FastEthernet0/3
 switchport access vlan 99
 switchport mode access
!
interface FastEthernet0/4
 switchport access vlan 99
 switchport mode access
!
interface FastEthernet0/5
 switchport access vlan 99
 switchport mode access
!
interface FastEthernet0/6
 switchport access vlan 10
 switchport trunk native vlan 99
 switchport mode trunk
 spanning-tree portfast
 spanning-tree bpduguard enable
!
interface FastEthernet0/7
!
interface FastEthernet0/8
!
interface FastEthernet0/9
!
interface FastEthernet0/10
 --More--
interface FastEthernet0/11
!
interface FastEthernet0/12
!
interface FastEthernet0/13
!
interface FastEthernet0/14
!
interface FastEthernet0/15
!
interface FastEthernet0/16
!
interface FastEthernet0/17
!
interface FastEthernet0/18
!
interface FastEthernet0/19
!
interface FastEthernet0/20
!
interface FastEthernet0/21
!
interface FastEthernet0/22
!
interface FastEthernet0/23
!
interface FastEthernet0/24
!
interface GigabitEthernet0/1
!
interface GigabitEthernet0/2
!
interface Vlan1
 no ip address
!
interface Vlan10
 ip address 192.168.10.1 255.255.255.0
!
interface Vlan20
 ip address 192.168.20.1 255.255.255.0
!
interface Vlan30
 ip address 192.168.30.1 255.255.255.0
!
interface Vlan99
 ip address 192.168.99.1 255.255.255.252
!
ip http server
ip http secure-server
!
line con 0
line vty 5 15
!
End

AS1#SH IP INT BRIEF
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  up                    down
Vlan10                 192.168.10.1    YES manual up                    down
Vlan20                 192.168.20.1    YES manual up                    down
Vlan30                 192.168.30.1    YES manual up                    down
Vlan99                 192.168.99.1    YES manual up                    up
FastEthernet0/1        unassigned      YES unset  up                    up
FastEthernet0/2        unassigned      YES unset  up                    up
FastEthernet0/3        unassigned      YES unset  up                    up
FastEthernet0/4        unassigned      YES unset  down                  down
FastEthernet0/5        unassigned      YES unset  down                  down
FastEthernet0/6        unassigned      YES unset  down                  down
FastEthernet0/7        unassigned      YES unset  down                  down
FastEthernet0/8        unassigned      YES unset  down                  down
FastEthernet0/9        unassigned      YES unset  down                  down
FastEthernet0/10       unassigned      YES unset  down                  down
FastEthernet0/11       unassigned      YES unset  down                  down
FastEthernet0/12       unassigned      YES unset  down                  down
FastEthernet0/13       unassigned      YES unset  down                  down
FastEthernet0/14       unassigned      YES unset  down                  down
FastEthernet0/15       unassigned      YES unset  down                  down
FastEthernet0/16       unassigned      YES unset  down                  down
FastEthernet0/17       unassigned      YES unset  down                  down
FastEthernet0/18       unassigned      YES unset  down                  down
FastEthernet0/19       unassigned      YES unset  down                  down
FastEthernet0/20       unassigned      YES unset  down                  down
FastEthernet0/21       unassigned      YES unset  down                  down
FastEthernet0/22       unassigned      YES unset  down                  down
FastEthernet0/23       unassigned      YES unset  down                  dow
FastEthernet0/24       unassigned      YES unset  down                  down
GigabitEthernet0/1     unassigned      YES unset  down                  down
GigabitEthernet0/2     unassigned      YES unset  down                  down

AS1#sh vlan

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active    Fa0/7, Fa0/8, Fa0/9, Fa0/10
                                                Fa0/11, Fa0/12, Fa0/13, Fa0/14
                                                Fa0/15, Fa0/16, Fa0/17, Fa0/18
                                                Fa0/19, Fa0/20, Fa0/21, Fa0/22
                                                Fa0/23, Fa0/24, Gi0/1, Gi0/2
10   Student                          active    Fa0/6
20   Staff                            active
30   Guest                            active
99   VLAN0099                         active    Fa0/1, Fa0/2, Fa0/3, Fa0/4
                                                Fa0/5
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup

VLAN Type  SAID       MTU   Parent RingNo BridgeNo Stp  BrdgMode Trans1 Trans2
---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------
1    enet  100001     1500  -      -      -        -    -        0      0
10   enet  100010     1500  -      -      -        -    -        0      0
20   enet  100020     1500  -      -      -        -    -        0      0

VLAN Type  SAID       MTU   Parent RingNo BridgeNo Stp  BrdgMode Trans1 Trans2
---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------
30   enet  100030     1500  -      -      -        -    -        0      0
99   enet  100099     1500  -      -      -        -    -        0      0
1002 fddi  101002     1500  -      -      -        -    -        0      0
1003 tr    101003     1500  -      -      -        -    srb      0      0
1004 fdnet 101004     1500  -      -      -        ieee -        0      0
1005 trnet 101005     1500  -      -      -        ibm  -        0      0

Remote SPAN VLANs
------------------------------------------------------------------------------


Primary Secondary Type              Ports
------- --------- ----------------- ------------------------------------------

AS1#sh etherchannel summary
Flags:  D - down        P - bundled in port-channel
        I - stand-alone s - suspended
        H - Hot-standby (LACP only)
        R - Layer3      S - Layer2
        U - in use      f - failed to allocate aggregator

        M - not in use, minimum links not met
        u - unsuitable for bundling
        w - waiting to be aggregated
        d - default port


Number of channel-groups in use: 3
Number of aggregators:           3
Group  Port-channel  Protocol    Ports
------+-------------+-----------+-----------------------------------------------
1      Po1(SD)          -
2      Po2(SD)          -
3      Po3(SU)         PAgP      Fa0/3(P)    Fa0/4(P)
[bookmark: _GoBack]

AS1#sh vtp status
VTP Version capable             : 1 to 3
VTP version running             : 1
VTP Domain Name                 : soac.com
VTP Pruning Mode                : Disabled
VTP Traps Generation            : Disabled
Device ID                       : 00e1.6ddb.2100
Configuration last modified by 0.0.0.0 at 3-1-93 01:28:21

Feature VLAN:
--------------
VTP Operating Mode                : Client
Maximum VLANs supported locally   : 255
Number of existing VLANs          : 9
Configuration Revision            : 0
MD5 digest                        : 0xA5 0x45 0x52 0xEC 0xD6 0x93 0x10 0x96
                                    0x8C 0xCE 0x47 0x47 0x48 0xBA 0xAF 0x40
