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Construction and Use Regulations – Tyres condition and Maintenance regulation 27

 (Scenario 7 – KINGSWAY SHOPPING CENTRE CAR PARK)

SCENARIO REQUIREMENTS

· One role actors, appropriately dressed – (as instructed by course trainers). One will play the driver.
· One officer appropriately dressed – ( as instructed by course trainers)
· Control room operator.
· Assessor to be in full possession of relevant definition regarding the offence being assessed as well as the relevant assessment criteria sheet that must be completed by the assessor during the observations.
· One vehicle to be used.
· Traffic Offence Report (TOR) ticket book.
· Tyre with the ply or cord exposed.


SAFETY REMINDER
[bookmark: _GoBack]
· Safe working environment, risk assessment to be completed of the venue.
· Assessor to have given full briefing to Role actor/s and Officers/s being assessed prior to the role play.
· If officer is to detain / arrest role actor then this will be done by the office taking hold of the role actors arm and informing them that they are being detained / arrested.
· No handcuffs are to be used, if the officer wishes to use handcuffs then they should inform the subject that they are handcuffed. Subject should place hands to the rear when informed.
· No actual UDT strikes are to be used.
· Vehicles NOT to be switched on.
· Students to be mindful of same gender searches.
· If there are any safety issues identified then the identifying officer should immediately call “CHECKMATE” to the role play and report their findings to the Assessor.
If there are no safety issues the role play will run its course and the assessor will call “END EX” once they are happy the role play has concluded.





TRAINER BRIEFING TO STUDENT(S)
You are mobile patrol near the KINGSWAY SHOPPING CENTRE CAR PARK (which is open to the public, free of charge 24 hours a day). You have caused a car to pull in to the car park as you need to speak to the driver, regarding his manner of driving.
You speak with the driver (details are the role players own), and you obtain the details and pass to the Force Control Room operator to carry out a PNC check and a Driving licence check and insurance check.
The driver’s documents are all in order.
You speak with the driver of the vehicle and check the condition of the vehicle, whilst walking around the vehicle you notice that the front offside and nearside tyres have the ply exposed.
You deal with the incident appropriately.
The time and day are current to the scenario.

The following details can be passed on to the student if they ask for further information-

· PNC shows that the driver has no previous convictions. The driver’s documents are all in order.
· There is another officer in close proximity.
· If you require any radio checks and have a radio available, use your radio to gather any further information required, the course trainer will designate someone to act as the controller.
· There is transport (theoretically).
· Deal with the incident as you see fit.
· Consider the following-
1) Officer Safety
2) Communication Skills/ ambulance requirement
3) Relevant Offences
4) Legislation and the National Decision Module (NDM).




TRAINER BRIEFING TO ROLE ACTOR

Male/female Role Actor driver.
When the police officer speaks to you, they will ask you your details. You will ask the police officer, why you have stopped me. The police officer will explain that your manner of driving was erratic. You will apologise and state that you dropped your coffee.
The police officer will check your vehicle and notice that you have the two front tyres of your car with the ply exposed. You will apologise to the police officer and state that you will get them changed.
When the police officer reports you for the offence, you will become agitated and ask why.
You have no previous convictions. You have all your driving documents in place. 
Eventually you apologise and accept the Traffic Offence Report.


Overall outcome of the scenario
· The driver of the offending vehicle should be issued with a Traffic Offence Report for the ply exposed on both front tyres, using the correct legislation.
· NDM should be followed.
· Police personal procedures, radio procedures and recording of the incident in the EPNB should be carried out in line with force policy.




Scenario 7 Driving with the ply exposed on both tyres

Role Actors Script for the driver
When the police officer speaks to you, they will ask you your details. 
You will provide the police officer with your own details.
You will say to the officer;

“WHY HAVE YOU STOPPED ME?”

The police officer will explain that your manner of driving was erratic. 
You will say;

“I AM SORRY I DROPPED MY COFFEE”

The police officer will check your vehicle and notice that you have the two front tyres of your car with the ply exposed. 
You will say;
“I AM SORRY OFFICER I WILL GET THEM CHANGED”
The police officer reports you for the offence by explaining the TOR process;
 You will become agitated and say;
“WHY I’LL GET THEM CHANGED, HAVEN’T YOU GOT ANYTHING BETTER TO DO?”
You have no previous convictions. You have all your driving documents in place. 
Eventually you apologise and accept the Traffic Offence Report.
The police officer will explain that they are going to report you for the offence of driving on a road with two tyres with the ply exposed. The police officer will then explain that they will be issuing you with a Traffic Offence Report (TOR).The role actor will provide their own details.
Please follow the above script to ensure fairness to all candidates.


Construction and Use Regulations – Tyre condition and maintenance regulation 27


Regulation 27 of the Road Vehicles (Construction and Use) Regulations 1986 provides for the condition and maintenance of tyres with regard to motor vehicles and trailers.
27(1) Unless provided for in paragraphs (2), (3) and (4) below, a wheeled motor vehicle or trailer a wheel of which is fitted with a pneumatic tyre shall not be used on a road, if -
(a) the tyre is unsuitable having regard to the use to which the motor vehicle or trailer is being put or to the types of tyres fitted to its other wheels; (SEE ALSO PARAGRAPH (3) BELOW)
(b) the tyre is not so inflated as to make it fit for the use to which the motor vehicle or trailer is being put;
(c) the tyre has a cut in excess of 25 mm or 10 percent of the section width of the tyre, whichever is the greater, measured in any direction on the outside of the tyre and deep enough to reach the ply or cord;(SEE ALSO PARAGRAPH (2) BELOW)
(d) the tyre has any lump, bulge or tear caused by separation or partial failure of its structure; (SEE ALSO PARAGRAPH (2) BELOW)
(e) the tyre has any of the ply or cord exposed; (SEE ALSO PARAGRAPH (2) BELOW) 
(f) the base of any groove which showed in the original tread pattern of the tyre is not clearly visible;
(g) either
(i) the grooves of the tread pattern of the tyre do not have a depth of at least 1 mm throughout a continuous band measuring at least three-quarters of the breadth of the tread and round the entire outer circumference of the tyre; or
(ii) if the grooves of the original tread pattern of the tyre did not extend beyond three-quarters of the breadth of the tread, any groove which showed in the original tread pattern does not have a depth of at least 1 mm ( BUT 1.6mm IN MANY INSTANCES - SEE PARAGRAPHS (4)(c), (d), (e) AND (f) BELOW); or
(h) the tyre is not maintained in such condition as to be fit for the use to which the vehicle or trailer is being put or has a defect which might in any way cause damage to the surface of the road or damage to persons on or in the vehicle or to other persons using the road.
27(2) Paragraph (1) above does not prohibit the use on a road of a motor vehicle or trailer by reason only of the fact that a wheel of the vehicle or trailer is fitted with a tyre which is deflated and which has any of the defects described in sub-paragraph (c), (d) or (e) of that paragraph, if the tyre and the wheel to which it is fitted are so constructed as to make the tyre in that condition fit for the use to which the motor vehicle or trailer is being put and the outer sides of the wall of the tyre are marked enabling the tyre to be identified as having been constructed to comply with the requirements of this paragraph.

27(3) Paragraph (1)(a) does not prohibit the use on a road of a passenger vehicle (not being a bus) by reason only of the fact that a wheel of the vehicle is fitted with a temporary use spare tyre, unless the vehicle is driven at a speed exceeding 50 mph.

27(4)
(a) Paragraph (1)(a) to (g) does not apply to -
(i) an agricultural motor vehicle, not being a category T tractor, that is not driven at more than 20 mph;
(ii) an agricultural trailer ;
(iii) an agricultural trailed appliance;
(iv) a broken down vehicle or a vehicle proceeding to a place where it is to be broken up, being drawn, in either case, by a motor vehicle at a speed not exceeding 20 mph; or
(v) a category T tractor that is not driven at more than 40 km/h.
(b) Paragraph (1) (f) and (g) does not apply to:
(i) a three-wheeled motor cycle the unladen weight of which does not exceed 102 kg and which has a maximum speed of 12 mph; or
(ii) a pedestrian-controlled works truck.
(c) Paragraph (1)(g) does not apply to a motorcycle with an engine capacity which does not exceed 50 cc.
(d) Paragraph 1(f) and (g) does not apply to the vehicles specified in sub-paragraph (e) below, but such vehicles shall comply with the requirements specified in sub- paragraph (f) below.
(e) The vehicles referred to in sub-paragraph (d) above are:
(i) passenger vehicles other than motor cycles constructed or adapted to carry no more than 8 seated passengers in addition to the driver;
(ii) goods vehicles with a maximum gross weight which does not exceed 3500kg; and
(iii) light trailers not falling within (ii)above;
first used on or after 3 January 1993. 
Note:
In this regulation, in relation to a trailer, first used shall be construed as a reference to the date which is 6 months after the date of manufacture of the trailer. See the general definition of first used.
(f) The requirements referred to in sub-paragraph (d) above are that the grooves of the tread pattern of every tyre fitted to the wheels of a vehicle mentioned in sub-paragraph (e) above shall be of a depth of at least 1.6 mm throughout the continuous band comprising the central three-quarters of the breadth of tread and round the entire outer circumference of the tyre.
27(5) A recut pneumatic tyre shall not be fitted to any wheel of a motor vehicle or trailer if
(a) its ply or cord has been cut or exposed by the re- cutting process; or
(b) it has been wholly or partially re-cut in a pattern other than the manufacturer's re-cut tread pattern.
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