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Below listed are the assumptions report I have created for my take off the Fforwm building. Also, including the cost of items used in the cost plan.

Substructure
Pile foundations assumed to be double piles with a 750mm diameter and an average depth of 18 to 20 meters.
Rate to be used for piles is £150 a meter.

Upper floors
Openings for 2 number stairwells and lifts haven’t been deducted from area of concrete floors.
200mm in situ reinforced concrete upper floors rate of £115 m2. Assumed rate of Fforwm concrete floor is £140 m2 due to it being a depth of 275mm.

Stairs
2 number stairs from ground to second floor as per drawing at a rate of £22000 for one.

Roof lights
Assumed roof light opening is 3.4m x 1.6m as per drawings.
Largest roof light on Spons is 1.340m x 1400m.
Area divided and multiplied by rate of £774 to get total.

Floor Finishes
First and second floors are carpet floorings
All bathrooms have vinyl flooring.
Ground floor has a wood floor finish.

External Walls.
Aluminium wall cladding rate used £54.00 taken from spons architects 2020 page 98.
Facing brickwork rate of £180.00 m2 from spons architects 2020 from page 99.

Rainwater Goods
UPVC rainwater downpipes £21.00 a metre used from spons architects page 150.
UPVC rainwater gutters £26.00 a metre used from spons architects page 150.

Windows.
£490.00 a metre based on coated aluminium double glazed window system on page 89
£450.00 a metre based on coated aluminium double glazed curtain walling page 98. 
£1200.00 per fire escape door to the curtain walling page 98. 

Floor Finishes.
£35.00 a metre squared based on carpet tiling under floor finishes heading on page 106.
£53.00 a square meter for timber laminate flooring page 164.
£100.00 a square meter for vinyl flooring page 164.
Mechanical and Electrical Instillations. 
£530.00 a square meter to allow for mechanical and electrical services based on page 106. 

Internal Walls.
All internal walls to be assumed 140mm thick block work excluding the stair wells and lift shaft which will be incorporated within the concrete frame page 167 from spons.
Height from floor to ceiling for the internal walls 3.5m 
Decoration to walls rate used £9.00 a square meter on page 172. 
Plaster boarding fixed to walls on dabs £8.31 a meter squared on page 420.
3mm skim finish to walls based on £6.16 on page 543.
Decoration to skirting based on 1no primer coat and 2no gloss coats to skirting, rate used £11.86 per metre based on page 563.
Supply and fit of timber skirting, rate used is £16 per metre based on page 114.                    

External Frame.
Concrete frame to include all columns and beams.
Rate used £150.00 a metre squared on page 153. 

Doors
Type 1 internal door £925.00 based on rate page 164.
Type 6 internal door rate of £1550.00 based on rate page 167.
Type 2/4 internal door rate of £1125.00 based on page 167. 
Type 5/5B/5C rate prorated from internal door set rates on page 126 rate allowed within cost plan for these is £1600.00 per unit. 


1
Declan Thomas
