	Task 1 Practical Exam – IN-CLASS ASSESSMENT
Module name: Switching, Routing and Wireless
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Student ID: 2026077
1. Inter-VLAN Routing Challenge (2.5 Marks)
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1. EtherChannel Additional Activity (2.5 Marks)
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1. WLAN Additional Activity (2.5 Marks)
1. EIGRP Challenge (2.5 Marks)
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Enter configuration commands, one per line. End with CNTL/Z.
Router (config) finterface GigabitIthernetd/0.10

Rouser (config-subif) encap

Router (config-subif) fencapsulation dovlQ 10

Router (config-subif) $ip address 10.0.10.1 255.255.255.0
Router (config-subif) $interface G0/0.20

Rouser (config-subif) fen

Rouser (config-subif) fencapsulacion do

Router (config-subif) fencapsulavion dovlQ 20

Rouser (config-subif) #ip

Roucer (config-subif) #ip add

Router (config-subif) $ip address 10.0.20.1 255.255.255.0
Rouser (config-subif) fencaa

Rouser (config-subif) fencap

Router (config-subif) $interface GigabitEthernetd/0.30
Rouser (config-subif) fenca

Router (config-subif) fencapsulation dovld 30

Roucer (config-subif) #ip ad

Router (config-subif) $ip address 10.0.30.1.255.255.255.0

% Tnvalid inpuc devected av '~' marker.

Router (config-subif) $ip address 10.0.30.1.255.255.255.0

% Tnvalid inpuc devected av ' marker.

Rouer (config-supif) 8]
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M1 (config-if-range) $channel-group 1 mods desizable
M1 (conig-if-range) ¢
Creating a porc-channel interface Porc-channel 1
SLINEPROTO-5-UPDOWN: Line protocol on Interface FastEchernet0/l, changed state to down
SLINEPROTO-5-UPDOWN: Line protocol on Interface FastEchernet0/l, changed state to up
SLINEPROTO-5-UPDOWN: Line protocol on Interface FastEcherne0/2, changed state to down
SLINEPROTO-5-UPDOWN: Line protocol on Interface FastEchernet0/2, changed state ©o up
M1 (config-if-range) $switehpors mode Trunk
M1 (conig-if-range)¢
SLINEPROTO-5-UPDOWN: Line protocol on Interface FastEchernet0/L, changed state to down
SLINEPROTO-5-UPDOWN: Line protocol on Interface FastEchernet0/l, changed state to up
SEC-5-CANNOT_BUNDLEZ: FaO/L is not compatible with Fa0/2 and will be suspended (dtp mode
of Fao/1 is on, Fav/2is off )
SLINEPROTO-5-UPDOWN: Line protocol on Interface FastEchernet0/l, changed state to down
SLINEPROTO-5-UPDOWN: Line protocol on Interface FastEcherne0/2, changed state to down
SLINEPROTO-5-UPDOWN: Line protocol on Interface FastEchernet0/2, changed state ©o up
SLINEPROTO-5-UPDOWN: Line protocol on Interface FastEchernet0/l, changed state to up
M1 (config-if-range) sexic
M1 (contig) tinterface port-channel 1
M1 (config-if) swicchport mode trumk
M1 (config-if)s
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Toweer (SonFig-SwEiTTIp sddress 00 10 T 258 258 255 0
Router (config-subif) $interface G0/0.20

Rouser (config-subif) fen

Rouser (config-subif) fencapsulacion do

Router (config-subif) fencapsulavion dovlQ 20

Rouser (config-subif) #ip

Roucer (config-subif) #ip add

Router (config-subif) $ip address 10.0.20.1 255.255.255.0
Rouser (config-subif) fencaa

Rouser (config-subif) fencap

Router (config-subif) $interface GigabitEthernetd/0.30
Rouser (config-subif) fenca

Router (config-subif) fencapsulation dovld 30

Roucer (config-subif) #ip ad

Router (config-subif) $ip address 10.0.30.1.255.255.255.0

% Tnvalid inpuc devected av ' marker.

Router (config-subif) $ip address 10.0.30.1.255.255.255.0

% Tnvalid inpuc devected av ' marker.

Rouser (config-subif) gexic
Rouser (config)®
Rouser (config) finterface DovllRadiod

% Tnvalid inpuc devected av ' marker.

Rouser (config)s
Rouser (config) router eigrp 100

Router (config-router) necwork 152.165.1.0 0.0.0.255
Router (config-router) fexic

Rouser (config) router eigrp 100

Rouser (config-router) network 192.165.2.0 0.0.0.255
Rouser (config-router)
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