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Running Configs
HQ
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname HQ
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
username webuser password 0 soac1234 privilege 15
!
!
license udi pid CISCO1941/K9 sn FTX15243NAQ-
!
!
!
!
!
!
!
!
!
no ip domain-lookup
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface Loopback1
 ip address 1.1.1.1 255.255.255.255
!
interface GigabitEthernet0/0
 ip address 209.165.200.30 255.255.255.248
 duplex auto
 speed auto
 ipv6 address 2001:DB8:ACAD:1::30/64
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface Serial0/0/0
 ip address 10.10.10.2 255.255.255.252
 ipv6 address 2001:DB8:CAFE:1::2/64
 clock rate 2000000
!
interface Serial0/0/1
 ip address 10.10.4.2 255.255.255.252
 ipv6 address 2001:DB8:CAFE:2::2/64
 clock rate 2000000
!
interface Vlan1
 no ip address
 shutdown
!
router eigrp 1
 passive-interface default
 
!
router rip
 passive-interface default
 network 10.0.0.0
 network 209.165.200.0
!
ip classless
!
ip flow-export version 9
!
!
!
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
 login
!
!
!
end
Branch2
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname Branch2
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO1941/K9 sn FTX1524DSN2-
!
!
!
!
!
!
!
!
!
no ip domain-lookup
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface Loopback6
 no ip address
 ipv6 address 2001:DB8:BEEF:10::1/64
!
interface Loopback7
 no ip address
 ipv6 address 2001:DB8:CEED:10::1/64
!
interface Loopback11
 ip address 11.11.11.1 255.255.255.0
!
interface Loopback12
 ip address 12.12.12.1 255.255.255.0
!
interface Loopback13
 ip address 13.13.13.1 255.255.255.0
!
interface GigabitEthernet0/0
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface Serial0/0/0
 ip address 10.10.10.1 255.255.255.252
 ipv6 address 2001:DB8:CAFE:1::1/64
!
interface Serial0/0/1
 no ip address
 clock rate 2000000
 shutdown
!
interface Vlan1
 no ip address
 shutdown
!
router eigrp 1
 passive-interface default
 
!
router rip
 passive-interface default
 network 10.0.0.0
!
ip classless
!
ip flow-export version 9
!
!
!
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
 login
!
!
!
end
Branch1
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname Branch1
!
!
!
!
ip dhcp excluded-address 192.168.5.1 192.168.5.10
ip dhcp excluded-address 192.168.6.1 192.168.6.10
ip dhcp excluded-address 192.168.7.1 192.168.7.10
ip dhcp excluded-address 192.168.8.1 192.168.8.10
!
ip dhcp pool VLAN5
 network 192.168.5.0 255.255.255.0
 default-router 192.168.5.1
 dns-server 209.165.200.25
ip dhcp pool VLAN6
 network 192.168.6.0 255.255.255.0
 default-router 192.168.6.1
 dns-server 209.165.200.25
ip dhcp pool VLAN7
 network 192.168.7.0 255.255.255.0
 default-router 192.168.7.1
 dns-server 209.165.200.25
ip dhcp pool VLAN8
 network 192.168.8.0 255.255.255.0
 default-router 192.168.8.1
 dns-server 209.165.200.25
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO1941/K9 sn FTX1524X7N8-
!
!
!
!
!
!
!
!
!
no ip domain-lookup
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface Loopback2
 ip address 192.168.2.1 255.255.255.192
!
interface Loopback3
 ip address 192.168.2.65 255.255.255.224
!
interface Loopback4
 ip address 192.168.2.97 255.255.255.240
!
interface Loopback5
 no ip address
 ipv6 address 2001:DB8:CAFE:5::1/64
!
interface Loopback6
 no ip address
 ipv6 address 2001:DB8:CAFE:6::1/64
!
interface GigabitEthernet0/0
 no ip address
 duplex auto
 speed auto
!
interface GigabitEthernet0/0.5
 encapsulation dot1Q 5
 ip address 192.168.5.1 255.255.255.0
!
interface GigabitEthernet0/0.6
 encapsulation dot1Q 6
 ip address 192.168.6.1 255.255.255.0
!
interface GigabitEthernet0/0.7
 encapsulation dot1Q 7
 ip address 192.168.7.1 255.255.255.0
!
interface GigabitEthernet0/0.8
 encapsulation dot1Q 8
 ip address 192.168.8.1 255.255.255.0
!
interface GigabitEthernet0/0.9
 encapsulation dot1Q 9
 ip address 192.168.9.1 255.255.255.0
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface Serial0/0/0
 no ip address
 clock rate 2000000
 shutdown
!
interface Serial0/0/1
 ip address 10.10.4.1 255.255.255.252
 ipv6 address 2001:DB8:CAFE:2::1/64
!
interface Vlan1
 no ip address
 shutdown
!
router eigrp 1
 passive-interface default
 
!
router rip
 passive-interface default
 network 10.0.0.0
 network 192.168.5.0
 network 192.168.6.0
 network 192.168.7.0
 network 192.168.8.0
 network 192.168.9.0
!
ip classless
!
ip flow-export version 9
!
!
!
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
 login
!
!
!
end

S1
!
version 12.2
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname S1
!
!
!
no ip domain-lookup
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
interface FastEthernet0/1
 switchport mode trunk
!
interface FastEthernet0/2
 switchport access vlan 5
 switchport mode access
!
interface FastEthernet0/3
 switchport access vlan 5
 switchport mode access
!
interface FastEthernet0/4
 switchport access vlan 5
 switchport mode access
!
interface FastEthernet0/5
 switchport access vlan 5
 switchport mode access
!
interface FastEthernet0/6
 switchport access vlan 21
 switchport mode access
!
interface FastEthernet0/7
 switchport access vlan 5
 switchport mode access
!
interface FastEthernet0/8
 switchport access vlan 6
 switchport mode access
!
interface FastEthernet0/9
 switchport access vlan 6
 switchport mode access
!
interface FastEthernet0/10
 switchport access vlan 6
 switchport mode access
!
interface FastEthernet0/11
 switchport access vlan 6
 switchport mode access
!
interface FastEthernet0/12
 switchport access vlan 6
 switchport mode access
!
interface FastEthernet0/13
 switchport access vlan 6
 switchport mode access
!
interface FastEthernet0/14
 switchport access vlan 6
 switchport mode access
!
interface FastEthernet0/15
 switchport access vlan 7
 switchport mode access
!
interface FastEthernet0/16
 switchport access vlan 7
 switchport mode access
!
interface FastEthernet0/17
 switchport access vlan 7
 switchport mode access
!
interface FastEthernet0/18
 switchport access vlan 7
 switchport mode access
!
interface FastEthernet0/19
 switchport access vlan 7
 switchport mode access
!
interface FastEthernet0/20
 switchport access vlan 7
 switchport mode access
!
interface FastEthernet0/21
 switchport access vlan 8
 switchport mode access
!
interface FastEthernet0/22
 switchport access vlan 8
 switchport mode access
!
interface FastEthernet0/23
 switchport access vlan 8
 switchport mode access
!
interface FastEthernet0/24
 switchport access vlan 8
 switchport mode access
!
interface GigabitEthernet0/1
 switchport mode trunk
!
interface GigabitEthernet0/2
!
interface Vlan1
 no ip address
 shutdown
!
interface Vlan9
 mac-address 0007.ec8c.3801
 ip address 192.168.9.2 255.255.255.0
!
ip default-gateway 192.168.9.1
!
!
!
!
line con 0
!
line vty 0 4
 login
line vty 5 15
 login
!
!
!
!
end

S2
!
version 12.2
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname S2
!
!
!
no ip domain-lookup
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
interface FastEthernet0/1
!
interface FastEthernet0/2
 switchport access vlan 5
 switchport mode access
!
interface FastEthernet0/3
 switchport access vlan 5
 switchport mode access
!
interface FastEthernet0/4
 switchport access vlan 5
 switchport mode access
!
interface FastEthernet0/5
 switchport access vlan 5
 switchport mode access
!
interface FastEthernet0/6
 switchport access vlan 5
 switchport mode access
!
interface FastEthernet0/7
 switchport access vlan 5
 switchport mode access
!
interface FastEthernet0/8
 switchport access vlan 6
 switchport mode access
!
interface FastEthernet0/9
 switchport access vlan 6
 switchport mode access
!
interface FastEthernet0/10
 switchport access vlan 6
 switchport mode access
!
interface FastEthernet0/11
 switchport access vlan 6
 switchport mode access
!
interface FastEthernet0/12
 switchport access vlan 6
 switchport mode access
!
interface FastEthernet0/13
 switchport access vlan 6
 switchport mode access
!
interface FastEthernet0/14
 switchport access vlan 6
 switchport mode access
!
interface FastEthernet0/15
 switchport access vlan 7
 switchport mode access
!
interface FastEthernet0/16
 switchport access vlan 7
 switchport mode access
!
interface FastEthernet0/17
 switchport access vlan 7
 switchport mode access
!
interface FastEthernet0/18
 switchport access vlan 23
 switchport mode access
!
interface FastEthernet0/19
 switchport access vlan 7
 switchport mode access
!
interface FastEthernet0/20
 switchport access vlan 7
 switchport mode access
!
interface FastEthernet0/21
 switchport access vlan 8
 switchport mode access
!
interface FastEthernet0/22
 switchport access vlan 8
 switchport mode access
!
interface FastEthernet0/23
 switchport access vlan 8
 switchport mode access
!
interface FastEthernet0/24
 switchport access vlan 8
 switchport mode access
!
interface GigabitEthernet0/1
!
interface GigabitEthernet0/2
!
interface Vlan1
 no ip address
 shutdown
!
interface Vlan9
 mac-address 0060.3e51.4d01
 ip address 192.168.9.3 255.255.255.0
!
ip default-gateway 192.168.9.1
!
!
!
!
line con 0
!
line vty 0 4
 login
line vty 5 15
 login
!
!
!
!
end
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