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2.2 Create all appropriate A records for all servers on Swansea and London Network
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          5.1 Join L-CD, ClientS1, ClientL1 to the yourname.acca domain
[image: ]


[bookmark: _Toc216783708]6 DHCP Server
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          6.3 All the Clients should receive IP Address automatically via DHCP Server 
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